docdata["FW-190A8"] =
{
           "Circuit Breakers": {
                                             "CBR_COVER1": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Circuit Breaker Cover 1",
                                                                        "identifier": "CBR_COVER1",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14374,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 1,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                             "CBR_COVER2": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Circuit Breaker Cover 2",
                                                                        "identifier": "CBR_COVER2",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14374,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 2,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                     "CB_ART_HORIZON_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Artificial Horizon Power Off",
                                                                        "identifier": "CB_ART_HORIZON_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 2,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_ART_HORIZON_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Artificial Horizon Power On",
                                                                        "identifier": "CB_ART_HORIZON_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 1,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                   "CB_AUX_TANK_PUMP_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Aux. Tank Fuel Pump Power Off",
                                                                        "identifier": "CB_AUX_TANK_PUMP_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 16,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 4,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                    "CB_AUX_TANK_PUMP_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Aux. Tank Fuel Pump Power On",
                                                                        "identifier": "CB_AUX_TANK_PUMP_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 8,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 3,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                     "CB_A_TANK_PUMP_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Aft Tank Fuel Pump Power Off",
                                                                        "identifier": "CB_A_TANK_PUMP_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_A_TANK_PUMP_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Aft Tank Fuel Pump Power On",
                                                                        "identifier": "CB_A_TANK_PUMP_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32768,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 15,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                            "CB_BATT_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Battery Power Off",
                                                                        "identifier": "CB_BATT_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1024,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 10,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                             "CB_BATT_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Battery Power On",
                                                                        "identifier": "CB_BATT_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 512,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 9,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                    "CB_CABIN_LIGHTS_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Cabin Illumination Power Off",
                                                                        "identifier": "CB_CABIN_LIGHTS_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 16384,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 14,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                     "CB_CABIN_LIGHTS_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Cabin Illumination Power On",
                                                                        "identifier": "CB_CABIN_LIGHTS_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 8192,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 13,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_CLOTH_HEAT_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Clothes Heating Power Off",
                                                                        "identifier": "CB_CLOTH_HEAT_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_CLOTH_HEAT_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Clothes Heating Power On",
                                                                        "identifier": "CB_CLOTH_HEAT_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32768,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 15,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                     "CB_D_TANK_PUMP_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Drop Tank Fuel Pump Power Off",
                                                                        "identifier": "CB_D_TANK_PUMP_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 2,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_D_TANK_PUMP_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Drop Tank Fuel Pump Power On",
                                                                        "identifier": "CB_D_TANK_PUMP_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 1,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                          "CB_EXT_PW_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Battery Power Off",
                                                                        "identifier": "CB_EXT_PW_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4096,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 12,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                           "CB_EXT_PW_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Battery Power On",
                                                                        "identifier": "CB_EXT_PW_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2048,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 11,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                           "CB_FLAPS_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Landing Flaps Power Off",
                                                                        "identifier": "CB_FLAPS_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1024,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 10,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                            "CB_FLAPS_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Landing Flaps Power On",
                                                                        "identifier": "CB_FLAPS_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 512,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 9,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                     "CB_F_TANK_PUMP_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Fore Tank Fuel Pump Power Off",
                                                                        "identifier": "CB_F_TANK_PUMP_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 16384,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 14,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_F_TANK_PUMP_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Fore Tank Fuel Pump Power On",
                                                                        "identifier": "CB_F_TANK_PUMP_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 8192,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 13,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_GEAR_CONT_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Undercarriage Controls Power Off",
                                                                        "identifier": "CB_GEAR_CONT_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 256,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 8,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                        "CB_GEAR_CONT_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Undercarriage Controls Power On",
                                                                        "identifier": "CB_GEAR_CONT_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 128,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 7,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                            "CB_GEAR_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Undercarriage Drives Power Off",
                                                                        "identifier": "CB_GEAR_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 256,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 8,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                             "CB_GEAR_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Undercarriage Drives Power On",
                                                                        "identifier": "CB_GEAR_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 128,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 7,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                             "CB_GEN_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Generator Power Off",
                                                                        "identifier": "CB_GEN_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 256,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 8,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                              "CB_GEN_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Generator Power On",
                                                                        "identifier": "CB_GEN_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 128,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 7,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_GUNS_COWL_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Cowling Guns Power Off",
                                                                        "identifier": "CB_GUNS_COWL_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14374,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                        "CB_GUNS_COWL_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Cowling Guns Power On",
                                                                        "identifier": "CB_GUNS_COWL_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32768,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 15,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                         "CB_GUNS_IN_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Inner Wing Guns Power Off",
                                                                        "identifier": "CB_GUNS_IN_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 16384,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 14,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                          "CB_GUNS_IN_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Inner Wing Guns Power On",
                                                                        "identifier": "CB_GUNS_IN_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 8192,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 13,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                        "CB_GUNS_OUT_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Outer Wing Guns Power Off",
                                                                        "identifier": "CB_GUNS_OUT_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4096,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 12,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                         "CB_GUNS_OUT_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Outer Wing Guns Power On",
                                                                        "identifier": "CB_GUNS_OUT_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2048,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 11,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                         "CB_GUN_CAM_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Gun Sight and Gun Camera Power Off",
                                                                        "identifier": "CB_GUN_CAM_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 256,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 8,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                          "CB_GUN_CAM_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Gun Sight and Gun Camera Power On",
                                                                        "identifier": "CB_GUN_CAM_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 128,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 7,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                        "CB_IFF_DEST_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "FuG 25a IFF Self-Destruct Power Off",
                                                                        "identifier": "CB_IFF_DEST_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1024,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 10,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                         "CB_IFF_DEST_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "FuG 25a IFF Self-Destruct Power On",
                                                                        "identifier": "CB_IFF_DEST_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 512,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 9,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                             "CB_IFF_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "FuG 25a IFF Power Off",
                                                                        "identifier": "CB_IFF_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 64,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 6,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                              "CB_IFF_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "FuG 25a IFF Power On",
                                                                        "identifier": "CB_IFF_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 5,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                        "CB_IGNITION_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Ignition Power Off",
                                                                        "identifier": "CB_IGNITION_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 16,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 4,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                         "CB_IGNITION_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Ignition Power On",
                                                                        "identifier": "CB_IGNITION_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 8,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 3,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                     "CB_INSTRUMENTS_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Instruments Power Off",
                                                                        "identifier": "CB_INSTRUMENTS_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1024,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 10,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_INSTRUMENTS_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Instruments Power On",
                                                                        "identifier": "CB_INSTRUMENTS_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 512,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 9,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                         "CB_MOT_GEN_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Motor-Generator Power Off",
                                                                        "identifier": "CB_MOT_GEN_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 16,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 4,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                          "CB_MOT_GEN_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Motor-Generator Power On",
                                                                        "identifier": "CB_MOT_GEN_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 8,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 3,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_NAV_LIGHTS_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Navigation Lights Power Off",
                                                                        "identifier": "CB_NAV_LIGHTS_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4096,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 12,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_NAV_LIGHTS_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Navigation Lights Power On",
                                                                        "identifier": "CB_NAV_LIGHTS_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2048,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 11,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                             "CB_ORD_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Drop Ordnance & Optional Armament Power Off",
                                                                        "identifier": "CB_ORD_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 64,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 6,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                              "CB_ORD_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Drop Ordnance & Optional Armament Power On",
                                                                        "identifier": "CB_ORD_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14364,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 5,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_PITOT_HEAT_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Pitot Heating Power Off",
                                                                        "identifier": "CB_PITOT_HEAT_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 2,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_PITOT_HEAT_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Pitot Heating Power On",
                                                                        "identifier": "CB_PITOT_HEAT_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14368,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 1,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_PROP_CONTR_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Prop. Pitch Controls Power Off",
                                                                        "identifier": "CB_PROP_CONTR_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 16384,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 14,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_PROP_CONTR_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Prop. Pitch Controls Power On",
                                                                        "identifier": "CB_PROP_CONTR_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 8192,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 13,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                      "CB_PROP_DRIVE_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Prop. Pitch Drive Power Off",
                                                                        "identifier": "CB_PROP_DRIVE_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 4096,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 12,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_PROP_DRIVE_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Prop. Pitch Drive Power On",
                                                                        "identifier": "CB_PROP_DRIVE_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 2048,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 11,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                           "CB_RADIO_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "FuG 16 ZY Radio Power Off",
                                                                        "identifier": "CB_RADIO_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 64,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 6,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                            "CB_RADIO_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "FuG 16 ZY Radio Power On",
                                                                        "identifier": "CB_RADIO_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 5,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                        "CB_REP_COMP_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Repeater Compass Power Off",
                                                                        "identifier": "CB_REP_COMP_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 64,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 6,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                         "CB_REP_COMP_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Repeater Compass Power On",
                                                                        "identifier": "CB_REP_COMP_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 5,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                       "CB_STAB_TRIM_OFF": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Stabilizer Trim Power Off",
                                                                        "identifier": "CB_STAB_TRIM_OFF",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14372,
                                                                                          "description": "selector position",
                                                                                                 "mask": 1,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           },
                                        "CB_STAB_TRIM_ON": {
                                                                          "category": "Circuit Breakers",
                                                                      "control_type": "selector",
                                                                       "description": "Stabilizer Trim Power On",
                                                                        "identifier": "CB_STAB_TRIM_ON",
                                                                            "inputs": [ {
                                                                                          "description": "switch to previous or next state",
                                                                                            "interface": "fixed_step"
                                                                                      }, {
                                                                                          "description": "set position",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 1
                                                                                      }, {
                                                                                             "argument": "TOGGLE",
                                                                                          "description": "Toggle switch state",
                                                                                            "interface": "action"
                                                                                      } ],
                                                               "momentary_positions": "none",
                                                                           "outputs": [ {
                                                                                              "address": 14370,
                                                                                          "description": "selector position",
                                                                                                 "mask": 32768,
                                                                                            "max_value": 1,
                                                                                             "shift_by": 15,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ],
                                                                  "physical_variant": "limited_rotary"
                                                           }
                               },
                      "Clock": {
                                      "CLOCK_ON_OFF": {
                                                                     "category": "Clock",
                                                                 "control_type": "selector",
                                                                  "description": "Clock Start / Stop",
                                                                   "identifier": "CLOCK_ON_OFF",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14374,
                                                                                     "description": "selector position",
                                                                                            "mask": 2048,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 11,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                      "CLOCK_PINION": {
                                                           "api_variant": "multiturn",
                                                              "category": "Clock",
                                                          "control_type": "analog_dial",
                                                           "description": "Clock Pinion",
                                                            "identifier": "CLOCK_PINION",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14384,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                       "CLOCK_SCALE": {
                                                           "api_variant": "multiturn",
                                                              "category": "Clock",
                                                          "control_type": "analog_dial",
                                                           "description": "Clock Scale",
                                                            "identifier": "CLOCK_SCALE",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14382,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                   "CLOCK_STOPWATCH": {
                                                                  "api_variant": "momentary_last_position",
                                                                     "category": "Clock",
                                                                 "control_type": "selector",
                                                                  "description": "Clock Stopwatch",
                                                                   "identifier": "CLOCK_STOPWATCH",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14374,
                                                                                     "description": "selector position",
                                                                                            "mask": 4096,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 12,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "push_button"
                                                      }
                               },
                    "Cockpit": {
                                     "ALT_PRESS_SET": {
                                                           "api_variant": "multiturn",
                                                              "category": "Cockpit",
                                                          "control_type": "analog_dial",
                                                           "description": "Altimeter Pressure Set",
                                                            "identifier": "ALT_PRESS_SET",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14344,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                    "CANOPY_EMG_REL": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Canopy Emergency Release Handle",
                                                                   "identifier": "CANOPY_EMG_REL",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 32768,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 15,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                   "CANOPY_HAND_CRK": {
                                                           "api_variant": "multiturn",
                                                              "category": "Cockpit",
                                                          "control_type": "analog_dial",
                                                           "description": "Canopy Hand Crank",
                                                            "identifier": "CANOPY_HAND_CRK",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14340,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                           "EL_KILL": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Electric Kill-switch",
                                                                   "identifier": "EL_KILL",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 16384,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 14,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                      "FUEL_CUTTOFF": {
                                                                  "api_variant": "momentary_last_position",
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Fuel Cutoff Handle",
                                                                   "identifier": "FUEL_CUTTOFF",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 2048,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 11,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "push_button"
                                                      },
                                    "FUEL_GAUGE_SEL": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Fuel Gauge Selector (FORWARD/NONE/AFT)",
                                                                   "identifier": "FUEL_GAUGE_SEL",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 3
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 768,
                                                                                       "max_value": 3,
                                                                                        "shift_by": 8,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                    "FUEL_PRIM_PMPL": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Primer Pump",
                                                                   "identifier": "FUEL_PRIM_PMPL",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 1024,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 10,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                      "FUEL_TNK_SEL": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Fuel Tank Selector Valve (CLOSE/FORWARD/BOTH/AFT)",
                                                                   "identifier": "FUEL_TNK_SEL",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 3
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 192,
                                                                                       "max_value": 3,
                                                                                        "shift_by": 6,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                          "HOR_CAGE": {
                                                              "category": "Cockpit",
                                                          "control_type": "limited_dial",
                                                           "description": "Horizon Cage",
                                                            "identifier": "HOR_CAGE",
                                                                "inputs": [ {
                                                                              "description": "set the position of the dial",
                                                                                "interface": "set_state",
                                                                                "max_value": 65535
                                                                          }, {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14346,
                                                                              "description": "position of the potentiometer",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                     "HOR_STAB_TRIM": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Stabilizer Trimmer Up/Down",
                                                                   "identifier": "HOR_STAB_TRIM",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 2
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14342,
                                                                                     "description": "selector position",
                                                                                            "mask": 24,
                                                                                       "max_value": 2,
                                                                                        "shift_by": 3,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                          "ING_MODE": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Ingnition Mode Manual/Auto)",
                                                                   "identifier": "ING_MODE",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 32,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 5,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                   "INSTR_LGHT_CTRL": {
                                                           "api_variant": "multiturn",
                                                              "category": "Cockpit",
                                                          "control_type": "analog_dial",
                                                           "description": "Instrument Lights Brightness",
                                                            "identifier": "INSTR_LGHT_CTRL",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14352,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                           "MAGNETO": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Magneto Switch",
                                                                   "identifier": "MAGNETO",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 3
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 3,
                                                                                       "max_value": 3,
                                                                                        "shift_by": 0,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                      "OXY_EMG_KNOB": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Oxygen Emergency Knob",
                                                                   "identifier": "OXY_EMG_KNOB",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 8192,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 13,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                    "OXY_FLOW_VALVE": {
                                                              "category": "Cockpit",
                                                          "control_type": "limited_dial",
                                                           "description": "Oxygen Flow Valve",
                                                            "identifier": "OXY_FLOW_VALVE",
                                                                "inputs": [ {
                                                                              "description": "set the position of the dial",
                                                                                "interface": "set_state",
                                                                                "max_value": 65535
                                                                          }, {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14338,
                                                                              "description": "position of the potentiometer",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                     "STARTER_BRUSH": {
                                                                  "api_variant": "momentary_last_position",
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Retract starter brushes",
                                                                   "identifier": "STARTER_BRUSH",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 4096,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 12,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "push_button"
                                                      },
                                       "STARTER_CVR": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Starter Switch Cover",
                                                                   "identifier": "STARTER_CVR",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 4,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 2,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                    "STARTER_SWITCH": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Starter Switch. Starter Power",
                                                                   "identifier": "STARTER_SWITCH",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 2
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14336,
                                                                                     "description": "selector position",
                                                                                            "mask": 24,
                                                                                       "max_value": 2,
                                                                                        "shift_by": 3,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                   "STARTER_SWITCH2": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Starter Switch. Magnetic Clutch",
                                                                   "identifier": "STARTER_SWITCH2",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 2
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14386,
                                                                                     "description": "selector position",
                                                                                            "mask": 384,
                                                                                       "max_value": 2,
                                                                                        "shift_by": 7,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                        "START_STOP": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Start - Stop Button",
                                                                   "identifier": "START_STOP",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14342,
                                                                                     "description": "selector position",
                                                                                            "mask": 2,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 1,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                         "STOPWATCH": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Stopwatch Button",
                                                                   "identifier": "STOPWATCH",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14342,
                                                                                     "description": "selector position",
                                                                                            "mask": 4,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 2,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                          "THR_LOCK": {
                                                                     "category": "Cockpit",
                                                                 "control_type": "selector",
                                                                  "description": "Throttle Lock",
                                                                   "identifier": "THR_LOCK",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14342,
                                                                                     "description": "selector position",
                                                                                            "mask": 1,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 0,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                          "TURN_BEZ": {
                                                           "api_variant": "multiturn",
                                                              "category": "Cockpit",
                                                          "control_type": "analog_dial",
                                                           "description": "Turnable Bezel",
                                                            "identifier": "TURN_BEZ",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14348,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                           "WND_SET": {
                                                           "api_variant": "multiturn",
                                                              "category": "Cockpit",
                                                          "control_type": "analog_dial",
                                                           "description": "Wind/Set Knob",
                                                            "identifier": "WND_SET",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14350,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      }
                               },
                    "Compass": {
                                   "CRS_SET": {
                                                   "api_variant": "multiturn",
                                                      "category": "Compass",
                                                  "control_type": "analog_dial",
                                                   "description": "Course Set",
                                                    "identifier": "CRS_SET",
                                                        "inputs": [ {
                                                                         "description": "turn the dial left or right",
                                                                           "interface": "variable_step",
                                                                           "max_value": 65535,
                                                                      "suggested_step": 3200
                                                                  } ],
                                                       "outputs": [ {
                                                                          "address": 14380,
                                                                      "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                             "mask": 65535,
                                                                        "max_value": 65535,
                                                                         "shift_by": 0,
                                                                           "suffix": "_KNOB_POS",
                                                                             "type": "integer"
                                                                  } ]
                                              }
                               },
                     "Engine": {
                                   "PROP_PITCH": {
                                                                "category": "Engine",
                                                            "control_type": "selector",
                                                             "description": "Propellor Pitch De/Increase",
                                                              "identifier": "PROP_PITCH",
                                                                  "inputs": [ {
                                                                                "description": "set the switch position -- 0 = held left/down, 1 = centered, 2 = held right/up",
                                                                                  "interface": "set_state",
                                                                                  "max_value": 2
                                                                            } ],
                                                     "momentary_positions": "first_and_last",
                                                                 "outputs": [ {
                                                                                    "address": 14342,
                                                                                "description": "selector position",
                                                                                       "mask": 12288,
                                                                                  "max_value": 2,
                                                                                   "shift_by": 12,
                                                                                     "suffix": "",
                                                                                       "type": "integer"
                                                                            } ],
                                                        "physical_variant": "rocker_switch"
                                                 }
                               },
    "External Aircraft Model": {
                                    "EXT_POSITION_LIGHT_LEFT": {
                                                                       "category": "External Aircraft Model",
                                                                   "control_type": "metadata",
                                                                    "description": "Left Position Light (red)",
                                                                     "identifier": "EXT_POSITION_LIGHT_LEFT",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 14386,
                                                                                       "description": "Left Position Light (red)",
                                                                                              "mask": 2048,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 11,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                   "EXT_POSITION_LIGHT_RIGHT": {
                                                                       "category": "External Aircraft Model",
                                                                   "control_type": "metadata",
                                                                    "description": "Right Position Light (green)",
                                                                     "identifier": "EXT_POSITION_LIGHT_RIGHT",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 14386,
                                                                                       "description": "Right Position Light (green)",
                                                                                              "mask": 4096,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 12,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                    "EXT_POSITION_LIGHT_TAIL": {
                                                                       "category": "External Aircraft Model",
                                                                   "control_type": "metadata",
                                                                    "description": "Tail Position Light (White)",
                                                                     "identifier": "EXT_POSITION_LIGHT_TAIL",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 14386,
                                                                                       "description": "Tail Position Light (White)",
                                                                                              "mask": 8192,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 13,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                               "EXT_WOW_LEFT": {
                                                                       "category": "External Aircraft Model",
                                                                   "control_type": "metadata",
                                                                    "description": "Weight ON Wheels Left Gear",
                                                                     "identifier": "EXT_WOW_LEFT",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 14500,
                                                                                       "description": "Weight ON Wheels Left Gear",
                                                                                              "mask": 1,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 0,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                              "EXT_WOW_RIGHT": {
                                                                       "category": "External Aircraft Model",
                                                                   "control_type": "metadata",
                                                                    "description": "Weight ON Wheels Right Gear",
                                                                     "identifier": "EXT_WOW_RIGHT",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 14386,
                                                                                       "description": "Weight ON Wheels Right Gear",
                                                                                              "mask": 32768,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 15,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                               "EXT_WOW_TAIL": {
                                                                       "category": "External Aircraft Model",
                                                                   "control_type": "metadata",
                                                                    "description": "Weight ON Wheels Tail Gear",
                                                                     "identifier": "EXT_WOW_TAIL",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 14386,
                                                                                       "description": "Weight ON Wheels Tail Gear",
                                                                                              "mask": 16384,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 14,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               }
                               },
                      "Flaps": {
                                    "COOL_FLAP_CTRL": {
                                                           "api_variant": "multiturn",
                                                              "category": "Flaps",
                                                          "control_type": "analog_dial",
                                                           "description": "Cooling Flaps Control",
                                                            "identifier": "COOL_FLAP_CTRL",
                                                                "inputs": [ {
                                                                                 "description": "turn the dial left or right",
                                                                                   "interface": "variable_step",
                                                                                   "max_value": 65535,
                                                                              "suggested_step": 3200
                                                                          } ],
                                                               "outputs": [ {
                                                                                  "address": 14354,
                                                                              "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                     "mask": 65535,
                                                                                "max_value": 65535,
                                                                                 "shift_by": 0,
                                                                                   "suffix": "_KNOB_POS",
                                                                                     "type": "integer"
                                                                          } ]
                                                      },
                                        "FLAPS_LAND": {
                                                                     "category": "Flaps",
                                                                 "control_type": "selector",
                                                                  "description": "Flaps Landing",
                                                                   "identifier": "FLAPS_LAND",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14342,
                                                                                     "description": "selector position",
                                                                                            "mask": 128,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 7,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                          "FLAPS_TO": {
                                                                     "category": "Flaps",
                                                                 "control_type": "selector",
                                                                  "description": "Flaps Take Off",
                                                                   "identifier": "FLAPS_TO",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14342,
                                                                                     "description": "selector position",
                                                                                            "mask": 64,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 6,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      },
                                   "FLAPS_UP_TOGGLE": {
                                                                     "category": "Flaps",
                                                                 "control_type": "selector",
                                                                  "description": "Flaps Up",
                                                                   "identifier": "FLAPS_UP_TOGGLE",
                                                                       "inputs": [ {
                                                                                     "description": "switch to previous or next state",
                                                                                       "interface": "fixed_step"
                                                                                 }, {
                                                                                     "description": "set position",
                                                                                       "interface": "set_state",
                                                                                       "max_value": 1
                                                                                 }, {
                                                                                        "argument": "TOGGLE",
                                                                                     "description": "Toggle switch state",
                                                                                       "interface": "action"
                                                                                 } ],
                                                          "momentary_positions": "none",
                                                                      "outputs": [ {
                                                                                         "address": 14342,
                                                                                     "description": "selector position",
                                                                                            "mask": 32,
                                                                                       "max_value": 1,
                                                                                        "shift_by": 5,
                                                                                          "suffix": "",
                                                                                            "type": "integer"
                                                                                 } ],
                                                             "physical_variant": "limited_rotary"
                                                      }
                               },
                       "Gear": {
                                   "EMG_LG_REL": {
                                                                "category": "Gear",
                                                            "control_type": "selector",
                                                             "description": "Landing Gear Emergency Release Handle",
                                                              "identifier": "EMG_LG_REL",
                                                                  "inputs": [ {
                                                                                "description": "switch to previous or next state",
                                                                                  "interface": "fixed_step"
                                                                            }, {
                                                                                "description": "set position",
                                                                                  "interface": "set_state",
                                                                                  "max_value": 1
                                                                            }, {
                                                                                   "argument": "TOGGLE",
                                                                                "description": "Toggle switch state",
                                                                                  "interface": "action"
                                                                            } ],
                                                     "momentary_positions": "none",
                                                                 "outputs": [ {
                                                                                    "address": 14342,
                                                                                "description": "selector position",
                                                                                       "mask": 2048,
                                                                                  "max_value": 1,
                                                                                   "shift_by": 11,
                                                                                     "suffix": "",
                                                                                       "type": "integer"
                                                                            } ],
                                                        "physical_variant": "limited_rotary"
                                                 },
                                       "LG_EXT": {
                                                                "category": "Gear",
                                                            "control_type": "selector",
                                                             "description": "Landing Gears Extending",
                                                              "identifier": "LG_EXT",
                                                                  "inputs": [ {
                                                                                "description": "switch to previous or next state",
                                                                                  "interface": "fixed_step"
                                                                            }, {
                                                                                "description": "set position",
                                                                                  "interface": "set_state",
                                                                                  "max_value": 1
                                                                            }, {
                                                                                   "argument": "TOGGLE",
                                                                                "description": "Toggle switch state",
                                                                                  "interface": "action"
                                                                            } ],
                                                     "momentary_positions": "none",
                                                                 "outputs": [ {
                                                                                    "address": 14342,
                                                                                "description": "selector position",
                                                                                       "mask": 1024,
                                                                                  "max_value": 1,
                                                                                   "shift_by": 10,
                                                                                     "suffix": "",
                                                                                       "type": "integer"
                                                                            } ],
                                                        "physical_variant": "limited_rotary"
                                                 },
                                       "LG_RET": {
                                                                "category": "Gear",
                                                            "control_type": "selector",
                                                             "description": "Landing Gears Retraction",
                                                              "identifier": "LG_RET",
                                                                  "inputs": [ {
                                                                                "description": "switch to previous or next state",
                                                                                  "interface": "fixed_step"
                                                                            }, {
                                                                                "description": "set position",
                                                                                  "interface": "set_state",
                                                                                  "max_value": 1
                                                                            }, {
                                                                                   "argument": "TOGGLE",
                                                                                "description": "Toggle switch state",
                                                                                  "interface": "action"
                                                                            } ],
                                                     "momentary_positions": "none",
                                                                 "outputs": [ {
                                                                                    "address": 14342,
                                                                                "description": "selector position",
                                                                                       "mask": 256,
                                                                                  "max_value": 1,
                                                                                   "shift_by": 8,
                                                                                     "suffix": "",
                                                                                       "type": "integer"
                                                                            } ],
                                                        "physical_variant": "limited_rotary"
                                                 },
                                   "LG_RET_CVR": {
                                                                "category": "Gear",
                                                            "control_type": "selector",
                                                             "description": "Landing Gears Retraction Cover",
                                                              "identifier": "LG_RET_CVR",
                                                                  "inputs": [ {
                                                                                "description": "switch to previous or next state",
                                                                                  "interface": "fixed_step"
                                                                            }, {
                                                                                "description": "set position",
                                                                                  "interface": "set_state",
                                                                                  "max_value": 1
                                                                            }, {
                                                                                   "argument": "TOGGLE",
                                                                                "description": "Toggle switch state",
                                                                                  "interface": "action"
                                                                            } ],
                                                     "momentary_positions": "none",
                                                                 "outputs": [ {
                                                                                    "address": 14342,
                                                                                "description": "selector position",
                                                                                       "mask": 512,
                                                                                  "max_value": 1,
                                                                                   "shift_by": 9,
                                                                                     "suffix": "",
                                                                                       "type": "integer"
                                                                            } ],
                                                        "physical_variant": "limited_rotary"
                                                 }
                               },
                  "Gun Sight": {
                                   "SIGHT_BRIGHT": {
                                                        "api_variant": "multiturn",
                                                           "category": "Gun Sight",
                                                       "control_type": "analog_dial",
                                                        "description": "Gunsight Brightness Rheostat",
                                                         "identifier": "SIGHT_BRIGHT",
                                                             "inputs": [ {
                                                                              "description": "turn the dial left or right",
                                                                                "interface": "variable_step",
                                                                                "max_value": 65535,
                                                                           "suggested_step": 3200
                                                                       } ],
                                                            "outputs": [ {
                                                                               "address": 14366,
                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                  "mask": 65535,
                                                                             "max_value": 65535,
                                                                              "shift_by": 0,
                                                                                "suffix": "_KNOB_POS",
                                                                                  "type": "integer"
                                                                       } ]
                                                   },
                                    "SIGHT_SMOKE": {
                                                                  "category": "Gun Sight",
                                                              "control_type": "selector",
                                                               "description": "Gun Sight Smoked Screen Controls",
                                                                "identifier": "SIGHT_SMOKE",
                                                                    "inputs": [ {
                                                                                  "description": "switch to previous or next state",
                                                                                    "interface": "fixed_step"
                                                                              }, {
                                                                                  "description": "set position",
                                                                                    "interface": "set_state",
                                                                                    "max_value": 1
                                                                              }, {
                                                                                     "argument": "TOGGLE",
                                                                                  "description": "Toggle switch state",
                                                                                    "interface": "action"
                                                                              } ],
                                                       "momentary_positions": "none",
                                                                   "outputs": [ {
                                                                                      "address": 14364,
                                                                                  "description": "selector position",
                                                                                         "mask": 16,
                                                                                    "max_value": 1,
                                                                                     "shift_by": 4,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ],
                                                          "physical_variant": "limited_rotary"
                                                   }
                               },
                        "IFF": {
                                   "IFF_CHAN_SEL": {
                                                                  "category": "IFF",
                                                              "control_type": "selector",
                                                               "description": "IFF Channel Selector",
                                                                "identifier": "IFF_CHAN_SEL",
                                                                    "inputs": [ {
                                                                                  "description": "switch to previous or next state",
                                                                                    "interface": "fixed_step"
                                                                              }, {
                                                                                  "description": "set position",
                                                                                    "interface": "set_state",
                                                                                    "max_value": 2
                                                                              } ],
                                                       "momentary_positions": "none",
                                                                   "outputs": [ {
                                                                                      "address": 14374,
                                                                                  "description": "selector position",
                                                                                         "mask": 24,
                                                                                    "max_value": 2,
                                                                                     "shift_by": 3,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ],
                                                          "physical_variant": "limited_rotary"
                                                   },
                                      "IFF_CHECK": {
                                                                  "category": "IFF",
                                                              "control_type": "selector",
                                                               "description": "IFF Check",
                                                                "identifier": "IFF_CHECK",
                                                                    "inputs": [ {
                                                                                  "description": "switch to previous or next state",
                                                                                    "interface": "fixed_step"
                                                                              }, {
                                                                                  "description": "set position",
                                                                                    "interface": "set_state",
                                                                                    "max_value": 1
                                                                              }, {
                                                                                     "argument": "TOGGLE",
                                                                                  "description": "Toggle switch state",
                                                                                    "interface": "action"
                                                                              } ],
                                                       "momentary_positions": "none",
                                                                   "outputs": [ {
                                                                                      "address": 14374,
                                                                                  "description": "selector position",
                                                                                         "mask": 32,
                                                                                    "max_value": 1,
                                                                                     "shift_by": 5,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ],
                                                          "physical_variant": "limited_rotary"
                                                   }
                               },
                  "Indicator": {
                                          "ADF_HORIZONT": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "ADF_Horizont",
                                                                "identifier": "ADF_HORIZONT",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14494,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "ADF_VERTICAL": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "ADF_Vertical",
                                                                "identifier": "ADF_VERTICAL",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14492,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "ALTIMETER_KM": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Altimeter_km",
                                                                "identifier": "ALTIMETER_KM",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14420,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                           "ALTIMETER_M": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Altimeter_m",
                                                                "identifier": "ALTIMETER_M",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14422,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                    "ALTIMETER_PRESSURE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Altimeter_Pressure",
                                                                "identifier": "ALTIMETER_PRESSURE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14424,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "AMMO_COUNTER_1": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Ammo_Counter_1",
                                                                "identifier": "AMMO_COUNTER_1",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14472,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "AMMO_COUNTER_2": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Ammo_Counter_2",
                                                                "identifier": "AMMO_COUNTER_2",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14474,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "AMMO_COUNTER_3": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Ammo_Counter_3",
                                                                "identifier": "AMMO_COUNTER_3",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14476,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "AMMO_COUNTER_4": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Ammo_Counter_4",
                                                                "identifier": "AMMO_COUNTER_4",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14478,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                                "CANOPY": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Canopy",
                                                                "identifier": "CANOPY",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14400,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "CANOPYDAMAGE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "CanopyDamage",
                                                                "identifier": "CANOPYDAMAGE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14498,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "CANOPY_CRANK": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Canopy Crank",
                                                                "identifier": "CANOPY_CRANK",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14402,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "CHRONO_MINUTES": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Chrono_Minutes",
                                                                "identifier": "CHRONO_MINUTES",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14470,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                       "COMMANDEDCOURSE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "CommandedCourse",
                                                                "identifier": "COMMANDEDCOURSE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14440,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "COMPASSHEADING": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "CompassHeading",
                                                                "identifier": "COMPASSHEADING",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14438,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                   "COOLANT_TEMPERATURE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Coolant_Temperature",
                                                                "identifier": "COOLANT_TEMPERATURE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14450,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "CURRTIME_HOURS": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "CurrTime_Hours",
                                                                "identifier": "CURRTIME_HOURS",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14464,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                      "CURRTIME_MINUTES": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "CurrTime_Minutes",
                                                                "identifier": "CURRTIME_MINUTES",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14466,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                      "CURRTIME_SECONDS": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "CurrTime_Seconds",
                                                                "identifier": "CURRTIME_SECONDS",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14468,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "ENGINETHROTTLE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Engine Throttle",
                                                                "identifier": "ENGINETHROTTLE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14404,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "ENGINE_RPM": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Engine_RPM",
                                                                "identifier": "ENGINE_RPM",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14444,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                           "FLUOR_LIGHT": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Fluor_Light",
                                                                "identifier": "FLUOR_LIGHT",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14460,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                             "FUELMETER": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "FuelMeter",
                                                                "identifier": "FUELMETER",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14458,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                         "FUEL_PRESSURE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Fuel_Pressure",
                                                                "identifier": "FUEL_PRESSURE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14456,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "GUN_FIRE_1": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Gun_Fire_1",
                                                                "identifier": "GUN_FIRE_1",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14480,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "GUN_FIRE_2": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Gun_Fire_2",
                                                                "identifier": "GUN_FIRE_2",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14482,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "GUN_FIRE_3": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Gun_Fire_3",
                                                                "identifier": "GUN_FIRE_3",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14484,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "GUN_FIRE_4": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Gun_Fire_4",
                                                                "identifier": "GUN_FIRE_4",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14486,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "HORIZON_BANK": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Horizon_Bank",
                                                                "identifier": "HORIZON_BANK",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14428,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                         "HORIZON_PITCH": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Horizon_Pitch",
                                                                "identifier": "HORIZON_PITCH",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14426,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                                   "IAS": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "IAS",
                                                                "identifier": "IAS",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14416,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                       "LAMPS_INTENSITY": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Lamps Intensity",
                                                                "identifier": "LAMPS_INTENSITY",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14398,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                     "MANIFOLD_PRESSURE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Manifold_Pressure",
                                                                "identifier": "MANIFOLD_PRESSURE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14442,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "OIL_PRESSURE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Oil_Pressure",
                                                                "identifier": "OIL_PRESSURE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14454,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                       "OIL_TEMPERATURE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Oil_Temperature",
                                                                "identifier": "OIL_TEMPERATURE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14452,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                   "OXYGEN_FLOW_BLINKER": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Oxygen_Flow_Blinker",
                                                                "identifier": "OXYGEN_FLOW_BLINKER",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14436,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                       "OXYGEN_PRESSURE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Oxygen_Pressure",
                                                                "identifier": "OXYGEN_PRESSURE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14434,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                           "PANEL_ROT_X": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Panel_Rot_X",
                                                                "identifier": "PANEL_ROT_X",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14392,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                         "PANEL_SHAKE_Y": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Panel_Shake_Y",
                                                                "identifier": "PANEL_SHAKE_Y",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14390,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                         "PANEL_SHAKE_Z": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Panel_Shake_Z",
                                                                "identifier": "PANEL_SHAKE_Z",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14388,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "PILOT_DRAW": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "pilot_draw",
                                                                "identifier": "PILOT_DRAW",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14462,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "PROP_PITCH_H": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Propeller Pitch Hour",
                                                                "identifier": "PROP_PITCH_H",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14448,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                          "PROP_PITCH_M": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Propeller Pitch Minute",
                                                                "identifier": "PROP_PITCH_M",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14446,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                        "RUDDERPOSITION": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "RudderPosition",
                                                                "identifier": "RUDDERPOSITION",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14410,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                           "SIGHTSHAKEY": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "SightShakeY",
                                                                "identifier": "SIGHTSHAKEY",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14396,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                           "SIGHTSHAKEZ": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "SightShakeZ",
                                                                "identifier": "SIGHTSHAKEZ",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14394,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                              "SLIPBALL": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Slipball",
                                                                "identifier": "SLIPBALL",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14432,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                             "STICKBANK": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Stick Bank",
                                                                "identifier": "STICKBANK",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14408,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "STICKPITCH": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Stick Pitch",
                                                                "identifier": "STICKPITCH",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14406,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "TARGETDIST": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "TargetDist",
                                                                "identifier": "TARGETDIST",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14488,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                           "TRIMMNEEDLE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "TrimmNeedle",
                                                                "identifier": "TRIMMNEEDLE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14490,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                            "TURNNEEDLE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "TurnNeedle",
                                                                "identifier": "TURNNEEDLE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14430,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                         "VERTICALSPEED": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "VerticalSpeed",
                                                                "identifier": "VERTICALSPEED",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14418,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                         "WHEEL_BRAKE_L": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Left Wheel Brake",
                                                                "identifier": "WHEEL_BRAKE_L",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14412,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                         "WHEEL_BRAKE_R": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "Right Wheel Brake",
                                                                "identifier": "WHEEL_BRAKE_R",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14414,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          },
                                      "WINDSHIELDDAMAGE": {
                                                                  "category": "Indicator",
                                                              "control_type": "analog_gauge",
                                                               "description": "WindshieldDamage",
                                                                "identifier": "WINDSHIELDDAMAGE",
                                                                    "inputs": [  ],
                                                                   "outputs": [ {
                                                                                      "address": 14496,
                                                                                  "description": "gauge position",
                                                                                         "mask": 65535,
                                                                                    "max_value": 65535,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ]
                                                          }
                               },
                      "Lamps": {
                                        "AFN2_LAMP": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "AFN 2 Light",
                                                           "identifier": "AFN2_LAMP",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14386,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 16,
                                                                               "max_value": 1,
                                                                                "shift_by": 4,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                       "FLAPS_DOWN": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Flaps Down",
                                                           "identifier": "FLAPS_DOWN",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14386,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 8,
                                                                               "max_value": 1,
                                                                                "shift_by": 3,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                      "FLAPS_START": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Flaps Start",
                                                           "identifier": "FLAPS_START",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14386,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 4,
                                                                               "max_value": 1,
                                                                                "shift_by": 2,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                         "FLAPS_UP": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Flaps Up",
                                                           "identifier": "FLAPS_UP",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14386,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 2,
                                                                               "max_value": 1,
                                                                                "shift_by": 1,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                     "FUEL_LOW_FWD": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Fuel_Low_Fwd",
                                                           "identifier": "FUEL_LOW_FWD",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14386,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 32,
                                                                               "max_value": 1,
                                                                                "shift_by": 5,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                    "FUEL_LOW_REAR": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Fuel_Low_Rear",
                                                           "identifier": "FUEL_LOW_REAR",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14386,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 64,
                                                                               "max_value": 1,
                                                                                "shift_by": 6,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                      "GUN_131_L_1": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Gun 131 Lamp  1",
                                                           "identifier": "GUN_131_L_1",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14374,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 8192,
                                                                               "max_value": 1,
                                                                                "shift_by": 13,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                      "GUN_131_L_2": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Gun 131 Lamp  2",
                                                           "identifier": "GUN_131_L_2",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14374,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 16384,
                                                                               "max_value": 1,
                                                                                "shift_by": 14,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                     "GUN_SZKK_L_1": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Gun SZKK Lamp  1",
                                                           "identifier": "GUN_SZKK_L_1",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14374,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 32768,
                                                                               "max_value": 1,
                                                                                "shift_by": 15,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                     "GUN_SZKK_L_2": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Gun SZKK Lamp  2",
                                                           "identifier": "GUN_SZKK_L_2",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 256,
                                                                               "max_value": 1,
                                                                                "shift_by": 8,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                     "GUN_SZKK_L_3": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Gun SZKK Lamp  3",
                                                           "identifier": "GUN_SZKK_L_3",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 512,
                                                                               "max_value": 1,
                                                                                "shift_by": 9,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                     "GUN_SZKK_L_4": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Gun SZKK Lamp  4",
                                                           "identifier": "GUN_SZKK_L_4",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 1024,
                                                                               "max_value": 1,
                                                                                "shift_by": 10,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                        "LG_L_DOWN": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Landing Gear Left Down",
                                                           "identifier": "LG_L_DOWN",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 16384,
                                                                               "max_value": 1,
                                                                                "shift_by": 14,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                          "LG_L_UP": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Landing Gear Left Up",
                                                           "identifier": "LG_L_UP",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 8192,
                                                                               "max_value": 1,
                                                                                "shift_by": 13,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                        "LG_R_DOWN": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Landing Gear Right Down",
                                                           "identifier": "LG_R_DOWN",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14386,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 1,
                                                                               "max_value": 1,
                                                                                "shift_by": 0,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                          "LG_R_UP": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Landing Gear Right Up",
                                                           "identifier": "LG_R_UP",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 32768,
                                                                               "max_value": 1,
                                                                                "shift_by": 15,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                       "PITOT_LAMP": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "Pitot Lamp",
                                                           "identifier": "PITOT_LAMP",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 4096,
                                                                               "max_value": 1,
                                                                                "shift_by": 12,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     },
                                   "ZSK244_READY_L": {
                                                             "category": "Lamps",
                                                         "control_type": "led",
                                                          "description": "ZSK244 Ready Lamp",
                                                           "identifier": "ZSK244_READY_L",
                                                               "inputs": [  ],
                                                              "outputs": [ {
                                                                                 "address": 14378,
                                                                             "description": "0 if light is off, 1 if light is on",
                                                                                    "mask": 2048,
                                                                               "max_value": 1,
                                                                                "shift_by": 11,
                                                                                  "suffix": "",
                                                                                    "type": "integer"
                                                                         } ]
                                                     }
                               },
                      "Radio": {
                                   "FT_ZF_SWITCH": {
                                                                  "category": "Radio",
                                                              "control_type": "selector",
                                                               "description": "FT FT / Y ZF Mode Switch",
                                                                "identifier": "FT_ZF_SWITCH",
                                                                    "inputs": [ {
                                                                                  "description": "switch to previous or next state",
                                                                                    "interface": "fixed_step"
                                                                              }, {
                                                                                  "description": "set position",
                                                                                    "interface": "set_state",
                                                                                    "max_value": 1
                                                                              }, {
                                                                                     "argument": "TOGGLE",
                                                                                  "description": "Toggle switch state",
                                                                                    "interface": "action"
                                                                              } ],
                                                       "momentary_positions": "none",
                                                                   "outputs": [ {
                                                                                      "address": 14374,
                                                                                  "description": "selector position",
                                                                                         "mask": 1024,
                                                                                    "max_value": 1,
                                                                                     "shift_by": 10,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ],
                                                          "physical_variant": "limited_rotary"
                                                   },
                                   "FUG16_TUNING": {
                                                                  "category": "Radio",
                                                              "control_type": "discrete_dial",
                                                               "description": "Radio Tuning (+/-30 kHz)",
                                                                "identifier": "FUG16_TUNING",
                                                                    "inputs": [ {
                                                                                  "description": "switch to previous or next state",
                                                                                    "interface": "fixed_step"
                                                                              } ],
                                                       "momentary_positions": "none",
                                                                   "outputs": [ {
                                                                                      "address": 14378,
                                                                                  "description": "selector position",
                                                                                         "mask": 255,
                                                                                    "max_value": 200,
                                                                                     "shift_by": 0,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ],
                                                          "physical_variant": "infinite_rotary"
                                                   },
                                   "FUG16_VOLUME": {
                                                        "api_variant": "multiturn",
                                                           "category": "Radio",
                                                       "control_type": "analog_dial",
                                                        "description": "Radio Volume",
                                                         "identifier": "FUG16_VOLUME",
                                                             "inputs": [ {
                                                                              "description": "turn the dial left or right",
                                                                                "interface": "variable_step",
                                                                                "max_value": 65535,
                                                                           "suggested_step": 3200
                                                                       } ],
                                                            "outputs": [ {
                                                                               "address": 14376,
                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                  "mask": 65535,
                                                                             "max_value": 65535,
                                                                              "shift_by": 0,
                                                                                "suffix": "_KNOB_POS",
                                                                                  "type": "integer"
                                                                       } ]
                                                   },
                                     "RADIO_MODE": {
                                                                  "category": "Radio",
                                                              "control_type": "selector",
                                                               "description": "FuG 16ZY Radio Channel Selector",
                                                                "identifier": "RADIO_MODE",
                                                                    "inputs": [ {
                                                                                  "description": "switch to previous or next state",
                                                                                    "interface": "fixed_step"
                                                                              }, {
                                                                                  "description": "set position",
                                                                                    "interface": "set_state",
                                                                                    "max_value": 3
                                                                              } ],
                                                       "momentary_positions": "none",
                                                                   "outputs": [ {
                                                                                      "address": 14374,
                                                                                  "description": "selector position",
                                                                                         "mask": 192,
                                                                                    "max_value": 3,
                                                                                     "shift_by": 6,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ],
                                                          "physical_variant": "limited_rotary"
                                                   },
                                      "RADIO_WIP": {
                                                                  "category": "Radio",
                                                              "control_type": "selector",
                                                               "description": "FuG 16ZY Radio WIP",
                                                                "identifier": "RADIO_WIP",
                                                                    "inputs": [ {
                                                                                  "description": "switch to previous or next state",
                                                                                    "interface": "fixed_step"
                                                                              }, {
                                                                                  "description": "set position",
                                                                                    "interface": "set_state",
                                                                                    "max_value": 3
                                                                              } ],
                                                       "momentary_positions": "none",
                                                                   "outputs": [ {
                                                                                      "address": 14374,
                                                                                  "description": "selector position",
                                                                                         "mask": 768,
                                                                                    "max_value": 3,
                                                                                     "shift_by": 8,
                                                                                       "suffix": "",
                                                                                         "type": "integer"
                                                                              } ],
                                                          "physical_variant": "limited_rotary"
                                                   }
                               },
             "Weapon Control": {
                                        "BMB_FUSE_SEL": {
                                                                       "category": "Weapon Control",
                                                                   "control_type": "selector",
                                                                    "description": "Bomb Fusing Selector",
                                                                     "identifier": "BMB_FUSE_SEL",
                                                                         "inputs": [ {
                                                                                       "description": "switch to previous or next state",
                                                                                         "interface": "fixed_step"
                                                                                   }, {
                                                                                       "description": "set position",
                                                                                         "interface": "set_state",
                                                                                         "max_value": 4
                                                                                   } ],
                                                            "momentary_positions": "none",
                                                                        "outputs": [ {
                                                                                           "address": 14364,
                                                                                       "description": "selector position",
                                                                                              "mask": 7,
                                                                                         "max_value": 4,
                                                                                          "shift_by": 0,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ],
                                                               "physical_variant": "limited_rotary"
                                                        },
                                          "GUN1_AMM_C": {
                                                             "api_variant": "multiturn",
                                                                "category": "Weapon Control",
                                                            "control_type": "analog_dial",
                                                             "description": "Set Gun 1 Ammunition Count",
                                                              "identifier": "GUN1_AMM_C",
                                                                  "inputs": [ {
                                                                                   "description": "turn the dial left or right",
                                                                                     "interface": "variable_step",
                                                                                     "max_value": 65535,
                                                                                "suggested_step": 3200
                                                                            } ],
                                                                 "outputs": [ {
                                                                                    "address": 14356,
                                                                                "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                       "mask": 65535,
                                                                                  "max_value": 65535,
                                                                                   "shift_by": 0,
                                                                                     "suffix": "_KNOB_POS",
                                                                                       "type": "integer"
                                                                            } ]
                                                        },
                                          "GUN2_AMM_C": {
                                                             "api_variant": "multiturn",
                                                                "category": "Weapon Control",
                                                            "control_type": "analog_dial",
                                                             "description": "Set Gun 2 Ammunition Count",
                                                              "identifier": "GUN2_AMM_C",
                                                                  "inputs": [ {
                                                                                   "description": "turn the dial left or right",
                                                                                     "interface": "variable_step",
                                                                                     "max_value": 65535,
                                                                                "suggested_step": 3200
                                                                            } ],
                                                                 "outputs": [ {
                                                                                    "address": 14358,
                                                                                "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                       "mask": 65535,
                                                                                  "max_value": 65535,
                                                                                   "shift_by": 0,
                                                                                     "suffix": "_KNOB_POS",
                                                                                       "type": "integer"
                                                                            } ]
                                                        },
                                          "GUN3_AMM_C": {
                                                             "api_variant": "multiturn",
                                                                "category": "Weapon Control",
                                                            "control_type": "analog_dial",
                                                             "description": "Set Gun 3 Ammunition Count",
                                                              "identifier": "GUN3_AMM_C",
                                                                  "inputs": [ {
                                                                                   "description": "turn the dial left or right",
                                                                                     "interface": "variable_step",
                                                                                     "max_value": 65535,
                                                                                "suggested_step": 3200
                                                                            } ],
                                                                 "outputs": [ {
                                                                                    "address": 14360,
                                                                                "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                       "mask": 65535,
                                                                                  "max_value": 65535,
                                                                                   "shift_by": 0,
                                                                                     "suffix": "_KNOB_POS",
                                                                                       "type": "integer"
                                                                            } ]
                                                        },
                                          "GUN4_AMM_C": {
                                                             "api_variant": "multiturn",
                                                                "category": "Weapon Control",
                                                            "control_type": "analog_dial",
                                                             "description": "Set Gun 4 Ammunition Count",
                                                              "identifier": "GUN4_AMM_C",
                                                                  "inputs": [ {
                                                                                   "description": "turn the dial left or right",
                                                                                     "interface": "variable_step",
                                                                                     "max_value": 65535,
                                                                                "suggested_step": 3200
                                                                            } ],
                                                                 "outputs": [ {
                                                                                    "address": 14362,
                                                                                "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                       "mask": 65535,
                                                                                  "max_value": 65535,
                                                                                   "shift_by": 0,
                                                                                     "suffix": "_KNOB_POS",
                                                                                       "type": "integer"
                                                                            } ]
                                                        },
                                     "JETT_FUS_STORES": {
                                                                       "category": "Weapon Control",
                                                                   "control_type": "selector",
                                                                    "description": "Jettison Fuselage Stores",
                                                                     "identifier": "JETT_FUS_STORES",
                                                                         "inputs": [ {
                                                                                       "description": "switch to previous or next state",
                                                                                         "interface": "fixed_step"
                                                                                   }, {
                                                                                       "description": "set position",
                                                                                         "interface": "set_state",
                                                                                         "max_value": 1
                                                                                   }, {
                                                                                          "argument": "TOGGLE",
                                                                                       "description": "Toggle switch state",
                                                                                         "interface": "action"
                                                                                   } ],
                                                            "momentary_positions": "none",
                                                                        "outputs": [ {
                                                                                           "address": 14364,
                                                                                       "description": "selector position",
                                                                                              "mask": 8,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 3,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ],
                                                               "physical_variant": "limited_rotary"
                                                        },
                                          "MASTER_ARM": {
                                                                       "category": "Weapon Control",
                                                                   "control_type": "selector",
                                                                    "description": "Master Arm",
                                                                     "identifier": "MASTER_ARM",
                                                                         "inputs": [ {
                                                                                       "description": "switch to previous or next state",
                                                                                         "interface": "fixed_step"
                                                                                   }, {
                                                                                       "description": "set position",
                                                                                         "interface": "set_state",
                                                                                         "max_value": 1
                                                                                   }, {
                                                                                          "argument": "TOGGLE",
                                                                                       "description": "Toggle switch state",
                                                                                         "interface": "action"
                                                                                   } ],
                                                            "momentary_positions": "none",
                                                                        "outputs": [ {
                                                                                           "address": 14342,
                                                                                       "description": "selector position",
                                                                                              "mask": 16384,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 14,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ],
                                                               "physical_variant": "limited_rotary"
                                                        },
                                        "QUT_WING_ARM": {
                                                                       "category": "Weapon Control",
                                                                   "control_type": "selector",
                                                                    "description": "Outer Wing Guns Arm",
                                                                     "identifier": "QUT_WING_ARM",
                                                                         "inputs": [ {
                                                                                       "description": "switch to previous or next state",
                                                                                         "interface": "fixed_step"
                                                                                   }, {
                                                                                       "description": "set position",
                                                                                         "interface": "set_state",
                                                                                         "max_value": 1
                                                                                   }, {
                                                                                          "argument": "TOGGLE",
                                                                                       "description": "Toggle switch state",
                                                                                         "interface": "action"
                                                                                   } ],
                                                            "momentary_positions": "none",
                                                                        "outputs": [ {
                                                                                           "address": 14342,
                                                                                       "description": "selector position",
                                                                                              "mask": 32768,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 15,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ],
                                                               "physical_variant": "limited_rotary"
                                                        },
                                   "ROCKET_EMERG_JETT": {
                                                                       "category": "Weapon Control",
                                                                   "control_type": "selector",
                                                                    "description": "Rocket Emergency Release",
                                                                     "identifier": "ROCKET_EMERG_JETT",
                                                                         "inputs": [ {
                                                                                       "description": "switch to previous or next state",
                                                                                         "interface": "fixed_step"
                                                                                   }, {
                                                                                       "description": "set position",
                                                                                         "interface": "set_state",
                                                                                         "max_value": 1
                                                                                   }, {
                                                                                          "argument": "TOGGLE",
                                                                                       "description": "Toggle switch state",
                                                                                         "interface": "action"
                                                                                   } ],
                                                            "momentary_positions": "none",
                                                                        "outputs": [ {
                                                                                           "address": 14386,
                                                                                       "description": "selector position",
                                                                                              "mask": 1024,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 10,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ],
                                                               "physical_variant": "limited_rotary"
                                                        },
                                      "ROCKET_MAIN_SW": {
                                                                       "category": "Weapon Control",
                                                                   "control_type": "selector",
                                                                    "description": "Main Rocket Switch",
                                                                     "identifier": "ROCKET_MAIN_SW",
                                                                         "inputs": [ {
                                                                                       "description": "switch to previous or next state",
                                                                                         "interface": "fixed_step"
                                                                                   }, {
                                                                                       "description": "set position",
                                                                                         "interface": "set_state",
                                                                                         "max_value": 1
                                                                                   }, {
                                                                                          "argument": "TOGGLE",
                                                                                       "description": "Toggle switch state",
                                                                                         "interface": "action"
                                                                                   } ],
                                                            "momentary_positions": "none",
                                                                        "outputs": [ {
                                                                                           "address": 14386,
                                                                                       "description": "selector position",
                                                                                              "mask": 512,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 9,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ],
                                                               "physical_variant": "limited_rotary"
                                                        }
                               }
};
