docdata["Alphajet"] =
{
                           "Accelerometer": {
                                                "GMETER_SET": {
                                                                          "api_variant": "momentary_last_position",
                                                                             "category": "Accelerometer",
                                                                         "control_type": "selector",
                                                                          "description": "Push to set G-Meter",
                                                                           "identifier": "GMETER_SET",
                                                                               "inputs": [ {
                                                                                             "description": "switch to previous or next state",
                                                                                               "interface": "fixed_step"
                                                                                         }, {
                                                                                             "description": "set position",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 1
                                                                                         }, {
                                                                                                "argument": "TOGGLE",
                                                                                             "description": "Toggle switch state",
                                                                                               "interface": "action"
                                                                                         } ],
                                                                  "momentary_positions": "none",
                                                                              "outputs": [ {
                                                                                                 "address": 25600,
                                                                                             "description": "selector position",
                                                                                                    "mask": 1,
                                                                                               "max_value": 1,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ],
                                                                     "physical_variant": "push_button"
                                                              }
                                            },
                               "Altimeter": {
                                                "ALT_PRESS_SET": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Altimeter",
                                                                     "control_type": "analog_dial",
                                                                      "description": "Altimeter Pressure Setting",
                                                                       "identifier": "ALT_PRESS_SET",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 25602,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "ALT_RESET": {
                                                                             "api_variant": "momentary_last_position",
                                                                                "category": "Altimeter",
                                                                            "control_type": "selector",
                                                                             "description": "Altimeter Reset 10000ft",
                                                                              "identifier": "ALT_RESET",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25600,
                                                                                                "description": "selector position",
                                                                                                       "mask": 64,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 6,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "push_button"
                                                                 },
                                                      "HDG_SET": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Altimeter",
                                                                     "control_type": "analog_dial",
                                                                      "description": "Set Heading Bug",
                                                                       "identifier": "HDG_SET",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 25606,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                     "HRZ_CAGE": {
                                                                                "category": "Altimeter",
                                                                            "control_type": "selector",
                                                                             "description": "Cache Horizon Hide/Show",
                                                                              "identifier": "HRZ_CAGE",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25600,
                                                                                                "description": "selector position",
                                                                                                       "mask": 128,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 7,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                      "HRZ_SET": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Altimeter",
                                                                     "control_type": "analog_dial",
                                                                      "description": "Horizon Plane Set",
                                                                       "identifier": "HRZ_SET",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 25610,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                 "HRZ_STBY_SET": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Altimeter",
                                                                     "control_type": "analog_dial",
                                                                      "description": "Reset Standby Horizon",
                                                                       "identifier": "HRZ_STBY_SET",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 25608,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                      "IAS_SET": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Altimeter",
                                                                     "control_type": "analog_dial",
                                                                      "description": "IAS Index Setting",
                                                                       "identifier": "IAS_SET",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 25604,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 }
                                            },
                                "Avionics": {
                                                 "FLAPS_DN": {
                                                                         "api_variant": "momentary_last_position",
                                                                            "category": "Avionics",
                                                                        "control_type": "selector",
                                                                         "description": "Flaps Full Down",
                                                                          "identifier": "FLAPS_DN",
                                                                              "inputs": [ {
                                                                                            "description": "switch to previous or next state",
                                                                                              "interface": "fixed_step"
                                                                                        }, {
                                                                                            "description": "set position",
                                                                                              "interface": "set_state",
                                                                                              "max_value": 1
                                                                                        }, {
                                                                                               "argument": "TOGGLE",
                                                                                            "description": "Toggle switch state",
                                                                                              "interface": "action"
                                                                                        } ],
                                                                 "momentary_positions": "none",
                                                                             "outputs": [ {
                                                                                                "address": 25600,
                                                                                            "description": "selector position",
                                                                                                   "mask": 8,
                                                                                              "max_value": 1,
                                                                                               "shift_by": 3,
                                                                                                 "suffix": "",
                                                                                                   "type": "integer"
                                                                                        } ],
                                                                    "physical_variant": "push_button"
                                                             },
                                                "FLAPS_MID": {
                                                                         "api_variant": "momentary_last_position",
                                                                            "category": "Avionics",
                                                                        "control_type": "selector",
                                                                         "description": "Flaps Mid",
                                                                          "identifier": "FLAPS_MID",
                                                                              "inputs": [ {
                                                                                            "description": "switch to previous or next state",
                                                                                              "interface": "fixed_step"
                                                                                        }, {
                                                                                            "description": "set position",
                                                                                              "interface": "set_state",
                                                                                              "max_value": 1
                                                                                        }, {
                                                                                               "argument": "TOGGLE",
                                                                                            "description": "Toggle switch state",
                                                                                              "interface": "action"
                                                                                        } ],
                                                                 "momentary_positions": "none",
                                                                             "outputs": [ {
                                                                                                "address": 25600,
                                                                                            "description": "selector position",
                                                                                                   "mask": 4,
                                                                                              "max_value": 1,
                                                                                               "shift_by": 2,
                                                                                                 "suffix": "",
                                                                                                   "type": "integer"
                                                                                        } ],
                                                                    "physical_variant": "push_button"
                                                             },
                                                 "FLAPS_UP": {
                                                                         "api_variant": "momentary_last_position",
                                                                            "category": "Avionics",
                                                                        "control_type": "selector",
                                                                         "description": "Flaps Up",
                                                                          "identifier": "FLAPS_UP",
                                                                              "inputs": [ {
                                                                                            "description": "switch to previous or next state",
                                                                                              "interface": "fixed_step"
                                                                                        }, {
                                                                                            "description": "set position",
                                                                                              "interface": "set_state",
                                                                                              "max_value": 1
                                                                                        }, {
                                                                                               "argument": "TOGGLE",
                                                                                            "description": "Toggle switch state",
                                                                                              "interface": "action"
                                                                                        } ],
                                                                 "momentary_positions": "none",
                                                                             "outputs": [ {
                                                                                                "address": 25600,
                                                                                            "description": "selector position",
                                                                                                   "mask": 2,
                                                                                              "max_value": 1,
                                                                                               "shift_by": 1,
                                                                                                 "suffix": "",
                                                                                                   "type": "integer"
                                                                                        } ],
                                                                    "physical_variant": "push_button"
                                                             },
                                                  "GEAR_DN": {
                                                                         "api_variant": "momentary_last_position",
                                                                            "category": "Avionics",
                                                                        "control_type": "selector",
                                                                         "description": "Gear Down",
                                                                          "identifier": "GEAR_DN",
                                                                              "inputs": [ {
                                                                                            "description": "switch to previous or next state",
                                                                                              "interface": "fixed_step"
                                                                                        }, {
                                                                                            "description": "set position",
                                                                                              "interface": "set_state",
                                                                                              "max_value": 1
                                                                                        }, {
                                                                                               "argument": "TOGGLE",
                                                                                            "description": "Toggle switch state",
                                                                                              "interface": "action"
                                                                                        } ],
                                                                 "momentary_positions": "none",
                                                                             "outputs": [ {
                                                                                                "address": 25600,
                                                                                            "description": "selector position",
                                                                                                   "mask": 16,
                                                                                              "max_value": 1,
                                                                                               "shift_by": 4,
                                                                                                 "suffix": "",
                                                                                                   "type": "integer"
                                                                                        } ],
                                                                    "physical_variant": "push_button"
                                                             },
                                                  "GEAR_UP": {
                                                                         "api_variant": "momentary_last_position",
                                                                            "category": "Avionics",
                                                                        "control_type": "selector",
                                                                         "description": "Gear UP",
                                                                          "identifier": "GEAR_UP",
                                                                              "inputs": [ {
                                                                                            "description": "switch to previous or next state",
                                                                                              "interface": "fixed_step"
                                                                                        }, {
                                                                                            "description": "set position",
                                                                                              "interface": "set_state",
                                                                                              "max_value": 1
                                                                                        }, {
                                                                                               "argument": "TOGGLE",
                                                                                            "description": "Toggle switch state",
                                                                                              "interface": "action"
                                                                                        } ],
                                                                 "momentary_positions": "none",
                                                                             "outputs": [ {
                                                                                                "address": 25600,
                                                                                            "description": "selector position",
                                                                                                   "mask": 32,
                                                                                              "max_value": 1,
                                                                                               "shift_by": 5,
                                                                                                 "suffix": "",
                                                                                                   "type": "integer"
                                                                                        } ],
                                                                    "physical_variant": "push_button"
                                                             }
                                            },
                           "Control Panel": {
                                                 "ALARM_SONORE": {
                                                                                "category": "Control Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Alarme Sonore, ON/OFF",
                                                                              "identifier": "ALARM_SONORE",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25600,
                                                                                                "description": "selector position",
                                                                                                       "mask": 32768,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 15,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                    "CANOPY_SW": {
                                                                                "category": "Control Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Cockpit Lever Open/Close",
                                                                              "identifier": "CANOPY_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 128,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 7,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                    "CENT_GYRO": {
                                                                                "category": "Control Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Centrale Gyroscopique, ON/OFF",
                                                                              "identifier": "CENT_GYRO",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 8,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 3,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                     "ELC_PUMP": {
                                                                                "category": "Control Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Electropompe, ON/OFF",
                                                                              "identifier": "ELC_PUMP",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 32,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 5,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                  "HRZ_SECOURS": {
                                                                                "category": "Control Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Horizon Secours, ON/OFF",
                                                                              "identifier": "HRZ_SECOURS",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 16,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 4,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                   "PITOT_HEAT": {
                                                                                "category": "Control Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Pitot Heat, ON/OFF",
                                                                              "identifier": "PITOT_HEAT",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 4,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 2,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                "SMOKE_SIDE_SW": {
                                                                                "category": "Control Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Side Smoke System Right/Left",
                                                                              "identifier": "SMOKE_SIDE_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 64,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 6,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 }
                                            },
                         "Electric System": {
                                                    "CRASH_BAR": {
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Crash Bar Switch",
                                                                              "identifier": "CRASH_BAR",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 8192,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 13,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                    "DELESTAGE": {
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Delestage",
                                                                              "identifier": "DELESTAGE",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 32768,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 15,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                     "GEN_L_SW": {
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Left Generator Switch",
                                                                              "identifier": "GEN_L_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 512,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 9,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                     "GEN_R_SW": {
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Right Generator Switch",
                                                                              "identifier": "GEN_R_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 1024,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 10,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                  "INVERT_L_SW": {
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Left Inverter Switch",
                                                                              "identifier": "INVERT_L_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 2048,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 11,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                  "INVERT_R_SW": {
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Right Inverter Switch",
                                                                              "identifier": "INVERT_R_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 4096,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 12,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                "MASTER_BAT_SW": {
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Master Battery Switch",
                                                                              "identifier": "MASTER_BAT_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 256,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 8,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                  "WARN_L_TEST": {
                                                                             "api_variant": "momentary_last_position",
                                                                                "category": "Electric System",
                                                                            "control_type": "selector",
                                                                             "description": "Warning Light Test",
                                                                              "identifier": "WARN_L_TEST",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 25616,
                                                                                                "description": "selector position",
                                                                                                       "mask": 16384,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 14,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "push_button"
                                                                 }
                                            },
                            "Engine Panel": {
                                                       "ENG_START_L": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Left Engine Start, START/VENT/OFF",
                                                                                   "identifier": "ENG_START_L",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 2
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 3,
                                                                                                       "max_value": 2,
                                                                                                        "shift_by": 0,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "3_position_switch"
                                                                      },
                                                       "ENG_START_R": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Right Engine Start, START/VENT/OFF",
                                                                                   "identifier": "ENG_START_R",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 2
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 12,
                                                                                                       "max_value": 2,
                                                                                                        "shift_by": 2,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "3_position_switch"
                                                                      },
                                                        "FUEL_CUT_L": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Fuel Cutoff Left",
                                                                                   "identifier": "FUEL_CUT_L",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 256,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 8,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "toggle_switch"
                                                                      },
                                                        "FUEL_CUT_R": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Fuel Cutoff Right",
                                                                                   "identifier": "FUEL_CUT_R",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 512,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 9,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "toggle_switch"
                                                                      },
                                                "LOW_PRESS_PUMP_BPD": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Low Pressure Pump, BPD",
                                                                                   "identifier": "LOW_PRESS_PUMP_BPD",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 32,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 5,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "toggle_switch"
                                                                      },
                                                "LOW_PRESS_PUMP_BPG": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Low Pressure Pump, BPG",
                                                                                   "identifier": "LOW_PRESS_PUMP_BPG",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 16,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 4,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "toggle_switch"
                                                                      },
                                                 "PROTECT_COVER_BPD": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Protective Cover, BPD",
                                                                                   "identifier": "PROTECT_COVER_BPD",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 128,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 7,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "toggle_switch"
                                                                      },
                                                 "PROTECT_COVER_BPG": {
                                                                                     "category": "Engine Panel",
                                                                                 "control_type": "selector",
                                                                                  "description": "Protective Cover, BPG",
                                                                                   "identifier": "PROTECT_COVER_BPG",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 25618,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 64,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 6,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "toggle_switch"
                                                                      }
                                            },
                 "External Aircraft Model": {
                                                "EXT_BOT_TAIL_LIGHTS": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Bottom Tail Lights (red)",
                                                                             "identifier": "EXT_BOT_TAIL_LIGHTS",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25684,
                                                                                               "description": "Bottom Tail Lights (red)",
                                                                                                      "mask": 8192,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 13,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                    "EXT_GEAR_LIGHTS": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Left Gear Light (white)",
                                                                             "identifier": "EXT_GEAR_LIGHTS",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25684,
                                                                                               "description": "Left Gear Light (white)",
                                                                                                      "mask": 2048,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 11,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                    "EXT_NOSE_LIGHTS": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Nose and Right Gear Lights (white)",
                                                                             "identifier": "EXT_NOSE_LIGHTS",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25684,
                                                                                               "description": "Nose and Right Gear Lights (white)",
                                                                                                      "mask": 4096,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 12,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                "EXT_POSITION_LIGHTS": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Position Lights (green/red)",
                                                                             "identifier": "EXT_POSITION_LIGHTS",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25684,
                                                                                               "description": "Position Lights (green/red)",
                                                                                                      "mask": 512,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 9,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                    "EXT_SPEED_BRAKE": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Speed Brake",
                                                                             "identifier": "EXT_SPEED_BRAKE",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25686,
                                                                                               "description": "Speed Brake",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                  "EXT_STROBE_LIGHTS": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Strobe Lights (white)",
                                                                             "identifier": "EXT_STROBE_LIGHTS",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25684,
                                                                                               "description": "Strobe Lights (white)",
                                                                                                      "mask": 1024,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 10,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                       "EXT_WOW_LEFT": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Weight ON Wheels Left Gear",
                                                                             "identifier": "EXT_WOW_LEFT",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25688,
                                                                                               "description": "Weight ON Wheels Left Gear",
                                                                                                      "mask": 1,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                       "EXT_WOW_NOSE": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Weight ON Wheels Nose Gear",
                                                                             "identifier": "EXT_WOW_NOSE",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25684,
                                                                                               "description": "Weight ON Wheels Nose Gear",
                                                                                                      "mask": 16384,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 14,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                      "EXT_WOW_RIGHT": {
                                                                               "category": "External Aircraft Model",
                                                                           "control_type": "metadata",
                                                                            "description": "Weight ON Wheels Right Gear",
                                                                             "identifier": "EXT_WOW_RIGHT",
                                                                                 "inputs": [  ],
                                                                                "outputs": [ {
                                                                                                   "address": 25684,
                                                                                               "description": "Weight ON Wheels Right Gear",
                                                                                                      "mask": 32768,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 15,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       }
                                            },
                                  "Gauges": {
                                                   "AHRZ_PITCH": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Artificial Horizon Pitch",
                                                                       "identifier": "AHRZ_PITCH",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25664,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "AHRZ_ROLL": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Artificial Horizon Roll",
                                                                       "identifier": "AHRZ_ROLL",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25662,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                 "ALT_DRUM_10K": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Altimeter 10000ft Drum",
                                                                       "identifier": "ALT_DRUM_10K",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25670,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                "ALT_NEEDLE_1K": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Altimeter 1000ft Needle",
                                                                       "identifier": "ALT_NEEDLE_1K",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25668,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "AOA_UNITS": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "AOA_Units",
                                                                       "identifier": "AOA_UNITS",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25660,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "CANOPY_POS": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Canopy Position",
                                                                       "identifier": "CANOPY_POS",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25620,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                     "CHRONO_H": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Chrono Hour",
                                                                       "identifier": "CHRONO_H",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25644,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                     "CHRONO_M": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Chrono Minute",
                                                                       "identifier": "CHRONO_M",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25646,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                     "CHRONO_S": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Chrono Second",
                                                                       "identifier": "CHRONO_S",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25648,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                      "CLOCK_H": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Clock Hour",
                                                                       "identifier": "CLOCK_H",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25636,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                      "CLOCK_M": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Clock Minute",
                                                                       "identifier": "CLOCK_M",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25638,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                      "CLOCK_S": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Clock Second",
                                                                       "identifier": "CLOCK_S",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25640,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "COMP_ROSE": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Compass Rose",
                                                                       "identifier": "COMP_ROSE",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25672,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                     "ENG_FF_L": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Engine FF Left",
                                                                       "identifier": "ENG_FF_L",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25626,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                     "ENG_FF_R": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Engine FF Right",
                                                                       "identifier": "ENG_FF_R",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25632,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "ENG_RPM_L": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Engine RPM Left",
                                                                       "identifier": "ENG_RPM_L",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25624,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "ENG_RPM_R": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Engine RPM Right",
                                                                       "identifier": "ENG_RPM_R",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25630,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "ENG_TEMP_L": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Engine Temperature Left",
                                                                       "identifier": "ENG_TEMP_L",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25628,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "ENG_TEMP_R": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Engine Temperature Right",
                                                                       "identifier": "ENG_TEMP_R",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25634,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                     "FLAP_POS": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "FLAP Position Gauge",
                                                                       "identifier": "FLAP_POS",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25682,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "FUEL_TOTAL": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Total Fuel",
                                                                       "identifier": "FUEL_TOTAL",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25674,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                       "G_LOAD": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "G-Load",
                                                                       "identifier": "G_LOAD",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25654,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                        "G_MAX": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "G-Load Maximum",
                                                                       "identifier": "G_MAX",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25656,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                        "G_MIN": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "G-Load Minimum",
                                                                       "identifier": "G_MIN",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25658,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "HYD_PRESS1": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Hydraulic Pressure Gauge 1",
                                                                       "identifier": "HYD_PRESS1",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25678,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "HYD_PRESS2": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Hydraulic Pressure Gauge 2",
                                                                       "identifier": "HYD_PRESS2",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25680,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "IAS_GAUGE": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "IAS Gauge",
                                                                       "identifier": "IAS_GAUGE",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25650,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                         "JOUR": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Jour",
                                                                       "identifier": "JOUR",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25642,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "MACH_METER": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Mach Meter",
                                                                       "identifier": "MACH_METER",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25676,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                       "MANCHE": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Manche",
                                                                       "identifier": "MANCHE",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25622,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                   "TRIM_PITCH": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Trim Pitch",
                                                                       "identifier": "TRIM_PITCH",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25666,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "VERT_VELO": {
                                                                         "category": "Gauges",
                                                                     "control_type": "analog_gauge",
                                                                      "description": "Vertical Velocity",
                                                                       "identifier": "VERT_VELO",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 25652,
                                                                                         "description": "gauge position",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 }
                                            },
                            "Light System": {
                                                  "LIGHTS_ANTICOL": {
                                                                                   "category": "Light System",
                                                                               "control_type": "selector",
                                                                                "description": "Anticollision Lights, ON/OFF",
                                                                                 "identifier": "LIGHTS_ANTICOL",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 25600,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 4096,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 12,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                  "LIGHTS_A_ALARM": {
                                                                                   "category": "Light System",
                                                                               "control_type": "selector",
                                                                                "description": "High Alpha Alarm, HIDRAG/OFF/LOWDRAG",
                                                                                 "identifier": "LIGHTS_A_ALARM",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 2
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 25616,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 3,
                                                                                                     "max_value": 2,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "3_position_switch"
                                                                    },
                                                "LIGHTS_FORMATION": {
                                                                                   "category": "Light System",
                                                                               "control_type": "selector",
                                                                                "description": "Formation Lights, ON/OFF",
                                                                                 "identifier": "LIGHTS_FORMATION",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 25600,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 1024,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 10,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                    "LIGHTS_ITENT": {
                                                                                   "category": "Light System",
                                                                               "control_type": "selector",
                                                                                "description": "Intensity, STRONG/LOWVIS",
                                                                                 "identifier": "LIGHTS_ITENT",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 25600,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 2048,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 11,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                     "LIGHTS_LAND": {
                                                                                   "category": "Light System",
                                                                               "control_type": "selector",
                                                                                "description": "Lights, OFF/TAXI/LANDING",
                                                                                 "identifier": "LIGHTS_LAND",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 2
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 25600,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 24576,
                                                                                                     "max_value": 2,
                                                                                                      "shift_by": 13,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "3_position_switch"
                                                                    },
                                                      "LIGHTS_NAV": {
                                                                                   "category": "Light System",
                                                                               "control_type": "selector",
                                                                                "description": "Navigation Lights, FLASH/OFF/STEADY",
                                                                                 "identifier": "LIGHTS_NAV",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 2
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 25600,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 768,
                                                                                                     "max_value": 2,
                                                                                                      "shift_by": 8,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "3_position_switch"
                                                                    }
                                            },
                           "Oxygen System": {
                                                "QXY_NORM_SW": {
                                                                              "category": "Oxygen System",
                                                                          "control_type": "selector",
                                                                           "description": "Oxygen Switch Normal/100%",
                                                                            "identifier": "QXY_NORM_SW",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 1
                                                                                          }, {
                                                                                                 "argument": "TOGGLE",
                                                                                              "description": "Toggle switch state",
                                                                                                "interface": "action"
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 25618,
                                                                                              "description": "selector position",
                                                                                                     "mask": 1024,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 10,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "toggle_switch"
                                                               },
                                                  "QXY_ON_SW": {
                                                                              "category": "Oxygen System",
                                                                          "control_type": "selector",
                                                                           "description": "Oxygen Switch Open/Close",
                                                                            "identifier": "QXY_ON_SW",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 1
                                                                                          }, {
                                                                                                 "argument": "TOGGLE",
                                                                                              "description": "Toggle switch state",
                                                                                                "interface": "action"
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 25618,
                                                                                              "description": "selector position",
                                                                                                     "mask": 2048,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 11,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "toggle_switch"
                                                               }
                                            },
                                   "Radio": {
                                                "UHF_VOL": {
                                                                   "category": "Radio",
                                                               "control_type": "limited_dial",
                                                                "description": "UHF Volume",
                                                                 "identifier": "UHF_VOL",
                                                                     "inputs": [ {
                                                                                   "description": "set the position of the dial",
                                                                                     "interface": "set_state",
                                                                                     "max_value": 65535
                                                                               }, {
                                                                                      "description": "turn the dial left or right",
                                                                                        "interface": "variable_step",
                                                                                        "max_value": 65535,
                                                                                   "suggested_step": 3200
                                                                               } ],
                                                                    "outputs": [ {
                                                                                       "address": 25612,
                                                                                   "description": "position of the potentiometer",
                                                                                          "mask": 65535,
                                                                                     "max_value": 65535,
                                                                                      "shift_by": 0,
                                                                                        "suffix": "",
                                                                                          "type": "integer"
                                                                               } ]
                                                           },
                                                "VHF_VOL": {
                                                                   "category": "Radio",
                                                               "control_type": "limited_dial",
                                                                "description": "VHF Volume",
                                                                 "identifier": "VHF_VOL",
                                                                     "inputs": [ {
                                                                                   "description": "set the position of the dial",
                                                                                     "interface": "set_state",
                                                                                     "max_value": 65535
                                                                               }, {
                                                                                      "description": "turn the dial left or right",
                                                                                        "interface": "variable_step",
                                                                                        "max_value": 65535,
                                                                                   "suggested_step": 3200
                                                                               } ],
                                                                    "outputs": [ {
                                                                                       "address": 25614,
                                                                                   "description": "position of the potentiometer",
                                                                                          "mask": 65535,
                                                                                     "max_value": 65535,
                                                                                      "shift_by": 0,
                                                                                        "suffix": "",
                                                                                          "type": "integer"
                                                                               } ]
                                                           }
                                            },
    "Warning, Caution and IndicatorLights": {
                                                        "AF_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "AF Lamp (yellow)",
                                                                      "identifier": "AF_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25618,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 16384,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 14,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                     "BRAKE_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Brake Lamp (yellow)",
                                                                      "identifier": "BRAKE_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 4,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 2,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                      "FLAP_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "FLAP Lamp (yellow)",
                                                                      "identifier": "FLAP_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 64,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 6,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                  "FUEL_250_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Fuel 250L Light (red)",
                                                                      "identifier": "FUEL_250_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 8,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 3,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                "FUEL_LWING_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Left Wing Fuel Lamp (yellow)",
                                                                      "identifier": "FUEL_LWING_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 16,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 4,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                "FUEL_RWING_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Right Wing Fuel Lamp (yellow)",
                                                                      "identifier": "FUEL_RWING_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 32,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 5,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                  "GEAR_BAY_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Gear Baydoor Light (red)",
                                                                      "identifier": "GEAR_BAY_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25618,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 4096,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 12,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                  "GEAR_HND_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Gear Handle Light (red)",
                                                                      "identifier": "GEAR_HND_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 1,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 0,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                      "GEAR_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Gear Lights (green)",
                                                                      "identifier": "GEAR_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25618,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 8192,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 13,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                "LIGHT_10K_FT": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Warning Lamp 10000ft (yellow)",
                                                                      "identifier": "LIGHT_10K_FT",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25618,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 32768,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 15,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                     "SMOKE_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Smoke Light (green)",
                                                                      "identifier": "SMOKE_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 2,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 1,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                    "TEMP_L_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Left Temperature Lamp (yellow)",
                                                                      "identifier": "TEMP_L_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 128,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 7,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                    "TEMP_R_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Right Temperature Lamp (yellow)",
                                                                      "identifier": "TEMP_R_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 25684,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 256,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 8,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                }
                                            }
};
