docdata["I-16"] =
{
                                  "Common": {
                                                "CRS_CAGE_KNOB": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Common",
                                                                     "control_type": "analog_dial",
                                                                      "description": "Course Cage Knob",
                                                                       "identifier": "CRS_CAGE_KNOB",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 16414,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                       "DOOR_L": {
                                                                                "category": "Common",
                                                                            "control_type": "selector",
                                                                             "description": "Left Door",
                                                                              "identifier": "DOOR_L",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 16394,
                                                                                                "description": "selector position",
                                                                                                       "mask": 16384,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 14,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                       "DOOR_R": {
                                                                                "category": "Common",
                                                                            "control_type": "selector",
                                                                             "description": "Right Door",
                                                                              "identifier": "DOOR_R",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 16394,
                                                                                                "description": "selector position",
                                                                                                       "mask": 32768,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 15,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                    "PRESS_SET": {
                                                                         "category": "Common",
                                                                     "control_type": "limited_dial",
                                                                      "description": "Set Pressure",
                                                                       "identifier": "PRESS_SET",
                                                                           "inputs": [ {
                                                                                         "description": "set the position of the dial",
                                                                                           "interface": "set_state",
                                                                                           "max_value": 65535
                                                                                     }, {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 16416,
                                                                                         "description": "position of the potentiometer",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                  "SEAT_HEIGHT": {
                                                                                "category": "Common",
                                                                            "control_type": "selector",
                                                                             "description": "Seat Level",
                                                                              "identifier": "SEAT_HEIGHT",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 4
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 16412,
                                                                                                "description": "selector position",
                                                                                                       "mask": 224,
                                                                                                  "max_value": 4,
                                                                                                   "shift_by": 5,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                 "SIGHT_FILTER": {
                                                                                "category": "Common",
                                                                            "control_type": "selector",
                                                                             "description": "Sight Filter",
                                                                              "identifier": "SIGHT_FILTER",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 16412,
                                                                                                "description": "selector position",
                                                                                                       "mask": 512,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 9,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                   "SIGHT_MECH": {
                                                                                "category": "Common",
                                                                            "control_type": "selector",
                                                                             "description": "Mech Sight",
                                                                              "identifier": "SIGHT_MECH",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 16412,
                                                                                                "description": "selector position",
                                                                                                       "mask": 256,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 8,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 }
                                            },
                                "Electric": {
                                                          "ACCU": {
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Accumulator",
                                                                               "identifier": "ACCU",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 8,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 3,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                    "CLOCK_HEAT": {
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Clock Heat",
                                                                               "identifier": "CLOCK_HEAT",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 1,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                     "CPT_LIGHT": {
                                                                          "category": "Electric",
                                                                      "control_type": "limited_dial",
                                                                       "description": "Cockpit Light Rheostat",
                                                                        "identifier": "CPT_LIGHT",
                                                                            "inputs": [ {
                                                                                          "description": "set the position of the dial",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 65535
                                                                                      }, {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 16388,
                                                                                          "description": "position of the potentiometer",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  },
                                                  "FIRE_TORCH_L": {
                                                                              "api_variant": "momentary_last_position",
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Fire Left Torch",
                                                                               "identifier": "FIRE_TORCH_L",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 64,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 6,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "push_button"
                                                                  },
                                                  "FIRE_TORCH_R": {
                                                                              "api_variant": "momentary_last_position",
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Fire Right Torch",
                                                                               "identifier": "FIRE_TORCH_R",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 256,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 8,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "push_button"
                                                                  },
                                                     "NAV_LIGHT": {
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Nav Light",
                                                                               "identifier": "NAV_LIGHT",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 4,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 2,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                "NAV_LIGHT_TEST": {
                                                                              "api_variant": "momentary_last_position",
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Nav Light Test",
                                                                               "identifier": "NAV_LIGHT_TEST",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 512,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 9,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "push_button"
                                                                  },
                                                    "PITOT_HEAT": {
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Pitot Heat",
                                                                               "identifier": "PITOT_HEAT",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 2,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 1,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                         "RADIO": {
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Radio",
                                                                               "identifier": "RADIO",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 32,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 5,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                 "ROCK_BOMB_ARM": {
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Rockets/Bombs Master Arm",
                                                                               "identifier": "ROCK_BOMB_ARM",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16394,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 8192,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 13,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                         "SHUNT": {
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Shunt",
                                                                               "identifier": "SHUNT",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 16,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 4,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                     "SIGHT_DIM": {
                                                                          "category": "Electric",
                                                                      "control_type": "limited_dial",
                                                                       "description": "Sight Dimmer Rheostat",
                                                                        "identifier": "SIGHT_DIM",
                                                                            "inputs": [ {
                                                                                          "description": "set the position of the dial",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 65535
                                                                                      }, {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 16386,
                                                                                          "description": "position of the potentiometer",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  },
                                                    "TORCH_JETT": {
                                                                              "api_variant": "momentary_last_position",
                                                                                 "category": "Electric",
                                                                             "control_type": "selector",
                                                                              "description": "Torches Jettison",
                                                                               "identifier": "TORCH_JETT",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 16384,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 128,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 7,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "push_button"
                                                                  }
                                            },
                 "External Aircraft Model": {
                                                 "EXT_POSITION_LIGHT_LEFT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Left Position Light (red)",
                                                                                  "identifier": "EXT_POSITION_LIGHT_LEFT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 16412,
                                                                                                    "description": "Left Position Light (red)",
                                                                                                           "mask": 4096,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 12,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                "EXT_POSITION_LIGHT_RIGHT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Right Position Light (green)",
                                                                                  "identifier": "EXT_POSITION_LIGHT_RIGHT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 16412,
                                                                                                    "description": "Right Position Light (green)",
                                                                                                           "mask": 8192,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 13,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                            "EXT_WOW_LEFT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Weight ON Wheels Left Gear",
                                                                                  "identifier": "EXT_WOW_LEFT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 16488,
                                                                                                    "description": "Weight ON Wheels Left Gear",
                                                                                                           "mask": 1,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                           "EXT_WOW_RIGHT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Weight ON Wheels Right Gear",
                                                                                  "identifier": "EXT_WOW_RIGHT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 16412,
                                                                                                    "description": "Weight ON Wheels Right Gear",
                                                                                                           "mask": 32768,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 15,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                            "EXT_WOW_TAIL": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Weight ON Wheels Tail Gear",
                                                                                  "identifier": "EXT_WOW_TAIL",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 16412,
                                                                                                    "description": "Weight ON Wheels Tail Gear",
                                                                                                           "mask": 16384,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 14,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            }
                                            },
                                   "Flaps": {
                                                "FLAPS_HANDLE": {
                                                                     "api_variant": "multiturn",
                                                                        "category": "Flaps",
                                                                    "control_type": "analog_dial",
                                                                     "description": "Flaps Handle",
                                                                      "identifier": "FLAPS_HANDLE",
                                                                          "inputs": [ {
                                                                                           "description": "turn the dial left or right",
                                                                                             "interface": "variable_step",
                                                                                             "max_value": 65535,
                                                                                        "suggested_step": 3200
                                                                                    } ],
                                                                         "outputs": [ {
                                                                                            "address": 16392,
                                                                                        "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                               "mask": 65535,
                                                                                          "max_value": 65535,
                                                                                           "shift_by": 0,
                                                                                             "suffix": "_KNOB_POS",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                }
                                            },
                                  "Gauges": {
                                                         "AIRSPEED": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Airspeed Indicator",
                                                                           "identifier": "AIRSPEED",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16432,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                         "AMPMETER": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Amperemeter",
                                                                           "identifier": "AMPMETER",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16466,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                     "BARO_ALT_100": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Altimeter 100m",
                                                                           "identifier": "BARO_ALT_100",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16442,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                    "BARO_ALT_1000": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Altimeter 1000m",
                                                                           "identifier": "BARO_ALT_1000",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16440,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                     "BARO_ALT_SEL": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Altimeter Pressure",
                                                                           "identifier": "BARO_ALT_SEL",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16444,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                          "CH_TEMP": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Cylinder Head Temperature Gauge",
                                                                           "identifier": "CH_TEMP",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16446,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                  "CLIMB_INDICATOR": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Climb Indicator",
                                                                           "identifier": "CLIMB_INDICATOR",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16460,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                          "CLOCK_H": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Clock Hours",
                                                                           "identifier": "CLOCK_H",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16424,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                          "CLOCK_M": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Clock Minutes",
                                                                           "identifier": "CLOCK_M",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16426,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                          "CLOCK_S": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Clock Seconds",
                                                                           "identifier": "CLOCK_S",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16428,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                        "COMP_BANK": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Compass Bank",
                                                                           "identifier": "COMP_BANK",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16436,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                         "COMP_CRS": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Compass Course",
                                                                           "identifier": "COMP_CRS",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16434,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                       "COMP_PITCH": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Compass Pitch",
                                                                           "identifier": "COMP_PITCH",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16438,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                       "DOOR_POS_L": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Left Door Position",
                                                                           "identifier": "DOOR_POS_L",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16484,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                       "DOOR_POS_R": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Right Door Position",
                                                                           "identifier": "DOOR_POS_R",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16486,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                        "ENG_RPM_G": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Engine RPM Gauge",
                                                                           "identifier": "ENG_RPM_G",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16430,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                  "FLAPS_INDICATOR": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Flaps Indicator",
                                                                           "identifier": "FLAPS_INDICATOR",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16464,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                       "FUEL_GAUGE": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Fuel Gauge",
                                                                           "identifier": "FUEL_GAUGE",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16462,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                       "FUEL_PRESS": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Fuel Pressure Gauge",
                                                                           "identifier": "FUEL_PRESS",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16452,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                       "GEAR_POS_L": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Left Gear Position Indicator",
                                                                           "identifier": "GEAR_POS_L",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16480,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                       "GEAR_POS_R": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Right Gear Position Indicator",
                                                                           "identifier": "GEAR_POS_R",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16482,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                   "MANIFOLD_PRESS": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Manifold Pressure Gauge",
                                                                           "identifier": "MANIFOLD_PRESS",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16454,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                        "OIL_PRESS": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Oil Pressure Gauge",
                                                                           "identifier": "OIL_PRESS",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16450,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                         "OIL_TEMP": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Oil Temperature Gauge",
                                                                           "identifier": "OIL_TEMP",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16448,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                "PANEL_SHAKE_CLOCK": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Cockpit Panel Clockwise Shake",
                                                                           "identifier": "PANEL_SHAKE_CLOCK",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16474,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                  "PANEL_SHAKE_FWD": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Cockpit Panel Forward Shake",
                                                                           "identifier": "PANEL_SHAKE_FWD",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16472,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                  "PANEL_SHAKE_HOR": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Cockpit Panel Horizontal Shake",
                                                                           "identifier": "PANEL_SHAKE_HOR",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16470,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                 "PANEL_SHAKE_VERT": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Cockpit Panel Vertikal Shake",
                                                                           "identifier": "PANEL_SHAKE_VERT",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16468,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                         "QXY_FLOW": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Oxygen Flow Manometer",
                                                                           "identifier": "QXY_FLOW",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16478,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                        "QXY_METER": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Oxygen Manometer",
                                                                           "identifier": "QXY_METER",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16476,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                   "SLIP_INDICATOR": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Slip Indicator",
                                                                           "identifier": "SLIP_INDICATOR",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16458,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                   "TURN_INDICATOR": {
                                                                             "category": "Gauges",
                                                                         "control_type": "analog_gauge",
                                                                          "description": "Turn Indicator",
                                                                           "identifier": "TURN_INDICATOR",
                                                                               "inputs": [  ],
                                                                              "outputs": [ {
                                                                                                 "address": 16456,
                                                                                             "description": "gauge position",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     }
                                            },
                                    "Gear": {
                                                "BRAKE_SPRING": {
                                                                               "category": "Gear",
                                                                           "control_type": "selector",
                                                                            "description": "Brake Spring Handle",
                                                                             "identifier": "BRAKE_SPRING",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 16384,
                                                                                               "description": "selector position",
                                                                                                      "mask": 4096,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 12,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                 "GEAR_DIRCET": {
                                                                               "category": "Gear",
                                                                           "control_type": "selector",
                                                                            "description": "Gear Direction",
                                                                             "identifier": "GEAR_DIRCET",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 16384,
                                                                                               "description": "selector position",
                                                                                                      "mask": 2048,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 11,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                 "GEAR_HANDLE": {
                                                                     "api_variant": "multiturn",
                                                                        "category": "Gear",
                                                                    "control_type": "analog_dial",
                                                                     "description": "Gear Handle",
                                                                      "identifier": "GEAR_HANDLE",
                                                                          "inputs": [ {
                                                                                           "description": "turn the dial left or right",
                                                                                             "interface": "variable_step",
                                                                                             "max_value": 65535,
                                                                                        "suggested_step": 3200
                                                                                    } ],
                                                                         "outputs": [ {
                                                                                            "address": 16390,
                                                                                        "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                               "mask": 65535,
                                                                                          "max_value": 65535,
                                                                                           "shift_by": 0,
                                                                                             "suffix": "_KNOB_POS",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                   "GEAR_LOCK": {
                                                                               "category": "Gear",
                                                                           "control_type": "selector",
                                                                            "description": "Gear Lock",
                                                                             "identifier": "GEAR_LOCK",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 16384,
                                                                                               "description": "selector position",
                                                                                                      "mask": 1024,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 10,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                }
                                            },
                                   "Motor": {
                                                 "ENG_COWL_FLAPS": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Motor",
                                                                       "control_type": "analog_dial",
                                                                        "description": "Motor Cowl Flaps",
                                                                         "identifier": "ENG_COWL_FLAPS",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16408,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                     "FUEL_VALVE": {
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Fuel Valve",
                                                                                "identifier": "FUEL_VALVE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16394,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 128,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 7,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                        "MAGNETO": {
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Magneto 0/1/2/1+2",
                                                                                "identifier": "MAGNETO",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 3
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16384,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 24576,
                                                                                                    "max_value": 3,
                                                                                                     "shift_by": 13,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                    "MAN_RATCHET": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Manual Ratchet Relay",
                                                                                "identifier": "MAN_RATCHET",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16394,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 256,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 8,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   },
                                                            "MIX": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Motor",
                                                                       "control_type": "analog_dial",
                                                                        "description": "Mixture",
                                                                         "identifier": "MIX",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16404,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                      "MOTOR_OFF": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Motor Shutdown",
                                                                                "identifier": "MOTOR_OFF",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16384,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 32768,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 15,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   },
                                                        "OIL_RAD": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Motor",
                                                                       "control_type": "analog_dial",
                                                                        "description": "Oil Radiator",
                                                                         "identifier": "OIL_RAD",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16410,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                    "PRI_FUEL_SW": {
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Primary Fuel Switch",
                                                                                "identifier": "PRI_FUEL_SW",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16394,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 24,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 3,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                        "RATCHET": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Ratchet Relay",
                                                                                "identifier": "RATCHET",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16394,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 1,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 0,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   },
                                                            "RPM": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Motor",
                                                                       "control_type": "analog_dial",
                                                                        "description": "RPM",
                                                                         "identifier": "RPM",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16402,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                 "STARTER_HANDLE": {
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Starter Handle",
                                                                                "identifier": "STARTER_HANDLE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16394,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 6,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 1,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "limited_rotary"
                                                                   },
                                                "START_PUMP_PULL": {
                                                                           "category": "Motor",
                                                                       "control_type": "limited_dial",
                                                                        "description": "Start Pump (Pull)",
                                                                         "identifier": "START_PUMP_PULL",
                                                                             "inputs": [ {
                                                                                           "description": "set the position of the dial",
                                                                                             "interface": "set_state",
                                                                                             "max_value": 65535
                                                                                       }, {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16398,
                                                                                           "description": "position of the potentiometer",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                "START_PUMP_TURN": {
                                                                           "category": "Motor",
                                                                       "control_type": "limited_dial",
                                                                        "description": "Start Pump (Turn)",
                                                                         "identifier": "START_PUMP_TURN",
                                                                             "inputs": [ {
                                                                                           "description": "set the position of the dial",
                                                                                             "interface": "set_state",
                                                                                             "max_value": 65535
                                                                                       }, {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16396,
                                                                                           "description": "position of the potentiometer",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                   "SUPERCHARGER": {
                                                                                  "category": "Motor",
                                                                              "control_type": "selector",
                                                                               "description": "Supercharge Speed 1/0/2",
                                                                                "identifier": "SUPERCHARGER",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 16394,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 96,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 5,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                       "THROTTLE": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Motor",
                                                                       "control_type": "analog_dial",
                                                                        "description": "Throttle",
                                                                         "identifier": "THROTTLE",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16406,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                            "WEB": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Motor",
                                                                       "control_type": "analog_dial",
                                                                        "description": "War Emergency Power (WEB)",
                                                                         "identifier": "WEB",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16400,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   }
                                            },
                                  "Oxygen": {
                                                  "OXY_ADJ_VALVE": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Oxygen",
                                                                       "control_type": "analog_dial",
                                                                        "description": "Oxygen Adjusting Valve",
                                                                         "identifier": "OXY_ADJ_VALVE",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16418,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                "OXY_EMERG_VALVE": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Oxygen",
                                                                       "control_type": "analog_dial",
                                                                        "description": "Oxygen Emergency Valve",
                                                                         "identifier": "OXY_EMERG_VALVE",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16420,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                  "OXY_OFF_VALVE": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "Oxygen",
                                                                       "control_type": "analog_dial",
                                                                        "description": "Oxygen Shutoff Valve",
                                                                         "identifier": "OXY_OFF_VALVE",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 16422,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   }
                                            },
    "Warning, Caution and IndicatorLights": {
                                                "NEEDLE_GLOW": {
                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                   "control_type": "led",
                                                                    "description": "Panel Needle Glow (yellow)",
                                                                     "identifier": "NEEDLE_GLOW",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 16412,
                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                              "mask": 2048,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 11,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                                 "PANEL_GLOW": {
                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                   "control_type": "led",
                                                                    "description": "Panel Glow (yellow)",
                                                                     "identifier": "PANEL_GLOW",
                                                                         "inputs": [  ],
                                                                        "outputs": [ {
                                                                                           "address": 16412,
                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                              "mask": 1024,
                                                                                         "max_value": 1,
                                                                                          "shift_by": 10,
                                                                                            "suffix": "",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               }
                                            },
                                 "Weapons": {
                                                "GUN_L_RECHARG_NOSE": {
                                                                                  "api_variant": "momentary_last_position",
                                                                                     "category": "Weapons",
                                                                                 "control_type": "selector",
                                                                                  "description": "Gun Nose Right Recharge",
                                                                                   "identifier": "GUN_L_RECHARG_NOSE",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 16394,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 4096,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 12,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "push_button"
                                                                      },
                                                "GUN_L_RECHARG_WING": {
                                                                                  "api_variant": "momentary_last_position",
                                                                                     "category": "Weapons",
                                                                                 "control_type": "selector",
                                                                                  "description": "Gun Wing Left Recharge",
                                                                                   "identifier": "GUN_L_RECHARG_WING",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 16394,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 512,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 9,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "push_button"
                                                                      },
                                                "GUN_R_RECHARG_NOSE": {
                                                                                  "api_variant": "momentary_last_position",
                                                                                     "category": "Weapons",
                                                                                 "control_type": "selector",
                                                                                  "description": "Gun Nose Left Recharge",
                                                                                   "identifier": "GUN_R_RECHARG_NOSE",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 16394,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 2048,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 11,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "push_button"
                                                                      },
                                                "GUN_R_RECHARG_WING": {
                                                                                  "api_variant": "momentary_last_position",
                                                                                     "category": "Weapons",
                                                                                 "control_type": "selector",
                                                                                  "description": "Gun Wing Right Recharge",
                                                                                   "identifier": "GUN_R_RECHARG_WING",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 1
                                                                                                 }, {
                                                                                                        "argument": "TOGGLE",
                                                                                                     "description": "Toggle switch state",
                                                                                                       "interface": "action"
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 16394,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 1024,
                                                                                                       "max_value": 1,
                                                                                                        "shift_by": 10,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "push_button"
                                                                      },
                                                   "ROCK_BOMB_COUNT": {
                                                                                     "category": "Weapons",
                                                                                 "control_type": "selector",
                                                                                  "description": "Rockets/Bombs Counter",
                                                                                   "identifier": "ROCK_BOMB_COUNT",
                                                                                       "inputs": [ {
                                                                                                     "description": "switch to previous or next state",
                                                                                                       "interface": "fixed_step"
                                                                                                 }, {
                                                                                                     "description": "set position",
                                                                                                       "interface": "set_state",
                                                                                                       "max_value": 17
                                                                                                 } ],
                                                                          "momentary_positions": "none",
                                                                                      "outputs": [ {
                                                                                                         "address": 16412,
                                                                                                     "description": "selector position",
                                                                                                            "mask": 31,
                                                                                                       "max_value": 17,
                                                                                                        "shift_by": 0,
                                                                                                          "suffix": "",
                                                                                                            "type": "integer"
                                                                                                 } ],
                                                                             "physical_variant": "toggle_switch"
                                                                      }
                                            }
};
