docdata["MiG-19P"] =
{
                              "ARK5 Panel": {
                                                   "ARK5_ANT_MOV": {
                                                                                  "category": "ARK5 Panel",
                                                                              "control_type": "selector",
                                                                               "description": "ARK-5 Loop Antenna Rotation Switch, L(EFT)/R(IGHT)",
                                                                                "identifier": "ARK5_ANT_MOV",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 96,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 5,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "3_position_switch"
                                                                   },
                                                  "ARK5_CHAN_SEL": {
                                                                                  "category": "ARK5 Panel",
                                                                              "control_type": "selector",
                                                                               "description": "ARK-5 NEAR Frequency Band Selector Switch",
                                                                                "identifier": "ARK5_CHAN_SEL",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5678,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 49152,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 14,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                  "ARK5_FREQ_SEL": {
                                                                                  "category": "ARK5 Panel",
                                                                              "control_type": "selector",
                                                                               "description": "ARK-5 FAR/NDB Frequency Band Selector Switch",
                                                                                "identifier": "ARK5_FREQ_SEL",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 6,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 1,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                 "ARK5_FREQ_TUNE": {
                                                                        "api_variant": "multiturn",
                                                                           "category": "ARK5 Panel",
                                                                       "control_type": "analog_dial",
                                                                        "description": "ARK-5 Frequency Fine Tuning Handle",
                                                                         "identifier": "ARK5_FREQ_TUNE",
                                                                             "inputs": [ {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 5690,
                                                                                           "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "_KNOB_POS",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                "ARK5_INST_LIGHT": {
                                                                           "category": "ARK5 Panel",
                                                                       "control_type": "limited_dial",
                                                                        "description": "ARK-5 Frequency Scale Backlight Knob",
                                                                         "identifier": "ARK5_INST_LIGHT",
                                                                             "inputs": [ {
                                                                                           "description": "set the position of the dial",
                                                                                             "interface": "set_state",
                                                                                             "max_value": 65535
                                                                                       }, {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 5686,
                                                                                           "description": "position of the potentiometer",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                      "ARK5_MODE": {
                                                                                  "category": "ARK5 Panel",
                                                                              "control_type": "selector",
                                                                               "description": "ARK-5 Function Selector Switch, OFF/COMP/ANT./LOOP",
                                                                                "identifier": "ARK5_MODE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 3
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 24,
                                                                                                    "max_value": 3,
                                                                                                     "shift_by": 3,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                 "ARK5_RECV_MODE": {
                                                                                  "category": "ARK5 Panel",
                                                                              "control_type": "selector",
                                                                               "description": "ARK-5 Receiver Mode Switch, TLG(Telegraph)/TLF(Telephony)",
                                                                                "identifier": "ARK5_RECV_MODE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 1,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 0,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                       "ARK5_VOL": {
                                                                           "category": "ARK5 Panel",
                                                                       "control_type": "limited_dial",
                                                                        "description": "ARK-5 Audio Volume Knob",
                                                                         "identifier": "ARK5_VOL",
                                                                             "inputs": [ {
                                                                                           "description": "set the position of the dial",
                                                                                             "interface": "set_state",
                                                                                             "max_value": 65535
                                                                                       }, {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 5688,
                                                                                           "description": "position of the potentiometer",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   }
                                            },
                    "Armament Sight Panel": {
                                                "ASP5_AIM_MODE": {
                                                                                "category": "Armament Sight Panel",
                                                                            "control_type": "selector",
                                                                             "description": "ASP-5 Sight Aiming Mode",
                                                                              "identifier": "ASP5_AIM_MODE",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 3
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5660,
                                                                                                "description": "selector position",
                                                                                                       "mask": 24576,
                                                                                                  "max_value": 3,
                                                                                                   "shift_by": 13,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                 "ASP5_OP_MODE": {
                                                                                "category": "Armament Sight Panel",
                                                                            "control_type": "selector",
                                                                             "description": "ASP-5 Sight Operational Mode (Radar/Optic)",
                                                                              "identifier": "ASP5_OP_MODE",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5660,
                                                                                                "description": "selector position",
                                                                                                       "mask": 32768,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 15,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                "BOMB_REL_MODE": {
                                                                                "category": "Armament Sight Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Bomb Release Mode (Single/Auto)",
                                                                              "identifier": "BOMB_REL_MODE",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5662,
                                                                                                "description": "selector position",
                                                                                                       "mask": 1,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 0,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 }
                                            },
                        "Bulkhead Panel 1": {
                                                   "AGI1_EMERG_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "AGI-1 Emergency Power",
                                                                                    "identifier": "AGI1_EMERG_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 64,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 6,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                          "ANTI_SKID": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Anti-Skid Brake",
                                                                                    "identifier": "ANTI_SKID",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5658,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 1,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 0,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                   "ASP5_SIGHT_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "ASP-5 Sight On/Off",
                                                                                    "identifier": "ASP5_SIGHT_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 4,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 2,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                    "ASP5_WARM_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "ASP-5 Sight Heater",
                                                                                    "identifier": "ASP5_WARM_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 2,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 1,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                      "BATTERY_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Battery Connect/Disconnect",
                                                                                    "identifier": "BATTERY_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16384,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 14,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                "BEACON_ELECTR_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Beacon and Radio Altimeter Electric Power",
                                                                                    "identifier": "BEACON_ELECTR_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 256,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 8,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "CPT_HEATING": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Cockpit Heating",
                                                                                    "identifier": "CPT_HEATING",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32768,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 15,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                     "ELEVATOR_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Elevator Control Electric Power",
                                                                                    "identifier": "ELEVATOR_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 512,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 9,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                  "GUN_CAM_CPT_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Cockpit Gun Camera Power",
                                                                                    "identifier": "GUN_CAM_CPT_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 128,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 7,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                 "GUN_CAM_NOSE_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Nose Gun Camera Power",
                                                                                    "identifier": "GUN_CAM_NOSE_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 256,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 8,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "L_GEN_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Left Generator Connect/Disconnect",
                                                                                    "identifier": "L_GEN_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32768,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 15,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "L_GUN_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Left Gun Electric Power",
                                                                                    "identifier": "L_GUN_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 5,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                       "ORO57K_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "ORO-57K Rocket Pods Electric Power",
                                                                                    "identifier": "ORO57K_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 4,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                  "PITOT_EMERG_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Emergency Pitot Heater Electric Power",
                                                                                    "identifier": "PITOT_EMERG_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8192,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 13,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "PITOT_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Pitot Heater Electric Power",
                                                                                    "identifier": "PITOT_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 4096,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 12,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                 "RADIO_ELECTR_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Radios Electric Power",
                                                                                    "identifier": "RADIO_ELECTR_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 128,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 7,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                  "RADIO_EMERG_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Radios Emergency Power",
                                                                                    "identifier": "RADIO_EMERG_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 5,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                    "RADIO_NAV_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Radio Navigation Electric Power",
                                                                                    "identifier": "RADIO_NAV_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 2048,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 11,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                          "RP5_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "RP-5 Radar Electric Power",
                                                                                    "identifier": "RP5_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 3,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "R_GEN_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Right Generator Connect/Disconnect",
                                                                                    "identifier": "R_GEN_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 1,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 0,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "R_GUN_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Right Gun Electric Power",
                                                                                    "identifier": "R_GUN_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5678,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 64,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 6,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                    "TANK1_FUEL_PUMP": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Tank 1 Fuel Pump",
                                                                                    "identifier": "TANK1_FUEL_PUMP",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 2048,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 11,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                    "TANK2_FUEL_PUMP": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Tank 2 Fuel Pump",
                                                                                    "identifier": "TANK2_FUEL_PUMP",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 4096,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 12,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                    "TANK3_FUEL_PUMP": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Tank 3 Fuel Pump",
                                                                                    "identifier": "TANK3_FUEL_PUMP",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8192,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 13,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                    "TANK4_FUEL_PUMP": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Tank 4 Fuel Pump",
                                                                                    "identifier": "TANK4_FUEL_PUMP",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16384,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 14,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                         "TRIM_PW_SW": {
                                                                                      "category": "Bulkhead Panel 1",
                                                                                  "control_type": "selector",
                                                                                   "description": "Trim System Electric Power",
                                                                                    "identifier": "TRIM_PW_SW",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5674,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 1024,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 10,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       }
                                            },
                        "Bulkhead Panel 2": {
                                                        "ARUFOSH_LAMP_L": {
                                                                                  "category": "Bulkhead Panel 2",
                                                                              "control_type": "limited_dial",
                                                                               "description": "RUFO-45 Left Side ARUFOSH UV Lamp Intensity Control Knob",
                                                                                "identifier": "ARUFOSH_LAMP_L",
                                                                                    "inputs": [ {
                                                                                                  "description": "set the position of the dial",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 65535
                                                                                              }, {
                                                                                                     "description": "turn the dial left or right",
                                                                                                       "interface": "variable_step",
                                                                                                       "max_value": 65535,
                                                                                                  "suggested_step": 3200
                                                                                              } ],
                                                                                   "outputs": [ {
                                                                                                      "address": 5680,
                                                                                                  "description": "position of the potentiometer",
                                                                                                         "mask": 65535,
                                                                                                    "max_value": 65535,
                                                                                                     "shift_by": 0,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ]
                                                                          },
                                                        "ARUFOSH_LAMP_R": {
                                                                                  "category": "Bulkhead Panel 2",
                                                                              "control_type": "limited_dial",
                                                                               "description": "RUFO-45 Right Side ARUFOSH UV Lamp Intensity Control Knob",
                                                                                "identifier": "ARUFOSH_LAMP_R",
                                                                                    "inputs": [ {
                                                                                                  "description": "set the position of the dial",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 65535
                                                                                              }, {
                                                                                                     "description": "turn the dial left or right",
                                                                                                       "interface": "variable_step",
                                                                                                       "max_value": 65535,
                                                                                                  "suggested_step": 3200
                                                                                              } ],
                                                                                   "outputs": [ {
                                                                                                      "address": 5682,
                                                                                                  "description": "position of the potentiometer",
                                                                                                         "mask": 65535,
                                                                                                    "max_value": 65535,
                                                                                                     "shift_by": 0,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ]
                                                                          },
                                                             "ENG_START": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "Engine Start Power Switch",
                                                                                       "identifier": "ENG_START",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5658,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 2,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 1,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                         "FIRE_EX_PW_SW": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "Fire Extinguisher Power Switch",
                                                                                       "identifier": "FIRE_EX_PW_SW",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5658,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 4,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 2,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                          "FLOOD_LAMP_R": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "Right Side Flood Lamp Switch, ON/OFF",
                                                                                       "identifier": "FLOOD_LAMP_R",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5678,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 8192,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 13,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                                "IFF_PW": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "SRO-2 IFF Power Switch, ON/OFF",
                                                                                       "identifier": "IFF_PW",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5678,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 4096,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 12,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                          "IFF_PW_COVER": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "SRO-2 IFF Power Switch Cover",
                                                                                       "identifier": "IFF_PW_COVER",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5678,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 2048,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 11,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                      "IFF_SELFDESTRUCT": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "SRO-2 IFF Self-destruct Button - Press to activate self-destruction",
                                                                                       "identifier": "IFF_SELFDESTRUCT",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5678,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 1024,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 10,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                "IFF_SELFDESTRUCT_COVER": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "SRO-2 IFF Self-destruct Button Cover",
                                                                                       "identifier": "IFF_SELFDESTRUCT_COVER",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5678,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 512,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 9,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                      "L_ENG_BURNER_CUT": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "Left Engine Afterburner Cut",
                                                                                       "identifier": "L_ENG_BURNER_CUT",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5658,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 64,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 6,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                         "L_ENG_OIL_CUT": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "Left Engine Oil Cutoff",
                                                                                       "identifier": "L_ENG_OIL_CUT",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5658,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 16,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 4,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                      "R_ENG_BURNER_CUT": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "Right Engine Afterburner Cut",
                                                                                       "identifier": "R_ENG_BURNER_CUT",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5658,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 32,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 5,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          },
                                                         "R_ENG_OIL_CUT": {
                                                                                         "category": "Bulkhead Panel 2",
                                                                                     "control_type": "selector",
                                                                                      "description": "Right Engine Oil Cutoff",
                                                                                       "identifier": "R_ENG_OIL_CUT",
                                                                                           "inputs": [ {
                                                                                                         "description": "switch to previous or next state",
                                                                                                           "interface": "fixed_step"
                                                                                                     }, {
                                                                                                         "description": "set position",
                                                                                                           "interface": "set_state",
                                                                                                           "max_value": 1
                                                                                                     }, {
                                                                                                            "argument": "TOGGLE",
                                                                                                         "description": "Toggle switch state",
                                                                                                           "interface": "action"
                                                                                                     } ],
                                                                              "momentary_positions": "none",
                                                                                          "outputs": [ {
                                                                                                             "address": 5658,
                                                                                                         "description": "selector position",
                                                                                                                "mask": 8,
                                                                                                           "max_value": 1,
                                                                                                            "shift_by": 3,
                                                                                                              "suffix": "",
                                                                                                                "type": "integer"
                                                                                                     } ],
                                                                                 "physical_variant": "toggle_switch"
                                                                          }
                                            },
                        "Bulkhead Panel 3": {
                                                         "ARU2_MANUAL": {
                                                                                       "category": "Bulkhead Panel 3",
                                                                                   "control_type": "selector",
                                                                                    "description": "ARU-2 Manual Arm Selector",
                                                                                     "identifier": "ARU2_MANUAL",
                                                                                         "inputs": [ {
                                                                                                       "description": "switch to previous or next state",
                                                                                                         "interface": "fixed_step"
                                                                                                   }, {
                                                                                                       "description": "set position",
                                                                                                         "interface": "set_state",
                                                                                                         "max_value": 2
                                                                                                   } ],
                                                                            "momentary_positions": "none",
                                                                                        "outputs": [ {
                                                                                                           "address": 5658,
                                                                                                       "description": "selector position",
                                                                                                              "mask": 768,
                                                                                                         "max_value": 2,
                                                                                                          "shift_by": 8,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ],
                                                                               "physical_variant": "3_position_switch"
                                                                        },
                                                           "ARU2_MODE": {
                                                                                       "category": "Bulkhead Panel 3",
                                                                                   "control_type": "selector",
                                                                                    "description": "ARU-2 Operational Mode (Auto/Manual)",
                                                                                     "identifier": "ARU2_MODE",
                                                                                         "inputs": [ {
                                                                                                       "description": "switch to previous or next state",
                                                                                                         "interface": "fixed_step"
                                                                                                   }, {
                                                                                                       "description": "set position",
                                                                                                         "interface": "set_state",
                                                                                                         "max_value": 1
                                                                                                   }, {
                                                                                                          "argument": "TOGGLE",
                                                                                                       "description": "Toggle switch state",
                                                                                                         "interface": "action"
                                                                                                   } ],
                                                                            "momentary_positions": "none",
                                                                                        "outputs": [ {
                                                                                                           "address": 5658,
                                                                                                       "description": "selector position",
                                                                                                              "mask": 128,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 7,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ],
                                                                               "physical_variant": "toggle_switch"
                                                                        },
                                                "TP19_BRAKECUTE_COVER": {
                                                                                       "category": "Bulkhead Panel 3",
                                                                                   "control_type": "selector",
                                                                                    "description": "TP-19 Braking Parachute Jettison Button Cover",
                                                                                     "identifier": "TP19_BRAKECUTE_COVER",
                                                                                         "inputs": [ {
                                                                                                       "description": "switch to previous or next state",
                                                                                                         "interface": "fixed_step"
                                                                                                   }, {
                                                                                                       "description": "set position",
                                                                                                         "interface": "set_state",
                                                                                                         "max_value": 1
                                                                                                   }, {
                                                                                                          "argument": "TOGGLE",
                                                                                                       "description": "Toggle switch state",
                                                                                                         "interface": "action"
                                                                                                   } ],
                                                                            "momentary_positions": "none",
                                                                                        "outputs": [ {
                                                                                                           "address": 5658,
                                                                                                       "description": "selector position",
                                                                                                              "mask": 1024,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 10,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ],
                                                                               "physical_variant": "toggle_switch"
                                                                        },
                                                 "TP19_BRAKECUTE_JETT": {
                                                                                    "api_variant": "momentary_last_position",
                                                                                       "category": "Bulkhead Panel 3",
                                                                                   "control_type": "selector",
                                                                                    "description": "TP-19 Braking Parachute Jettison Button - Press to jettison drag chute",
                                                                                     "identifier": "TP19_BRAKECUTE_JETT",
                                                                                         "inputs": [ {
                                                                                                       "description": "switch to previous or next state",
                                                                                                         "interface": "fixed_step"
                                                                                                   }, {
                                                                                                       "description": "set position",
                                                                                                         "interface": "set_state",
                                                                                                         "max_value": 1
                                                                                                   }, {
                                                                                                          "argument": "TOGGLE",
                                                                                                       "description": "Toggle switch state",
                                                                                                         "interface": "action"
                                                                                                   } ],
                                                                            "momentary_positions": "none",
                                                                                        "outputs": [ {
                                                                                                           "address": 5658,
                                                                                                       "description": "selector position",
                                                                                                              "mask": 2048,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 11,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ],
                                                                               "physical_variant": "push_button"
                                                                        },
                                                            "WARN_BTN": {
                                                                                    "api_variant": "momentary_last_position",
                                                                                       "category": "Bulkhead Panel 3",
                                                                                   "control_type": "selector",
                                                                                    "description": "Warning Button",
                                                                                     "identifier": "WARN_BTN",
                                                                                         "inputs": [ {
                                                                                                       "description": "switch to previous or next state",
                                                                                                         "interface": "fixed_step"
                                                                                                   }, {
                                                                                                       "description": "set position",
                                                                                                         "interface": "set_state",
                                                                                                         "max_value": 1
                                                                                                   }, {
                                                                                                          "argument": "TOGGLE",
                                                                                                       "description": "Toggle switch state",
                                                                                                         "interface": "action"
                                                                                                   } ],
                                                                            "momentary_positions": "none",
                                                                                        "outputs": [ {
                                                                                                           "address": 5658,
                                                                                                       "description": "selector position",
                                                                                                              "mask": 4096,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 12,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ],
                                                                               "physical_variant": "push_button"
                                                                        }
                                            },
                        "Bulkhead Panel 4": {
                                                  "ENG_FIRE_TEST_BTN": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Engine Fire Lamp Test Button",
                                                                                    "identifier": "ENG_FIRE_TEST_BTN",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5658,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16384,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 14,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                            "FIRE_EX": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Fire Extinguisher",
                                                                                    "identifier": "FIRE_EX",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5660,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 4,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                      "FIRE_EX_COVER": {
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Fire Extinguisher Cover",
                                                                                    "identifier": "FIRE_EX_COVER",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5660,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 3,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                 "FUEL_TANK_WARN_BTN": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Fuel Tanks 2,3,4 Warning Lamps Test Button",
                                                                                    "identifier": "FUEL_TANK_WARN_BTN",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5658,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8192,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 13,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                      "L_ENG_FUELCUT": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Left Engine Fuel Cutoff",
                                                                                    "identifier": "L_ENG_FUELCUT",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5660,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 2,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 1,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                "L_ENG_FUELCUT_COVER": {
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Left Engine Fuel Cutoff Cover",
                                                                                    "identifier": "L_ENG_FUELCUT_COVER",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5658,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32768,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 15,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "L_ENG_START": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Left Engine Start",
                                                                                    "identifier": "L_ENG_START",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5660,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 128,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 7,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                      "R_ENG_FUELCUT": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Right Engine Fuel Cutoff",
                                                                                    "identifier": "R_ENG_FUELCUT",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5660,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 4,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 2,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                "R_ENG_FUELCUT_COVER": {
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Right Engine Fuel Cutoff Cover",
                                                                                    "identifier": "R_ENG_FUELCUT_COVER",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5660,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 1,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 0,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                        "R_ENG_START": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Bulkhead Panel 4",
                                                                                  "control_type": "selector",
                                                                                   "description": "Right Engine Start",
                                                                                    "identifier": "R_ENG_START",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5660,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 256,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 8,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       }
                                            },
                        "Bulkhead Panel 5": {
                                                      "L_ENG_AIR_START": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Bulkhead Panel 5",
                                                                                    "control_type": "selector",
                                                                                     "description": "Left Air Engine Start",
                                                                                      "identifier": "L_ENG_AIR_START",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5660,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2048,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 11,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                "L_ENG_AIR_START_COVER": {
                                                                                        "category": "Bulkhead Panel 5",
                                                                                    "control_type": "selector",
                                                                                     "description": "Left Engine Air Start Button Cover",
                                                                                      "identifier": "L_ENG_AIR_START_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5660,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 512,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 9,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                    "L_ENG_START_COVER": {
                                                                                        "category": "Bulkhead Panel 5",
                                                                                    "control_type": "selector",
                                                                                     "description": "Left Engine Start Button Cover",
                                                                                      "identifier": "L_ENG_START_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5660,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 32,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 5,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                      "R_ENG_AIR_START": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Bulkhead Panel 5",
                                                                                    "control_type": "selector",
                                                                                     "description": "Right Air Engine Start",
                                                                                      "identifier": "R_ENG_AIR_START",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5660,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 4096,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 12,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                "R_ENG_AIR_START_COVER": {
                                                                                        "category": "Bulkhead Panel 5",
                                                                                    "control_type": "selector",
                                                                                     "description": "Right Engine Air Start Button Cover",
                                                                                      "identifier": "R_ENG_AIR_START_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5660,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1024,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 10,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                    "R_ENG_START_COVER": {
                                                                                        "category": "Bulkhead Panel 5",
                                                                                    "control_type": "selector",
                                                                                     "description": "Right Engine Start Button Cover",
                                                                                      "identifier": "R_ENG_START_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5660,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 64,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 6,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         }
                                            },
                                  "Canopy": {
                                                "CANOPY_LOCK_L": {
                                                                                "category": "Canopy",
                                                                            "control_type": "selector",
                                                                             "description": "Canopy Lock Lever L",
                                                                              "identifier": "CANOPY_LOCK_L",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5694,
                                                                                                "description": "selector position",
                                                                                                       "mask": 128,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 7,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                "CANOPY_LOCK_R": {
                                                                                "category": "Canopy",
                                                                            "control_type": "selector",
                                                                             "description": "Canopy Lock Lever R",
                                                                              "identifier": "CANOPY_LOCK_R",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5694,
                                                                                                "description": "selector position",
                                                                                                       "mask": 256,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 8,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                  "CANOPY_OPEN": {
                                                                                "category": "Canopy",
                                                                            "control_type": "selector",
                                                                             "description": "Canopy Open/Close Handle",
                                                                              "identifier": "CANOPY_OPEN",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5694,
                                                                                                "description": "selector position",
                                                                                                       "mask": 2048,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 11,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                 "CANOPY_PRESS": {
                                                                                "category": "Canopy",
                                                                            "control_type": "selector",
                                                                             "description": "Canopy Pressurization Switch",
                                                                              "identifier": "CANOPY_PRESS",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5694,
                                                                                                "description": "selector position",
                                                                                                       "mask": 512,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 9,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                 "EMERG_CANOPY": {
                                                                                "category": "Canopy",
                                                                            "control_type": "selector",
                                                                             "description": "Emergency Canopy Release Lever",
                                                                              "identifier": "EMERG_CANOPY",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5694,
                                                                                                "description": "selector position",
                                                                                                       "mask": 1024,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 10,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 }
                                            },
                          "Center Console": {
                                                "BOMB_ARM_SW": {
                                                                              "category": "Center Console",
                                                                          "control_type": "selector",
                                                                           "description": "Bombs Arm Switch",
                                                                            "identifier": "BOMB_ARM_SW",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 1
                                                                                          }, {
                                                                                                 "argument": "TOGGLE",
                                                                                              "description": "Toggle switch state",
                                                                                                "interface": "action"
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 5636,
                                                                                              "description": "selector position",
                                                                                                     "mask": 1024,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 10,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "toggle_switch"
                                                               },
                                                  "GUN_L_ROF": {
                                                                    "api_variant": "multiturn",
                                                                       "category": "Center Console",
                                                                   "control_type": "analog_dial",
                                                                    "description": "Left Gun Ammo Counter Reset",
                                                                     "identifier": "GUN_L_ROF",
                                                                         "inputs": [ {
                                                                                          "description": "turn the dial left or right",
                                                                                            "interface": "variable_step",
                                                                                            "max_value": 65535,
                                                                                       "suggested_step": 3200
                                                                                   } ],
                                                                        "outputs": [ {
                                                                                           "address": 5654,
                                                                                       "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                              "mask": 65535,
                                                                                         "max_value": 65535,
                                                                                          "shift_by": 0,
                                                                                            "suffix": "_KNOB_POS",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                                  "GUN_R_ROF": {
                                                                    "api_variant": "multiturn",
                                                                       "category": "Center Console",
                                                                   "control_type": "analog_dial",
                                                                    "description": "Right Gun Ammo Counter Reset",
                                                                     "identifier": "GUN_R_ROF",
                                                                         "inputs": [ {
                                                                                          "description": "turn the dial left or right",
                                                                                            "interface": "variable_step",
                                                                                            "max_value": 65535,
                                                                                       "suggested_step": 3200
                                                                                   } ],
                                                                        "outputs": [ {
                                                                                           "address": 5656,
                                                                                       "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                              "mask": 65535,
                                                                                         "max_value": 65535,
                                                                                          "shift_by": 0,
                                                                                            "suffix": "_KNOB_POS",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               }
                                            },
                        "Circuit Breakers": {
                                                 "CB_AILERON_ACT": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "BU-13M Aileron and BU-14M Stabilizer Hydraulic Booster Circuit Breaker",
                                                                                "identifier": "CB_AILERON_ACT",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5694,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 32,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 5,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                        "CB_ARK5": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "ARK-5 Radio Navigation System Circuit Breaker",
                                                                                "identifier": "CB_ARK5",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5694,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 4,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 2,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                       "CB_ARU2V": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "ARU-2V Flight Control System Circuit Breaker",
                                                                                "identifier": "CB_ARU2V",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 16384,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 14,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                   "CB_BOMB_FUSE": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Bomb Fuzing System Circuit Breaker",
                                                                                "identifier": "CB_BOMB_FUSE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 32768,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 15,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                   "CB_BOMB_JETT": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Bomb, Drop Tank and Rocket Emergency Jettison System Circuit Breaker",
                                                                                "identifier": "CB_BOMB_JETT",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5694,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 2,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 1,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                "CB_BOMB_RELEASE": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Bomb Release System Circuit Breaker",
                                                                                "identifier": "CB_BOMB_RELEASE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5694,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 1,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 0,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                        "CB_GFAB": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Landing Gear, Airbrake and Flaps Systems Circuit Breaker",
                                                                                "identifier": "CB_GFAB",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5694,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 16,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 4,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                 "CB_GFAB_LIGHTS": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Landing Gear, Airbrake and Flaps Annunciator Lights Circuit Breaker",
                                                                                "identifier": "CB_GFAB_LIGHTS",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5694,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 8,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 3,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                      "CB_LIGHTS": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Aircraft External Lights Circuit Breaker",
                                                                                "identifier": "CB_LIGHTS",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 8192,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 13,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                        "CB_LOCK": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Circuit Breakers Panel Lock",
                                                                                "identifier": "CB_LOCK",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 4096,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 12,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                 "CB_ROCKET_PODS": {
                                                                                  "category": "Circuit Breakers",
                                                                              "control_type": "selector",
                                                                               "description": "Rocket Pods Circuit Breaker",
                                                                                "identifier": "CB_ROCKET_PODS",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5694,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 64,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 6,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   }
                                            },
                             "Environment": {
                                                "OXY_CONTROL": {
                                                                              "category": "Environment",
                                                                          "control_type": "selector",
                                                                           "description": "Oxygen-Air Diluter Lever, MIXTURE/100% O2",
                                                                            "identifier": "OXY_CONTROL",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 1
                                                                                          }, {
                                                                                                 "argument": "TOGGLE",
                                                                                              "description": "Toggle switch state",
                                                                                                "interface": "action"
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 5668,
                                                                                              "description": "selector position",
                                                                                                     "mask": 8192,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 13,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "toggle_switch"
                                                               },
                                                   "OXY_FLOW": {
                                                                    "api_variant": "multiturn",
                                                                       "category": "Environment",
                                                                   "control_type": "analog_dial",
                                                                    "description": "Oxygen shut-off valve",
                                                                     "identifier": "OXY_FLOW",
                                                                         "inputs": [ {
                                                                                          "description": "turn the dial left or right",
                                                                                            "interface": "variable_step",
                                                                                            "max_value": 65535,
                                                                                       "suggested_step": 3200
                                                                                   } ],
                                                                        "outputs": [ {
                                                                                           "address": 5670,
                                                                                       "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                              "mask": 65535,
                                                                                         "max_value": 65535,
                                                                                          "shift_by": 0,
                                                                                            "suffix": "_KNOB_POS",
                                                                                              "type": "integer"
                                                                                   } ]
                                                               },
                                                   "OXY_MODE": {
                                                                              "category": "Environment",
                                                                          "control_type": "selector",
                                                                           "description": "Suit Oxygen Supply Lever, AUTOMATIC TURN-OFF/N(EUTRAL)/SUIT TURN-ON",
                                                                            "identifier": "OXY_MODE",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 2
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 5668,
                                                                                              "description": "selector position",
                                                                                                     "mask": 6144,
                                                                                                "max_value": 2,
                                                                                                 "shift_by": 11,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "3_position_switch"
                                                               }
                                            },
                   "Exterior Lights Panel": {
                                                 "NAV_LIGHTS": {
                                                                              "category": "Exterior Lights Panel",
                                                                          "control_type": "selector",
                                                                           "description": "Navigation Lights",
                                                                            "identifier": "NAV_LIGHTS",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 5
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 5634,
                                                                                              "description": "selector position",
                                                                                                     "mask": 7168,
                                                                                                "max_value": 5,
                                                                                                 "shift_by": 10,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "toggle_switch"
                                                               },
                                                "NOSE_LIGHTS": {
                                                                              "category": "Exterior Lights Panel",
                                                                          "control_type": "selector",
                                                                           "description": "Nose Lights Switch, LANDING/OFF/TAXI",
                                                                            "identifier": "NOSE_LIGHTS",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 2
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 5634,
                                                                                              "description": "selector position",
                                                                                                     "mask": 24576,
                                                                                                "max_value": 2,
                                                                                                 "shift_by": 13,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "3_position_switch"
                                                               }
                                            },
                 "External Aircraft Model": {
                                                 "EXT_POSITION_LIGHT_LEFT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Left Position Light (red)",
                                                                                  "identifier": "EXT_POSITION_LIGHT_LEFT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 5702,
                                                                                                    "description": "Left Position Light (red)",
                                                                                                           "mask": 32,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 5,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                "EXT_POSITION_LIGHT_RIGHT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Right Position Light (green)",
                                                                                  "identifier": "EXT_POSITION_LIGHT_RIGHT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 5702,
                                                                                                    "description": "Right Position Light (green)",
                                                                                                           "mask": 64,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 6,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                    "EXT_SPEED_BRAKE_LEFT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Left Speed Brake",
                                                                                  "identifier": "EXT_SPEED_BRAKE_LEFT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 5824,
                                                                                                    "description": "Left Speed Brake",
                                                                                                           "mask": 65535,
                                                                                                      "max_value": 65535,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                   "EXT_SPEED_BRAKE_RIGHT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Right Speed Brake",
                                                                                  "identifier": "EXT_SPEED_BRAKE_RIGHT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 5822,
                                                                                                    "description": "Right Speed Brake",
                                                                                                           "mask": 65535,
                                                                                                      "max_value": 65535,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                            "EXT_WOW_LEFT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Weight ON Wheels Left Gear",
                                                                                  "identifier": "EXT_WOW_LEFT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 5702,
                                                                                                    "description": "Weight ON Wheels Left Gear",
                                                                                                           "mask": 512,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 9,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                            "EXT_WOW_NOSE": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Weight ON Wheels Nose Gear",
                                                                                  "identifier": "EXT_WOW_NOSE",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 5702,
                                                                                                    "description": "Weight ON Wheels Nose Gear",
                                                                                                           "mask": 128,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 7,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                           "EXT_WOW_RIGHT": {
                                                                                    "category": "External Aircraft Model",
                                                                                "control_type": "metadata",
                                                                                 "description": "Weight ON Wheels Right Gear",
                                                                                  "identifier": "EXT_WOW_RIGHT",
                                                                                      "inputs": [  ],
                                                                                     "outputs": [ {
                                                                                                        "address": 5702,
                                                                                                    "description": "Weight ON Wheels Right Gear",
                                                                                                           "mask": 256,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 8,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            }
                                            },
                          "Flight Control": {
                                                   "AILERON_HYDRO": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "BU-13M Aileron Hydraulic Booster Switch, ON/OFF",
                                                                                 "identifier": "AILERON_HYDRO",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 32768,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 15,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                    "AILERON_TRIM": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Aileron Trimmer Switch, LEFT/RIGHT",
                                                                                 "identifier": "AILERON_TRIM",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 2
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5668,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 3,
                                                                                                     "max_value": 2,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "3_position_switch"
                                                                    },
                                                   "ARU2V_MAN_SET": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Elevator Control Manual Mode Selector (Long/Short)",
                                                                                 "identifier": "ARU2V_MAN_SET",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 2
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 12288,
                                                                                                     "max_value": 2,
                                                                                                      "shift_by": 12,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "3_position_switch"
                                                                    },
                                                   "ARU2V_OP_MODE": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Elevator Control (ARU-2V) Mode (Automatic/Manual)",
                                                                                 "identifier": "ARU2V_OP_MODE",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 2048,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 11,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                "ELEVATOR_ACT_SEL": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Elevator Actuator Switch, HYDRAULIC(BU-14M BOOSTER)/ELECTRIC(MUS-2 SYSTEM)",
                                                                                 "identifier": "ELEVATOR_ACT_SEL",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 16384,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 14,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                 "FLAPS_BTN_RESET": {
                                                                                "api_variant": "momentary_last_position",
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Flaps buttons reset",
                                                                                 "identifier": "FLAPS_BTN_RESET",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5668,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 32,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 5,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "push_button"
                                                                    },
                                                      "FLAPS_LAND": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Flaps Landing",
                                                                                 "identifier": "FLAPS_LAND",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5668,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 4,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 2,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "limited_rotary"
                                                                    },
                                                       "FLAPS_OFF": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Flaps Off",
                                                                                 "identifier": "FLAPS_OFF",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5668,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 16,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 4,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "limited_rotary"
                                                                    },
                                                   "FLAPS_TAKEOFF": {
                                                                                   "category": "Flight Control",
                                                                               "control_type": "selector",
                                                                                "description": "Flaps Take Off",
                                                                                 "identifier": "FLAPS_TAKEOFF",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5668,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 8,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 3,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "limited_rotary"
                                                                    }
                                            },
                      "Flight Instruments": {
                                                    "PITOT_SEL": {
                                                                                "category": "Flight Instruments",
                                                                            "control_type": "selector",
                                                                             "description": "Pitot Tube Selector, MAIN(PVD-4)/EMERGENCY(TP-156)",
                                                                              "identifier": "PITOT_SEL",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5668,
                                                                                                "description": "selector position",
                                                                                                       "mask": 1024,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 10,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                "RADAR_ALT_SEL": {
                                                                                "category": "Flight Instruments",
                                                                            "control_type": "selector",
                                                                             "description": "RV-5 Radio Altimeter Minimum Altitude Selector",
                                                                              "identifier": "RADAR_ALT_SEL",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 9
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5668,
                                                                                                "description": "selector position",
                                                                                                       "mask": 960,
                                                                                                  "max_value": 9,
                                                                                                   "shift_by": 6,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 }
                                            },
                "Flight Instruments Panel": {
                                                          "AGI1_TRIM": {
                                                                               "category": "Flight Instruments Panel",
                                                                           "control_type": "limited_dial",
                                                                            "description": "AGI-1 Artificial Horizon Pitch Trim Knob",
                                                                             "identifier": "AGI1_TRIM",
                                                                                 "inputs": [ {
                                                                                               "description": "set the position of the dial",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 65535
                                                                                           }, {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 5640,
                                                                                               "description": "position of the potentiometer",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                    "ARU2V_LAMP_TEST": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Flight Instruments Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "ARU-2V Lamp Test Button",
                                                                                    "identifier": "ARU2V_LAMP_TEST",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 1,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 0,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                     "BALT_PRESS_SEL": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Flight Instruments Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Barometric Altimeter Setting (bars)",
                                                                             "identifier": "BALT_PRESS_SEL",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 5642,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                 "CLOCK_L_KNOB_PRESS": {
                                                                                      "category": "Flight Instruments Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "AChS-1 Chronograph Left Knob (PRESS)",
                                                                                    "identifier": "CLOCK_L_KNOB_PRESS",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 2
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 48,
                                                                                                        "max_value": 2,
                                                                                                         "shift_by": 4,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "3_position_switch"
                                                                       },
                                                  "CLOCK_L_KNOB_TURN": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Flight Instruments Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "AChS-1 Chronograph Left Knob (Turn)",
                                                                             "identifier": "CLOCK_L_KNOB_TURN",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 5646,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                 "CLOCK_R_KNOB_PRESS": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Flight Instruments Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "AChS-1 Chronograph Right Knob (Press)",
                                                                                    "identifier": "CLOCK_R_KNOB_PRESS",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 3,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                  "CLOCK_R_KNOB_TURN": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Flight Instruments Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "AChS-1 Chronograph Right Knob (Turn)",
                                                                             "identifier": "CLOCK_R_KNOB_TURN",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 5644,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                         "GIK1_ALIGN": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Flight Instruments Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "GIK-1 Needle Alignment",
                                                                                    "identifier": "GIK1_ALIGN",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5634,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32768,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 15,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                       "GIK1_CRS_SEL": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Flight Instruments Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "GIK-1 Course Selector",
                                                                             "identifier": "GIK1_CRS_SEL",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 5638,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                       "GMETER_RESET": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Flight Instruments Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "AM-10 Accelerometer Min/Max G Reset Button",
                                                                                    "identifier": "GMETER_RESET",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 64,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 6,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                   "INST_L_DAY_NIGHT": {
                                                                                      "category": "Flight Instruments Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Instruments Lamps Day/Night Mode Switch",
                                                                                    "identifier": "INST_L_DAY_NIGHT",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5636,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 4,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 2,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                "RADAR_ANT_ELEVATION": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Flight Instruments Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "RP-5 Radar Electronic Horizon Elevation Adjustment Knob",
                                                                             "identifier": "RADAR_ANT_ELEVATION",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 5664,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       }
                                            },
                                  "Gauges": {
                                                  "AGI1_ART_HORIZON_BANK": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "AGI-1 Artificial Horizon Bank",
                                                                                 "identifier": "AGI1_ART_HORIZON_BANK",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5756,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                 "AGI1_ART_HORIZON_PITCH": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "AGI-1 Artificial Horizon Pitch",
                                                                                 "identifier": "AGI1_ART_HORIZON_PITCH",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5754,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                           "AIRSPEED_IAS": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "KUS-2000 Airspeed IAS",
                                                                                 "identifier": "AIRSPEED_IAS",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5730,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                           "AIRSPEED_TAS": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "KUS-2000 Airspeed TAS",
                                                                                 "identifier": "AIRSPEED_TAS",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5732,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "ARK5P_FREQ_150": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK-5P Frequency Range 150-310",
                                                                                 "identifier": "ARK5P_FREQ_150",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5808,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "ARK5P_FREQ_310": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK-5P Frequency Range 310-640",
                                                                                 "identifier": "ARK5P_FREQ_310",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5810,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "ARK5P_FREQ_640": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK-5P Frequency Range 640-1300",
                                                                                 "identifier": "ARK5P_FREQ_640",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5812,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                     "ARK5P_SIG_STRENGTH": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK-5P Signal Strength Meter",
                                                                                 "identifier": "ARK5P_SIG_STRENGTH",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5806,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                    "ARK5_FREQ_150_SCALE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK5 Frequency 150-310 Scale",
                                                                                 "identifier": "ARK5_FREQ_150_SCALE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5706,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                    "ARK5_FREQ_310_SCALE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK5 Frequency 310-640 Scale",
                                                                                 "identifier": "ARK5_FREQ_310_SCALE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5708,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                    "ARK5_FREQ_640_SCALE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK5 Frequency 640-1300 Scale",
                                                                                 "identifier": "ARK5_FREQ_640_SCALE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5710,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                        "ARK5_FREQ_SCALE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARK5 Frequency Scale",
                                                                                 "identifier": "ARK5_FREQ_SCALE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5704,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                        "ARU2V_STABI_IND": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ARU-2V Stabilizer Positin Indicator",
                                                                                 "identifier": "ARU2V_STABI_IND",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5758,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                       "ASP5N_DIVE_ANGLE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ASP-5N Dive Angle Selection Scale",
                                                                                 "identifier": "ASP5N_DIVE_ANGLE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5816,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "ASP5N_TRG_SPAN": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "ASP-5N Target Span Selection Scale",
                                                                                 "identifier": "ASP5N_TRG_SPAN",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5814,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                           "BARO_ALT_100": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "VD-20 Barometric Altimeter 100m",
                                                                                 "identifier": "BARO_ALT_100",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5720,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                          "BARO_ALT_1000": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "VD-20 Barometric Altimeter 1000m",
                                                                                 "identifier": "BARO_ALT_1000",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5718,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                           "BARO_ALT_SEL": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "VD-20 Barometric Altimeter Selected Pressure",
                                                                                 "identifier": "BARO_ALT_SEL",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5722,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                          "BRAKE_PRESS_L": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Dual Pointer Brake Pressure Indicator Left",
                                                                                 "identifier": "BRAKE_PRESS_L",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5784,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                          "BRAKE_PRESS_R": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Dual Pointer Brake Pressure Indicator Right",
                                                                                 "identifier": "BRAKE_PRESS_R",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5786,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                              "CLOCK_DAY": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Clock Daytime",
                                                                                 "identifier": "CLOCK_DAY",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5752,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "CLOCK_FLIGHT_H": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Clock Flight Time Hours",
                                                                                 "identifier": "CLOCK_FLIGHT_H",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5740,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "CLOCK_FLIGHT_M": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Clock Flight Time Minutes",
                                                                                 "identifier": "CLOCK_FLIGHT_M",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5742,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                "CLOCK_H": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Clock Hours",
                                                                                 "identifier": "CLOCK_H",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5744,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                "CLOCK_M": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Clock Minutes",
                                                                                 "identifier": "CLOCK_M",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5746,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                "CLOCK_S": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Clock Seconds",
                                                                                 "identifier": "CLOCK_S",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5748,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                          "CPT_ALTIMETER": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Cabin Altitude",
                                                                                 "identifier": "CPT_ALTIMETER",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5778,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "CPT_DIFF_PRESS": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Cabin Differential Pressure",
                                                                                 "identifier": "CPT_DIFF_PRESS",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5780,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                            "EGT_GAUGE_L": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Dual Engine EGT Left Gauge",
                                                                                 "identifier": "EGT_GAUGE_L",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5760,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                            "EGT_GAUGE_R": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Dual Engine EGT Right Gauge",
                                                                                 "identifier": "EGT_GAUGE_R",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5762,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                "EMERG_FLAPS_PRESS_GAUGE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "MA-250 Pneumatic Air Pressure Emergency Flaps",
                                                                                 "identifier": "EMERG_FLAPS_PRESS_GAUGE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5802,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                 "EMERG_GEAR_PRESS_GAUGE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "MA-80 Pneumatic Air Pressure Emergency Landing Gear",
                                                                                 "identifier": "EMERG_GEAR_PRESS_GAUGE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5798,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                             "EUP53_TURN": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "EUP-53 Turn Indicator",
                                                                                 "identifier": "EUP53_TURN",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5734,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                          "FUEL_FLOW_IND": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Fuel Flow Meter",
                                                                                 "identifier": "FUEL_FLOW_IND",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5774,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                               "FUEL_IND": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Fuel Gauge",
                                                                                 "identifier": "FUEL_IND",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5772,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                "GIK_CRS": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "GIK-1 Compass Course",
                                                                                 "identifier": "GIK_CRS",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5726,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                "GIK_HDG": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "GIK-1 Compass Heading",
                                                                                 "identifier": "GIK_HDG",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5724,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                "GIK_NDB": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "GIK-1 Compass NDB Station",
                                                                                 "identifier": "GIK_NDB",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5728,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                "G_METER": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "G-Meter",
                                                                                 "identifier": "G_METER",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5790,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                      "G_METER_L_POINTER": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "G-Meter Left Record Pointer",
                                                                                 "identifier": "G_METER_L_POINTER",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5794,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                      "G_METER_R_POINTER": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "G-Meter Right Record Pointer",
                                                                                 "identifier": "G_METER_R_POINTER",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5792,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                        "HYD_BOOST_PRESS": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Booster Hydraulic System Pressure",
                                                                                 "identifier": "HYD_BOOST_PRESS",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5788,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                          "HYD_SYS_GAUGE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "MA-250 Hydraulic System Pressure",
                                                                                 "identifier": "HYD_SYS_GAUGE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5800,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                  "L_RPM": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Left RPM Gauge",
                                                                                 "identifier": "L_RPM",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5766,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                               "MACH_IND": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Machmeter",
                                                                                 "identifier": "MACH_IND",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5770,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                     "OXY_FLOW_INDICATOR": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "IK-18 Oxygen Flow Indicator",
                                                                                 "identifier": "OXY_FLOW_INDICATOR",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5716,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                        "OXY_PRESS_GAUGE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "IK-18 Oxygen Pressure",
                                                                                 "identifier": "OXY_PRESS_GAUGE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5714,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                            "OXY_SYS_ALT": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Oxygen System Altitude",
                                                                                 "identifier": "OXY_SYS_ALT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5782,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "PNEU_SYS_GAUGE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "MA-250 Pneumatic System Air",
                                                                                 "identifier": "PNEU_SYS_GAUGE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5804,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                              "RADAR_ALT": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "UV-57 Radar Altimeter (raw)",
                                                                                 "identifier": "RADAR_ALT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5738,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                                  "R_RPM": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Right RPM Gauge",
                                                                                 "identifier": "R_RPM",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5768,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                         "SLIP_INDICATOR": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Slip Indicator",
                                                                                 "identifier": "SLIP_INDICATOR",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5736,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                            "STOPWATCH_S": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Stopwatch Seconds",
                                                                                 "identifier": "STOPWATCH_S",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5750,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                             "TARGET_DIS": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Target Distance Gauge",
                                                                                 "identifier": "TARGET_DIS",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5796,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                      "USB1_L_AMMO_COUNT": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "USB-1 Left Cannon Ammo Counter",
                                                                                 "identifier": "USB1_L_AMMO_COUNT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5818,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                      "USB1_R_AMMO_COUNT": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "USB-1 Right Cannon Ammo Counter",
                                                                                 "identifier": "USB1_R_AMMO_COUNT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5820,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                             "VARIOMETER": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "VAR-150 Variometer",
                                                                                 "identifier": "VARIOMETER",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5764,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                              "VOLTMETER": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "V-1 Voltmeter",
                                                                                 "identifier": "VOLTMETER",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5776,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                   "VOLT_MANOMETER_GAUGE": {
                                                                                   "category": "Gauges",
                                                                               "control_type": "analog_gauge",
                                                                                "description": "Voltmeter/Manometer Gauge",
                                                                                 "identifier": "VOLT_MANOMETER_GAUGE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 5712,
                                                                                                   "description": "gauge position",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           }
                                            },
                               "Gunsights": {
                                                "ASP5_BOMB_MIL": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Gunsights",
                                                                     "control_type": "analog_dial",
                                                                      "description": "ASP-5 Mil Depression Setting",
                                                                       "identifier": "ASP5_BOMB_MIL",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 5650,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                  "ASP5_BRIGHT": {
                                                                         "category": "Gunsights",
                                                                     "control_type": "limited_dial",
                                                                      "description": "ASP-5 Brightness",
                                                                       "identifier": "ASP5_BRIGHT",
                                                                           "inputs": [ {
                                                                                         "description": "set the position of the dial",
                                                                                           "interface": "set_state",
                                                                                           "max_value": 65535
                                                                                     }, {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 5652,
                                                                                         "description": "position of the potentiometer",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                    "ASP5_CAGE": {
                                                                                "category": "Gunsights",
                                                                            "control_type": "selector",
                                                                             "description": "ASP-5 Sight Cage/Uncage",
                                                                              "identifier": "ASP5_CAGE",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5636,
                                                                                                "description": "selector position",
                                                                                                       "mask": 128,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 7,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 },
                                                "ASP5_WINGSPAN": {
                                                                      "api_variant": "multiturn",
                                                                         "category": "Gunsights",
                                                                     "control_type": "analog_dial",
                                                                      "description": "ASP-5 Target Wingspan Selector",
                                                                       "identifier": "ASP5_WINGSPAN",
                                                                           "inputs": [ {
                                                                                            "description": "turn the dial left or right",
                                                                                              "interface": "variable_step",
                                                                                              "max_value": 65535,
                                                                                         "suggested_step": 3200
                                                                                     } ],
                                                                          "outputs": [ {
                                                                                             "address": 5648,
                                                                                         "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                "mask": 65535,
                                                                                           "max_value": 65535,
                                                                                            "shift_by": 0,
                                                                                              "suffix": "_KNOB_POS",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 }
                                            },
                          "Jettison Panel": {
                                                           "BEACON_SEL": {
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Near/Far Beacon",
                                                                                      "identifier": "BEACON_SEL",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 16,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 4,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "limited_rotary"
                                                                         },
                                                       "BRAKE_PARA_BTN": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "TP-19 Braking Parachute Deploy Button - Press to deploy drag chute",
                                                                                      "identifier": "BRAKE_PARA_BTN",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 64,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 6,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                 "BRAKE_PARA_BTN_COVER": {
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "TP-19 Braking Parachute Deploy Button Cover",
                                                                                      "identifier": "BRAKE_PARA_BTN_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 32,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 5,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                      "FUEL_BOMBS_JETT": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fuel Tanks/Bombs Jettison",
                                                                                      "identifier": "FUEL_BOMBS_JETT",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 256,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 8,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                "FUEL_BOMBS_JETT_COVER": {
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fuel Tanks/Bombs Jettison Button Cover",
                                                                                      "identifier": "FUEL_BOMBS_JETT_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 128,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 7,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                            "L_GUN_ARM": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Left Gun Arm",
                                                                                      "identifier": "L_GUN_ARM",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 512,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 9,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                          "ROCKET_JETT": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Rocket pods Jettison",
                                                                                      "identifier": "ROCKET_JETT",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 4096,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 12,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                    "ROCKET_JETT_COVER": {
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Rocket pods Jettison Button Cover",
                                                                                      "identifier": "ROCKET_JETT_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2048,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 11,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                            "R_GUN_ARM": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Jettison Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Right Gun Arm",
                                                                                      "identifier": "R_GUN_ARM",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 5672,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1024,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 10,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         }
                                            },
                      "Landing Gear Panel": {
                                                      "AGI1_CAGE": {
                                                                                  "category": "Landing Gear Panel",
                                                                              "control_type": "selector",
                                                                               "description": "AGI-1 Artificial Horizon Cage Button - Push to cage",
                                                                                "identifier": "AGI1_CAGE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5636,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 2,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 1,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                    "EMERG_BRAKE": {
                                                                                  "category": "Landing Gear Panel",
                                                                              "control_type": "selector",
                                                                               "description": "Emergency Brake",
                                                                                "identifier": "EMERG_BRAKE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5634,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 256,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 8,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                     "GEAR_LEVER": {
                                                                                  "category": "Landing Gear Panel",
                                                                              "control_type": "selector",
                                                                               "description": "Landing Gear Lever, Down/Neutral/Up",
                                                                                "identifier": "GEAR_LEVER",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5634,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 48,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 4,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "3_position_switch"
                                                                   },
                                                "GEAR_LIGHT_TEST": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Landing Gear Panel",
                                                                              "control_type": "selector",
                                                                               "description": "PPS-2 Landing Gear Lights Test Button - Push to test",
                                                                                "identifier": "GEAR_LIGHT_TEST",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5634,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 128,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 7,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   },
                                                      "GEAR_LOCK": {
                                                                                  "category": "Landing Gear Panel",
                                                                              "control_type": "selector",
                                                                               "description": "Landing Gear Lever Lock",
                                                                                "identifier": "GEAR_LOCK",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5634,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 64,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 6,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                "NOSE_GEAR_BRAKE": {
                                                                                  "category": "Landing Gear Panel",
                                                                              "control_type": "selector",
                                                                               "description": "Nose Gear Brake System On/Off",
                                                                                "identifier": "NOSE_GEAR_BRAKE",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5634,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 512,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 9,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   }
                                            },
                                   "Radar": {
                                                "RP5_TELEMETRY": {
                                                                                "category": "Radar",
                                                                            "control_type": "selector",
                                                                             "description": "RP-5 Radar/Telemetry Selector",
                                                                              "identifier": "RP5_TELEMETRY",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 1
                                                                                            }, {
                                                                                                   "argument": "TOGGLE",
                                                                                                "description": "Toggle switch state",
                                                                                                  "interface": "action"
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 5636,
                                                                                                "description": "selector position",
                                                                                                       "mask": 256,
                                                                                                  "max_value": 1,
                                                                                                   "shift_by": 8,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "toggle_switch"
                                                                 }
                                            },
                     "Radar Control Panel": {
                                                  "RADAR_BIT_TEST": {
                                                                                "api_variant": "momentary_last_position",
                                                                                   "category": "Radar Control Panel",
                                                                               "control_type": "selector",
                                                                                "description": "RP-5 Radar Built-In Test (BIT) Button - Press 2 seconds to start test",
                                                                                 "identifier": "RADAR_BIT_TEST",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 32,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 5,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "push_button"
                                                                    },
                                                      "RADAR_ECCM": {
                                                                                   "category": "Radar Control Panel",
                                                                               "control_type": "selector",
                                                                                "description": "RP-5 Radar ECCM Mode Switch, ON/OFF",
                                                                                 "identifier": "RADAR_ECCM",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 16,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 4,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                "RADAR_GAUGE_MODE": {
                                                                                   "category": "Radar Control Panel",
                                                                               "control_type": "selector",
                                                                                "description": "RP-5 Radar Gauge Display Mode Switch, VOLTAGE/AIR PRESSURE",
                                                                                 "identifier": "RADAR_GAUGE_MODE",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 64,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 6,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                      "RADAR_MODE": {
                                                                                   "category": "Radar Control Panel",
                                                                               "control_type": "selector",
                                                                                "description": "RP-5 Radar Mode Control Switch, ON/STANDBY/OFF",
                                                                                 "identifier": "RADAR_MODE",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 3
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 384,
                                                                                                     "max_value": 3,
                                                                                                      "shift_by": 7,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                "RADAR_SCR_BRIGHT": {
                                                                            "category": "Radar Control Panel",
                                                                        "control_type": "limited_dial",
                                                                         "description": "RP-5 Radar Screen Brightness Adjustment Knob",
                                                                          "identifier": "RADAR_SCR_BRIGHT",
                                                                              "inputs": [ {
                                                                                            "description": "set the position of the dial",
                                                                                              "interface": "set_state",
                                                                                              "max_value": 65535
                                                                                        }, {
                                                                                               "description": "turn the dial left or right",
                                                                                                 "interface": "variable_step",
                                                                                                 "max_value": 65535,
                                                                                            "suggested_step": 3200
                                                                                        } ],
                                                                             "outputs": [ {
                                                                                                "address": 5666,
                                                                                            "description": "position of the potentiometer",
                                                                                                   "mask": 65535,
                                                                                              "max_value": 65535,
                                                                                               "shift_by": 0,
                                                                                                 "suffix": "",
                                                                                                   "type": "integer"
                                                                                        } ]
                                                                    },
                                                  "RADAR_SCR_MODE": {
                                                                                   "category": "Radar Control Panel",
                                                                               "control_type": "selector",
                                                                                "description": "RP-5 Radar Screen Mode Switch, DAY/NIGHT",
                                                                                 "identifier": "RADAR_SCR_MODE",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 512,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 9,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                  "RADAR_TGT_LOCK": {
                                                                                   "category": "Radar Control Panel",
                                                                               "control_type": "selector",
                                                                                "description": "RP-5 Radar Target Lock Switch (AR-18-16 Tracking Antenna), ON/OFF",
                                                                                 "identifier": "RADAR_TGT_LOCK",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 5662,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 1024,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 10,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    }
                                            },
                            "Radio RSIU4V": {
                                                  "RADIO_ON_OFF": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Interference Suppression Switch, ON/OFF",
                                                                               "identifier": "RADIO_ON_OFF",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5674,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 16,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 4,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                "RADIO_OPT_MODE": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Audio Output: ADF/Radio",
                                                                               "identifier": "RADIO_OPT_MODE",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5674,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 8,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 3,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                    "RADIO_PRE1": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Preset Radio Channel 1",
                                                                               "identifier": "RADIO_PRE1",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5672,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 8192,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 13,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "limited_rotary"
                                                                  },
                                                    "RADIO_PRE2": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Preset Radio Channel 2",
                                                                               "identifier": "RADIO_PRE2",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5672,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 16384,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 14,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "limited_rotary"
                                                                  },
                                                    "RADIO_PRE3": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Preset Radio Channel 3",
                                                                               "identifier": "RADIO_PRE3",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5672,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 32768,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 15,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "limited_rotary"
                                                                  },
                                                    "RADIO_PRE4": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Preset Radio Channel 4",
                                                                               "identifier": "RADIO_PRE4",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5674,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 1,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "limited_rotary"
                                                                  },
                                                    "RADIO_PRE5": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Preset Radio Channel 5",
                                                                               "identifier": "RADIO_PRE5",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5674,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 2,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 1,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "limited_rotary"
                                                                  },
                                                    "RADIO_PRE6": {
                                                                                 "category": "Radio RSIU4V",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Preset Radio Channel 6",
                                                                               "identifier": "RADIO_PRE6",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5674,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 4,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 2,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "limited_rotary"
                                                                  },
                                                     "RADIO_VOL": {
                                                                          "category": "Radio RSIU4V",
                                                                      "control_type": "limited_dial",
                                                                       "description": "RSIU-4V Volume Control Knob",
                                                                        "identifier": "RADIO_VOL",
                                                                            "inputs": [ {
                                                                                          "description": "set the position of the dial",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 65535
                                                                                      }, {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 5676,
                                                                                          "description": "position of the potentiometer",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  }
                                            },
                           "Right Console": {
                                                "CPT_PRESS_LEVER": {
                                                                           "category": "Right Console",
                                                                       "control_type": "limited_dial",
                                                                        "description": "Cockpit Pressurization Lever",
                                                                         "identifier": "CPT_PRESS_LEVER",
                                                                             "inputs": [ {
                                                                                           "description": "set the position of the dial",
                                                                                             "interface": "set_state",
                                                                                             "max_value": 65535
                                                                                       }, {
                                                                                              "description": "turn the dial left or right",
                                                                                                "interface": "variable_step",
                                                                                                "max_value": 65535,
                                                                                           "suggested_step": 3200
                                                                                       } ],
                                                                            "outputs": [ {
                                                                                               "address": 5692,
                                                                                           "description": "position of the potentiometer",
                                                                                                  "mask": 65535,
                                                                                             "max_value": 65535,
                                                                                              "shift_by": 0,
                                                                                                "suffix": "",
                                                                                                  "type": "integer"
                                                                                       } ]
                                                                   },
                                                       "CPT_TEMP": {
                                                                                  "category": "Right Console",
                                                                              "control_type": "selector",
                                                                               "description": "Cockpit Temperature Select",
                                                                                "identifier": "CPT_TEMP",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 2
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 1536,
                                                                                                    "max_value": 2,
                                                                                                     "shift_by": 9,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "3_position_switch"
                                                                   },
                                                    "CPT_VENT_SW": {
                                                                                  "category": "Right Console",
                                                                              "control_type": "selector",
                                                                               "description": "Cockpit Ventilation Switch, OPEN/CLOSE",
                                                                                "identifier": "CPT_VENT_SW",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 2048,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 11,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                    "EMERG_FLAPS": {
                                                                                  "category": "Right Console",
                                                                              "control_type": "selector",
                                                                               "description": "Flaps Emergency Deployment",
                                                                                "identifier": "EMERG_FLAPS",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 256,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 8,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                     "EMERG_GEAR": {
                                                                                  "category": "Right Console",
                                                                              "control_type": "selector",
                                                                               "description": "Landing Gear Emergency Deployment",
                                                                                "identifier": "EMERG_GEAR",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 5684,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 128,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 7,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   }
                                            },
                        "Rocket Pod Panel": {
                                                "ROCKET_COUNTER_MODE": {
                                                                                      "category": "Rocket Pod Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rockets Counter Mode (day/night)",
                                                                                    "identifier": "ROCKET_COUNTER_MODE",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5662,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 3,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                  "ROCKET_SLAVO_MODE": {
                                                                                      "category": "Rocket Pod Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rockets Salvo Mode Selector",
                                                                                    "identifier": "ROCKET_SLAVO_MODE",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 2
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 5662,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 6,
                                                                                                        "max_value": 2,
                                                                                                         "shift_by": 1,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "3_position_switch"
                                                                       }
                                            },
                                 "Sensors": {
                                                "SPO2_PW_SW": {
                                                                             "category": "Sensors",
                                                                         "control_type": "selector",
                                                                          "description": "SPO-2 SIRENA RWR Power Switch",
                                                                           "identifier": "SPO2_PW_SW",
                                                                               "inputs": [ {
                                                                                             "description": "switch to previous or next state",
                                                                                               "interface": "fixed_step"
                                                                                         }, {
                                                                                             "description": "set position",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 1
                                                                                         }, {
                                                                                                "argument": "TOGGLE",
                                                                                             "description": "Toggle switch state",
                                                                                               "interface": "action"
                                                                                         } ],
                                                                  "momentary_positions": "none",
                                                                              "outputs": [ {
                                                                                                 "address": 5636,
                                                                                             "description": "selector position",
                                                                                                    "mask": 512,
                                                                                               "max_value": 1,
                                                                                                "shift_by": 9,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ],
                                                                     "physical_variant": "toggle_switch"
                                                              }
                                            },
                     "Signal Flares Panel": {
                                                  "FLARE_DISP": {
                                                                               "category": "Signal Flares Panel",
                                                                           "control_type": "selector",
                                                                            "description": "EKSR-46 Signal Flare Dispenser Switch, OFF/ARMED",
                                                                             "identifier": "FLARE_DISP",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 5668,
                                                                                               "description": "selector position",
                                                                                                      "mask": 32768,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 15,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                 "FLARE_GREEN": {
                                                                            "api_variant": "momentary_last_position",
                                                                               "category": "Signal Flares Panel",
                                                                           "control_type": "selector",
                                                                            "description": "EKSR-46 Green Signal Flare Release Button",
                                                                             "identifier": "FLARE_GREEN",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 5672,
                                                                                               "description": "selector position",
                                                                                                      "mask": 2,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 1,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "push_button"
                                                                },
                                                   "FLARE_RED": {
                                                                            "api_variant": "momentary_last_position",
                                                                               "category": "Signal Flares Panel",
                                                                           "control_type": "selector",
                                                                            "description": "EKSR-46 Red Signal Flare Release Button",
                                                                             "identifier": "FLARE_RED",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 5672,
                                                                                               "description": "selector position",
                                                                                                      "mask": 4,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 2,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "push_button"
                                                                },
                                                 "FLARE_WHITE": {
                                                                            "api_variant": "momentary_last_position",
                                                                               "category": "Signal Flares Panel",
                                                                           "control_type": "selector",
                                                                            "description": "EKSR-46 White Signal Flare Release Button",
                                                                             "identifier": "FLARE_WHITE",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 5672,
                                                                                               "description": "selector position",
                                                                                                      "mask": 8,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 3,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "push_button"
                                                                },
                                                "FLARE_YELLOW": {
                                                                            "api_variant": "momentary_last_position",
                                                                               "category": "Signal Flares Panel",
                                                                           "control_type": "selector",
                                                                            "description": "EKSR-46 Yellow Signal Flare Release Button",
                                                                             "identifier": "FLARE_YELLOW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 5672,
                                                                                               "description": "selector position",
                                                                                                      "mask": 1,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "push_button"
                                                                }
                                            },
                                "Throttle": {
                                                 "AFTERBURN_DIS": {
                                                                              "api_variant": "momentary_last_position",
                                                                                 "category": "Throttle",
                                                                             "control_type": "selector",
                                                                              "description": "Mil-power Limit/Afterburner Disable",
                                                                               "identifier": "AFTERBURN_DIS",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5634,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 4,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 2,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "push_button"
                                                                  },
                                                  "AFTERBURN_EN": {
                                                                              "api_variant": "momentary_last_position",
                                                                                 "category": "Throttle",
                                                                             "control_type": "selector",
                                                                              "description": "Afterburner Enable",
                                                                               "identifier": "AFTERBURN_EN",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5634,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 8,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 3,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "push_button"
                                                                  },
                                                   "AIRBRAKE_SW": {
                                                                                 "category": "Throttle",
                                                                             "control_type": "selector",
                                                                              "description": "Airbrake Switch",
                                                                               "identifier": "AIRBRAKE_SW",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5634,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 2,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 1,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                "ASP_TAAGET_DIS": {
                                                                       "api_variant": "multiturn",
                                                                          "category": "Throttle",
                                                                      "control_type": "analog_dial",
                                                                       "description": "ASP-5 Target Distance Selector",
                                                                        "identifier": "ASP_TAAGET_DIS",
                                                                            "inputs": [ {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 5632,
                                                                                          "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "_KNOB_POS",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  },
                                                    "RSIU_TRANS": {
                                                                              "api_variant": "momentary_last_position",
                                                                                 "category": "Throttle",
                                                                             "control_type": "selector",
                                                                              "description": "RSIU-4V Transmit Button - Push to Transmit",
                                                                               "identifier": "RSIU_TRANS",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 5634,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 1,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "push_button"
                                                                  }
                                            },
                                 "Unknown": {
                                                "ANTI_FREZZE": {
                                                                              "category": "Unknown",
                                                                          "control_type": "selector",
                                                                           "description": "Canopy Front Anti Freeze",
                                                                            "identifier": "ANTI_FREZZE",
                                                                                "inputs": [ {
                                                                                              "description": "switch to previous or next state",
                                                                                                "interface": "fixed_step"
                                                                                          }, {
                                                                                              "description": "set position",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 1
                                                                                          }, {
                                                                                                 "argument": "TOGGLE",
                                                                                              "description": "Toggle switch state",
                                                                                                "interface": "action"
                                                                                          } ],
                                                                   "momentary_positions": "none",
                                                                               "outputs": [ {
                                                                                                  "address": 5668,
                                                                                              "description": "selector position",
                                                                                                     "mask": 16384,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 14,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ],
                                                                      "physical_variant": "toggle_switch"
                                                               }
                                            },
    "Warning, Caution and IndicatorLights": {
                                                  "AILERON_TRIM_NEUTRAL_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Aileron Trim Neutral Lamp (green)",
                                                                                     "identifier": "AILERON_TRIM_NEUTRAL_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 1,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 0,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "AIRBRAKE_DOWN": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Airbrake Deployed Lamp (green)",
                                                                                     "identifier": "AIRBRAKE_DOWN",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 3,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ARK5P_PW_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "ARK-5P On/Off Lamp (green)",
                                                                                     "identifier": "ARK5P_PW_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 1,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 0,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                          "ARK5_FREQ_SCALE_L": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "ARK5 Frequency Scale Light (yellow)",
                                                                                     "identifier": "ARK5_FREQ_SCALE_L",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5702,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 4,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                "ARU2V_TAKEOFF_LAND_POS_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "ARU-2V Take-off/Landing Position Lamp (green)",
                                                                                     "identifier": "ARU2V_TAKEOFF_LAND_POS_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 128,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 7,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                           "BEACON_MARK_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Beacon Marker Lamp (green)",
                                                                                     "identifier": "BEACON_MARK_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 64,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 6,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                         "BOMB_FUSE_ARM_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Bomb Fuse Armed Lamp (red)",
                                                                                     "identifier": "BOMB_FUSE_ARM_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 64,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 6,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                            "DROP_TANK_EMPTY": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "External Drop Tank Empty Lamp (green)",
                                                                                     "identifier": "DROP_TANK_EMPTY",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 512,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 9,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "ENGINE_FIRE": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Engine Fire Lamp (red)",
                                                                                     "identifier": "ENGINE_FIRE",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5694,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 32768,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 15,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                 "FLAPS_DOWN": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Flaps Deployed Lamp (green)",
                                                                                     "identifier": "FLAPS_DOWN",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 2,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "FUEL_550_REST": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Fuel Tank 1 550 Liters Lamp (red)",
                                                                                     "identifier": "FUEL_550_REST",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 2,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                          "FUEL_TANK_1_EMPTY": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Fuel Tank 1 Empty Lamp (red)",
                                                                                     "identifier": "FUEL_TANK_1_EMPTY",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 2,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 1,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                          "FUEL_TANK_2_EMPTY": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Fuel Tank 2 Empty Lamp (green)",
                                                                                     "identifier": "FUEL_TANK_2_EMPTY",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5694,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16384,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 14,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                        "FUEL_TANK_3_4_EMPTY": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Fuel Tanks 3 and 4 Empty Lamp (green)",
                                                                                     "identifier": "FUEL_TANK_3_4_EMPTY",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5694,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8192,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 13,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                            "GEAR_MOVE_LIGHT": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Gear in Transit Lamp (red)",
                                                                                     "identifier": "GEAR_MOVE_LIGHT",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 2,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 1,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                        "GUNSIGHT_BREAK_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Gunsight BREAK Lamp (red)",
                                                                                     "identifier": "GUNSIGHT_BREAK_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8192,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 13,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                         "GUNSIGHT_LOCK_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Gunsight LOCK Lamp (green)",
                                                                                     "identifier": "GUNSIGHT_LOCK_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4096,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 12,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                         "HYD_LOW_PRESS_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Main Hydraulic System Low Pressure Lamp (red)",
                                                                                     "identifier": "HYD_LOW_PRESS_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 3,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                      "IFF_SELFDESTRUCT_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "SRO-2 Self-destruction Lamp (red)",
                                                                                     "identifier": "IFF_SELFDESTRUCT_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5694,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4096,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 12,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                               "L_CANNON_ARM": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Cannon Armed Lamp (red)",
                                                                                     "identifier": "L_CANNON_ARM",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 128,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 7,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                             "L_CONSOLE_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Console Lamp (White)",
                                                                                     "identifier": "L_CONSOLE_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 2048,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 11,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "L_ENGINE_AB": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Afterburner Lamp (green)",
                                                                                     "identifier": "L_ENGINE_AB",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8192,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 13,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                               "L_ENGINE_MIL": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Engine Mil Power Lamp (green)",
                                                                                     "identifier": "L_ENGINE_MIL",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 512,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 9,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                             "L_ENG_AIRSTART": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Engine Airstart Lamp (red)",
                                                                                     "identifier": "L_ENG_AIRSTART",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 4,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "L_ENG_OIL_LOW": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Engine Low Oil pressure Lamp (red)",
                                                                                     "identifier": "L_ENG_OIL_LOW",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 32768,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 15,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "L_GEAR_DOWN": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Gear DOWN Lamp (green)",
                                                                                     "identifier": "L_GEAR_DOWN",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 32768,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 15,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                  "L_GEAR_UP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Gear UP Lamp (red)",
                                                                                     "identifier": "L_GEAR_UP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4096,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 12,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                 "L_GEN_FAIL": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left Generator Failture Lamp (red)",
                                                                                     "identifier": "L_GEN_FAIL",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 2048,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 11,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "L_WING_LOAD": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Left External Wing Load Lamp (green)",
                                                                                     "identifier": "L_WING_LOAD",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 1024,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 10,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "N_GEAR_DOWN": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Nose Gear DOWN Lamp (green)",
                                                                                     "identifier": "N_GEAR_DOWN",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5702,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 1,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 0,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                  "N_GEAR_UP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Nose Gear UP Lamp (red)",
                                                                                     "identifier": "N_GEAR_UP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8192,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 13,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                    "PITCH_TRIM_NEUTRAL_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Pitch Trim Neutral Lamp (green)",
                                                                                     "identifier": "PITCH_TRIM_NEUTRAL_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 32,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 5,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                           "RADAR_BREAK_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Radar BREAK Lamp (red)",
                                                                                     "identifier": "RADAR_BREAK_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 32768,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 15,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                            "RADAR_EMIT_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Radar Emitting Lamp (green)",
                                                                                     "identifier": "RADAR_EMIT_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 4,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                            "RADAR_LOCK_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Radar LOCK Lamp (green)",
                                                                                     "identifier": "RADAR_LOCK_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16384,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 14,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                        "RADAR_OVERHEAT_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Radar Overheat Lamp (TURN OFF RADAR) (red)",
                                                                                     "identifier": "RADAR_OVERHEAT_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 256,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 8,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_1_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "1 Rocket Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_1_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 2,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_2_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "2 Rockets Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_2_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 3,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_3_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "3 Rockets Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_3_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 4,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_4_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "4 Rockets Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_4_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 32,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 5,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_5_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "5 Rockets Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_5_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 64,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 6,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_6_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "6 Rockets Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_6_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 128,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 7,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_7_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "7 Rockets Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_7_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 256,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 8,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "ROCKET_8_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "8 Rockets Installed Lamp (yellow)",
                                                                                     "identifier": "ROCKET_8_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 512,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 9,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                           "ROCKET_INST_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Rockets Installed Lamp (green)",
                                                                                     "identifier": "ROCKET_INST_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 2,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 1,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                               "R_CANNON_ARM": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Cannon Armed Lamp (red)",
                                                                                     "identifier": "R_CANNON_ARM",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 256,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 8,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                             "R_CONSOLE_LAMP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Console Lamp (White)",
                                                                                     "identifier": "R_CONSOLE_LAMP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 1024,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 10,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "R_ENGINE_AB": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Afterburner Lamp (green)",
                                                                                     "identifier": "R_ENGINE_AB",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16384,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 14,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                               "R_ENGINE_MIL": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Engine Mil Power Lamp (green)",
                                                                                     "identifier": "R_ENGINE_MIL",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 1024,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 10,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                             "R_ENG_AIRSTART": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Engine Airstart Lamp (red)",
                                                                                     "identifier": "R_ENG_AIRSTART",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 32,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 5,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                              "R_ENG_OIL_LOW": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Engine Low Oil pressure Lamp (red)",
                                                                                     "identifier": "R_ENG_OIL_LOW",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 1,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 0,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "R_GEAR_DOWN": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Gear DOWN Lamp (green)",
                                                                                     "identifier": "R_GEAR_DOWN",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5702,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 2,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 1,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                  "R_GEAR_UP": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Gear UP Lamp (red)",
                                                                                     "identifier": "R_GEAR_UP",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5700,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 16384,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 14,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                 "R_GEN_FAIL": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right Generator Failture Lamp (red)",
                                                                                     "identifier": "R_GEN_FAIL",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5696,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4096,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 12,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                                "R_WING_LOAD": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Right External Wing Load Power Lamp (green)",
                                                                                     "identifier": "R_WING_LOAD",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5698,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 2048,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 11,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                             "SRO2B_RWR_LOCK": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Radar Warning Receiver LOCK Lamp (red)",
                                                                                     "identifier": "SRO2B_RWR_LOCK",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5702,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 8,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 3,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               },
                                                               "SRO2B_RWR_PW": {
                                                                                       "category": "Warning, Caution and IndicatorLights",
                                                                                   "control_type": "led",
                                                                                    "description": "Radar Warning Receiver Power Lamp (red)",
                                                                                     "identifier": "SRO2B_RWR_PW",
                                                                                         "inputs": [  ],
                                                                                        "outputs": [ {
                                                                                                           "address": 5702,
                                                                                                       "description": "0 if light is off, 1 if light is on",
                                                                                                              "mask": 4,
                                                                                                         "max_value": 1,
                                                                                                          "shift_by": 2,
                                                                                                            "suffix": "",
                                                                                                              "type": "integer"
                                                                                                   } ]
                                                                               }
                                            }
};
