Original Author:
    - Weston Schmidt <weston_schmidt@alumni.purdue.edu>

Contributors:
    - Reinhard Arlt
        - at89c5131 chip support
    - Anton Blad
        - at90usb162 and at90usb82 chip support
    - David Brownell
        - compiler flag improvements
        - command line argument processing improvements
        - debugging system improvements
        - significant man page improvements
        - support for the at90usb series AVR chips
        - the beginnings of the move over to using stdint.h
    - Nick Hibma
        - bug fixes
    - Markus Schneider
        - OS X porting issues
    - Geoffrey Wossum
        - added reset command
    - Sean D'Epagnier
        - eeprom bug fix
        - 4K bootloader support fix
    - Peter Gammie
        - at90usb647 PID fix
    - Zachary Clifford
        - completed AVR32 support
        - identified a number of off-by-one errors waiting to happen
        - identified that AVR32 "User Pages" aren't supported yet
        - patch to allow proper handling of the trampoline code
        - patch to allow flashing user flash space & STDIN
        - patch to enable support for windows using mingw32
        - patch to enable setting/getting fuses for the AVR32 devices
    - Donald Davis
        - patch with new AVR devices & testing of support for the devices
    - Brad Schick
        - identified that the flash memory overlaps the bootloader memory
        - identified the off-by-one issue when the bootloader is in upper memory
    - Xavier Leprevost
        - patch to fix an error in the avr32 user flash dump command
    - Dave Fletcher
        - patch to enable atmega32u2 chips
    - Torsten Rottmann
        - patch to enable libusb 1.0 support
    - Mitko
        - patch to enable at32uc3b1512 and at32uc3b0512 chips
    - Darren Gibbs
        - identified dead/bad code around the bootloader overlap checking
