docdata["Yak-52"] =
{
                                 "ARK 15M": {
                                                     "FRONT_CB_ADF": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore ADF Marker",
                                                                                  "identifier": "FRONT_CB_ADF",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8236,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 32,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 5,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "toggle_switch"
                                                                     },
                                                "FRONT_RDF_CHANNEL": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore RDF Channel Selector",
                                                                                  "identifier": "FRONT_RDF_CHANNEL",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 5
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8236,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 7,
                                                                                                      "max_value": 5,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "limited_rotary"
                                                                     },
                                                "FRONT_RDF_CSWITCH": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore RDF Control",
                                                                                  "identifier": "FRONT_RDF_CSWITCH",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8236,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 16,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 4,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     },
                                                 "FRONT_RDF_LISTEN": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore RDF Listen Mode",
                                                                                  "identifier": "FRONT_RDF_LISTEN",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8224,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 16384,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 14,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "toggle_switch"
                                                                     },
                                                 "FRONT_RDF_MODE12": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore RDF Mode",
                                                                                  "identifier": "FRONT_RDF_MODE12",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8224,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 32768,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 15,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "toggle_switch"
                                                                     },
                                                  "FRONT_RDF_MODE3": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore RDF Loop",
                                                                                  "identifier": "FRONT_RDF_MODE3",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8236,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 8,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 3,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     },
                                                 "FRONT_RDF_VOLUME": {
                                                                             "category": "ARK 15M",
                                                                         "control_type": "limited_dial",
                                                                          "description": "Fore RDF Volume",
                                                                           "identifier": "FRONT_RDF_VOLUME",
                                                                               "inputs": [ {
                                                                                             "description": "set the position of the dial",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 65535
                                                                                         }, {
                                                                                                "description": "turn the dial left or right",
                                                                                                  "interface": "variable_step",
                                                                                                  "max_value": 65535,
                                                                                             "suggested_step": 3200
                                                                                         } ],
                                                                              "outputs": [ {
                                                                                                 "address": 8238,
                                                                                             "description": "position of the potentiometer",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                      "REAR_CB_ADF": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear ADF Marker",
                                                                                  "identifier": "REAR_CB_ADF",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8264,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 128,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 7,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "toggle_switch"
                                                                     },
                                                 "REAR_RDF_CHANNEL": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear RDF Channel Selector",
                                                                                  "identifier": "REAR_RDF_CHANNEL",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 5
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8264,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 7,
                                                                                                      "max_value": 5,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "limited_rotary"
                                                                     },
                                                 "REAR_RDF_CSWITCH": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear RDF Control",
                                                                                  "identifier": "REAR_RDF_CSWITCH",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8264,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 64,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 6,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     },
                                                  "REAR_RDF_LISTEN": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear RDF Listen Mode",
                                                                                  "identifier": "REAR_RDF_LISTEN",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8264,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 8,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 3,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "toggle_switch"
                                                                     },
                                                  "REAR_RDF_MODE12": {
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear RDF Mode",
                                                                                  "identifier": "REAR_RDF_MODE12",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8264,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 16,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 4,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "toggle_switch"
                                                                     },
                                                   "REAR_RDF_MODE3": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "ARK 15M",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear RDF Loop",
                                                                                  "identifier": "REAR_RDF_MODE3",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8264,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 32,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 5,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     },
                                                  "REAR_RDF_VOLUME": {
                                                                             "category": "ARK 15M",
                                                                         "control_type": "limited_dial",
                                                                          "description": "Rear RDF Volume",
                                                                           "identifier": "REAR_RDF_VOLUME",
                                                                               "inputs": [ {
                                                                                             "description": "set the position of the dial",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 65535
                                                                                         }, {
                                                                                                "description": "turn the dial left or right",
                                                                                                  "interface": "variable_step",
                                                                                                  "max_value": 65535,
                                                                                             "suggested_step": 3200
                                                                                         } ],
                                                                              "outputs": [ {
                                                                                                 "address": 8266,
                                                                                             "description": "position of the potentiometer",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     }
                                            },
                                "BAKLAN-5": {
                                                "FRONT_VHF_RADIO_KHZ": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "BAKLAN-5",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Fore VHF Radio Tune khz",
                                                                             "identifier": "FRONT_VHF_RADIO_KHZ",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8214,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                "FRONT_VHF_RADIO_MHZ": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "BAKLAN-5",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Fore VHF Radio Tune mhz",
                                                                             "identifier": "FRONT_VHF_RADIO_MHZ",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8212,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                 "FRONT_VHF_RADIO_SQ": {
                                                                                      "category": "BAKLAN-5",
                                                                                  "control_type": "selector",
                                                                                   "description": "Fore VHF Radio Squelch",
                                                                                    "identifier": "FRONT_VHF_RADIO_SQ",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8200,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 4,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                "FRONT_VHF_RADIO_VOL": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "BAKLAN-5",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Fore VHF Radio Volume Knob",
                                                                             "identifier": "FRONT_VHF_RADIO_VOL",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8210,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       }
                                            },
                                  "Canopy": {
                                                "FRONT_HATCH_JET": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Canopy",
                                                                              "control_type": "selector",
                                                                               "description": "Fore Canopy Jettison",
                                                                                "identifier": "FRONT_HATCH_JET",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 8236,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 256,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 8,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   },
                                                  "FRONT_HATCH_L": {
                                                                                  "category": "Canopy",
                                                                              "control_type": "selector",
                                                                               "description": "Fore Left Canopy Lever",
                                                                                "identifier": "FRONT_HATCH_L",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 8236,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 64,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 6,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                  "FRONT_HATCH_R": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Canopy",
                                                                              "control_type": "selector",
                                                                               "description": "Fore Right Canopy Lever",
                                                                                "identifier": "FRONT_HATCH_R",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 8236,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 128,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 7,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   },
                                                 "REAR_HATCH_JET": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Canopy",
                                                                              "control_type": "selector",
                                                                               "description": "Rear Canopy Jettison",
                                                                                "identifier": "REAR_HATCH_JET",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 8264,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 1024,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 10,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   },
                                                   "REAR_HATCH_L": {
                                                                                  "category": "Canopy",
                                                                              "control_type": "selector",
                                                                               "description": "Rear Left Canopy Lever",
                                                                                "identifier": "REAR_HATCH_L",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 8264,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 256,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 8,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "toggle_switch"
                                                                   },
                                                   "REAR_HATCH_R": {
                                                                               "api_variant": "momentary_last_position",
                                                                                  "category": "Canopy",
                                                                              "control_type": "selector",
                                                                               "description": "Rear Right Canopy Lever",
                                                                                "identifier": "REAR_HATCH_R",
                                                                                    "inputs": [ {
                                                                                                  "description": "switch to previous or next state",
                                                                                                    "interface": "fixed_step"
                                                                                              }, {
                                                                                                  "description": "set position",
                                                                                                    "interface": "set_state",
                                                                                                    "max_value": 1
                                                                                              }, {
                                                                                                     "argument": "TOGGLE",
                                                                                                  "description": "Toggle switch state",
                                                                                                    "interface": "action"
                                                                                              } ],
                                                                       "momentary_positions": "none",
                                                                                   "outputs": [ {
                                                                                                      "address": 8264,
                                                                                                  "description": "selector position",
                                                                                                         "mask": 512,
                                                                                                    "max_value": 1,
                                                                                                     "shift_by": 9,
                                                                                                       "suffix": "",
                                                                                                         "type": "integer"
                                                                                              } ],
                                                                          "physical_variant": "push_button"
                                                                   }
                                            },
                        "Circuit Breakers": {
                                                     "FRONT_CB_BATTERY": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Battery Selector",
                                                                                      "identifier": "FRONT_CB_BATTERY",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 32,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 5,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                      "FRONT_CB_E_HEAT": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore SSKUA-1 Heater CB",
                                                                                      "identifier": "FRONT_CB_E_HEAT",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1024,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 10,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                     "FRONT_CB_E_INSTR": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Engine Instrumentation CB",
                                                                                      "identifier": "FRONT_CB_E_INSTR",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8224,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 16,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 4,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                   "FRONT_CB_GENERATOR": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Generator CB",
                                                                                      "identifier": "FRONT_CB_GENERATOR",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 64,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 6,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                    "FRONT_CB_IGNITION": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Ignition CB",
                                                                                      "identifier": "FRONT_CB_IGNITION",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 128,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 7,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                    "FRONT_CB_INTERCOM": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Intercom CB",
                                                                                      "identifier": "FRONT_CB_INTERCOM",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8224,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 0,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                      "FRONT_CB_OILDIL": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Oil Dilution Button",
                                                                                      "identifier": "FRONT_CB_OILDIL",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 512,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 9,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                       "FRONT_CB_PITOT": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Pitot Heater CB",
                                                                                      "identifier": "FRONT_CB_PITOT",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 256,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 8,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                       "FRONT_CB_RADIO": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Radio CB",
                                                                                      "identifier": "FRONT_CB_RADIO",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 32768,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 15,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                         "FRONT_CB_RDF": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore RDF CB",
                                                                                      "identifier": "FRONT_CB_RDF",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8224,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 32,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 5,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                         "FRONT_CB_SDG": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore SDG CB",
                                                                                      "identifier": "FRONT_CB_SDG",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8224,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 64,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 6,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                       "FRONT_CB_STALL": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore SSKUA-1 CB",
                                                                                      "identifier": "FRONT_CB_STALL",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2048,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 11,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                          "FRONT_CB_UC": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore U/C CB",
                                                                                      "identifier": "FRONT_CB_UC",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8224,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 4,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 2,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                   "FRONT_CB_UMFORMER1": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore PT-200 CB",
                                                                                      "identifier": "FRONT_CB_UMFORMER1",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8224,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 8,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 3,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                   "FRONT_CB_UMFORMER2": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore PAG-1 CB",
                                                                                      "identifier": "FRONT_CB_UMFORMER2",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8224,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 1,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                   "REAR_CB_BRAKES_CUT": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Rear Wheel Brakes Purge CB",
                                                                                      "identifier": "REAR_CB_BRAKES_CUT",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8240,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 32768,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 15,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                    "REAR_CB_TPANEL_AH": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Rear Trainer AH CB",
                                                                                      "identifier": "REAR_CB_TPANEL_AH",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8240,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1024,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 10,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                "REAR_CB_TPANEL_MASTER": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Rear Trainer Master CB",
                                                                                      "identifier": "REAR_CB_TPANEL_MASTER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8240,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 256,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 8,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                 "REAR_CB_TPANEL_SPEED": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Rear Trainer Speedo CB",
                                                                                      "identifier": "REAR_CB_TPANEL_SPEED",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8240,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 512,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 9,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                  "REAR_CB_TPANEL_STAT": {
                                                                                        "category": "Circuit Breakers",
                                                                                    "control_type": "selector",
                                                                                     "description": "Rear Trainer Statistics CB",
                                                                                      "identifier": "REAR_CB_TPANEL_STAT",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8240,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2048,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 11,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         }
                                            },
                 "External Aircraft Model": {
                                                 "EXT_WOW_LEFT": {
                                                                         "category": "External Aircraft Model",
                                                                     "control_type": "metadata",
                                                                      "description": "Weight ON Wheels Left Gear",
                                                                       "identifier": "EXT_WOW_LEFT",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 8384,
                                                                                         "description": "Weight ON Wheels Left Gear",
                                                                                                "mask": 128,
                                                                                           "max_value": 1,
                                                                                            "shift_by": 7,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                 "EXT_WOW_NOSE": {
                                                                         "category": "External Aircraft Model",
                                                                     "control_type": "metadata",
                                                                      "description": "Weight ON Wheels Nose Gear",
                                                                       "identifier": "EXT_WOW_NOSE",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 8384,
                                                                                         "description": "Weight ON Wheels Nose Gear",
                                                                                                "mask": 32,
                                                                                           "max_value": 1,
                                                                                            "shift_by": 5,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 },
                                                "EXT_WOW_RIGHT": {
                                                                         "category": "External Aircraft Model",
                                                                     "control_type": "metadata",
                                                                      "description": "Weight ON Wheels Right Gear",
                                                                       "identifier": "EXT_WOW_RIGHT",
                                                                           "inputs": [  ],
                                                                          "outputs": [ {
                                                                                             "address": 8384,
                                                                                         "description": "Weight ON Wheels Right Gear",
                                                                                                "mask": 64,
                                                                                           "max_value": 1,
                                                                                            "shift_by": 6,
                                                                                              "suffix": "",
                                                                                                "type": "integer"
                                                                                     } ]
                                                                 }
                                            },
                         "Fore Main Panel": {
                                                      "FRONT_ACCEL_BTN": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Accelerometer Button",
                                                                                      "identifier": "FRONT_ACCEL_BTN",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 256,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 8,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                  "FRONT_AHORIZON_LOCK": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Artificial Horizon LOCK Button",
                                                                                      "identifier": "FRONT_AHORIZON_LOCK",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 512,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 9,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                  "FRONT_AHORIZON_ZERO": {
                                                                              "api_variant": "multiturn",
                                                                                 "category": "Fore Main Panel",
                                                                             "control_type": "analog_dial",
                                                                              "description": "Fore Artificial Horizon Zeroing",
                                                                               "identifier": "FRONT_AHORIZON_ZERO",
                                                                                   "inputs": [ {
                                                                                                    "description": "turn the dial left or right",
                                                                                                      "interface": "variable_step",
                                                                                                      "max_value": 65535,
                                                                                                 "suggested_step": 3200
                                                                                             } ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8196,
                                                                                                 "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "_KNOB_POS",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "FRONT_ALT_KNOB": {
                                                                              "api_variant": "multiturn",
                                                                                 "category": "Fore Main Panel",
                                                                             "control_type": "analog_dial",
                                                                              "description": "Fore Altimeter Knob",
                                                                               "identifier": "FRONT_ALT_KNOB",
                                                                                   "inputs": [ {
                                                                                                    "description": "turn the dial left or right",
                                                                                                      "interface": "variable_step",
                                                                                                      "max_value": 65535,
                                                                                                 "suggested_step": 3200
                                                                                             } ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8194,
                                                                                                 "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "_KNOB_POS",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                   "FRONT_CLOCK_PUSH_L": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Clock Left Push Button",
                                                                                      "identifier": "FRONT_CLOCK_PUSH_L",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 0,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                   "FRONT_CLOCK_PUSH_R": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Clock Right Push Button",
                                                                                      "identifier": "FRONT_CLOCK_PUSH_R",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8200,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 1,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                 "FRONT_CLOCK_ROTATE_L": {
                                                                              "api_variant": "multiturn",
                                                                                 "category": "Fore Main Panel",
                                                                             "control_type": "analog_dial",
                                                                              "description": "Fore Clock Left Rotate Knob",
                                                                               "identifier": "FRONT_CLOCK_ROTATE_L",
                                                                                   "inputs": [ {
                                                                                                    "description": "turn the dial left or right",
                                                                                                      "interface": "variable_step",
                                                                                                      "max_value": 65535,
                                                                                                 "suggested_step": 3200
                                                                                             } ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8202,
                                                                                                 "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "_KNOB_POS",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                 "FRONT_CLOCK_ROTATE_R": {
                                                                              "api_variant": "multiturn",
                                                                                 "category": "Fore Main Panel",
                                                                             "control_type": "analog_dial",
                                                                              "description": "Fore Clock Right Rotate Knob",
                                                                               "identifier": "FRONT_CLOCK_ROTATE_R",
                                                                                   "inputs": [ {
                                                                                                    "description": "turn the dial left or right",
                                                                                                      "interface": "variable_step",
                                                                                                      "max_value": 65535,
                                                                                                 "suggested_step": 3200
                                                                                             } ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8204,
                                                                                                 "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "_KNOB_POS",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                 "FRONT_FUEL_GAUGE_DIM": {
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Fuel Gauge Dimmer",
                                                                                      "identifier": "FRONT_FUEL_GAUGE_DIM",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 8192,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 13,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                "FRONT_FUEL_GAUGE_TEST": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Fuel Gauge Test Button",
                                                                                      "identifier": "FRONT_FUEL_GAUGE_TEST",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 4096,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 12,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                       "FRONT_HSI_KNOB": {
                                                                              "api_variant": "multiturn",
                                                                                 "category": "Fore Main Panel",
                                                                             "control_type": "analog_dial",
                                                                              "description": "Fore HSI Knob",
                                                                               "identifier": "FRONT_HSI_KNOB",
                                                                                   "inputs": [ {
                                                                                                    "description": "turn the dial left or right",
                                                                                                      "interface": "variable_step",
                                                                                                      "max_value": 65535,
                                                                                                 "suggested_step": 3200
                                                                                             } ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8198,
                                                                                                 "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "_KNOB_POS",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                      "FRONT_LAMP_TEST": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Lamp Test Button",
                                                                                      "identifier": "FRONT_LAMP_TEST",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 64,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 6,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                     "FRONT_MAGNET_SEL": {
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Magnet Selector",
                                                                                      "identifier": "FRONT_MAGNET_SEL",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 3
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 48,
                                                                                                          "max_value": 3,
                                                                                                           "shift_by": 4,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "limited_rotary"
                                                                         },
                                                    "FRONT_PRIMER_PUMP": {
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Primer Pump Selector OFF/Trunk/Cylinders",
                                                                                      "identifier": "FRONT_PRIMER_PUMP",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 2
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 49152,
                                                                                                          "max_value": 2,
                                                                                                           "shift_by": 14,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "limited_rotary"
                                                                         },
                                                          "FRONT_SMOKE": {
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Smoke Apparat",
                                                                                      "identifier": "FRONT_SMOKE",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 1,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                     "FRONT_STALL_TEST": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Stall Warning Test Button",
                                                                                      "identifier": "FRONT_STALL_TEST",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 128,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 7,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                        "FRONT_STARTER": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Starter Button",
                                                                                      "identifier": "FRONT_STARTER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 8,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 3,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                  "FRONT_STARTER_COVER": {
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Starter Button Cover",
                                                                                      "identifier": "FRONT_STARTER_COVER",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 4,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 2,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                       "FRONT_UCE_LOCK": {
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Undercarriage Extension Lock",
                                                                                      "identifier": "FRONT_UCE_LOCK",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1024,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 10,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "toggle_switch"
                                                                         },
                                                    "FRONT_VOLTAMP_BTN": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Voltamperemeter Button",
                                                                                      "identifier": "FRONT_VOLTAMP_BTN",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 2048,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 11,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         },
                                                   "FRONT_WBRAKES_LOCK": {
                                                                                     "api_variant": "momentary_last_position",
                                                                                        "category": "Fore Main Panel",
                                                                                    "control_type": "selector",
                                                                                     "description": "Fore Wheel Brakes Lock",
                                                                                      "identifier": "FRONT_WBRAKES_LOCK",
                                                                                          "inputs": [ {
                                                                                                        "description": "switch to previous or next state",
                                                                                                          "interface": "fixed_step"
                                                                                                    }, {
                                                                                                        "description": "set position",
                                                                                                          "interface": "set_state",
                                                                                                          "max_value": 1
                                                                                                    }, {
                                                                                                           "argument": "TOGGLE",
                                                                                                        "description": "Toggle switch state",
                                                                                                          "interface": "action"
                                                                                                    } ],
                                                                             "momentary_positions": "none",
                                                                                         "outputs": [ {
                                                                                                            "address": 8192,
                                                                                                        "description": "selector position",
                                                                                                               "mask": 1,
                                                                                                          "max_value": 1,
                                                                                                           "shift_by": 0,
                                                                                                             "suffix": "",
                                                                                                               "type": "integer"
                                                                                                    } ],
                                                                                "physical_variant": "push_button"
                                                                         }
                                            },
                                  "GMK-1A": {
                                                "FRONT_SDG_CONTROL": {
                                                                                    "category": "GMK-1A",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore Gyro Test Switch, 0 deg/OFF/300deg",
                                                                                  "identifier": "FRONT_SDG_CONTROL",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 2
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8224,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 3072,
                                                                                                      "max_value": 2,
                                                                                                       "shift_by": 10,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "3_position_switch"
                                                                     },
                                                 "FRONT_SDG_COURSE": {
                                                                                    "category": "GMK-1A",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore Gyro Heading Selector, Counter-Clockwise/OFF/Clockwise",
                                                                                  "identifier": "FRONT_SDG_COURSE",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 2
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8224,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 12288,
                                                                                                      "max_value": 2,
                                                                                                       "shift_by": 12,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "3_position_switch"
                                                                     },
                                                   "FRONT_SDG_HEMI": {
                                                                                    "category": "GMK-1A",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore Gyro Hemisphere Selector",
                                                                                  "identifier": "FRONT_SDG_HEMI",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8224,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 256,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 8,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "toggle_switch"
                                                                     },
                                                    "FRONT_SDG_LAT": {
                                                                          "api_variant": "multiturn",
                                                                             "category": "GMK-1A",
                                                                         "control_type": "analog_dial",
                                                                          "description": "Fore Gyro Latitude Selector",
                                                                           "identifier": "FRONT_SDG_LAT",
                                                                               "inputs": [ {
                                                                                                "description": "turn the dial left or right",
                                                                                                  "interface": "variable_step",
                                                                                                  "max_value": 65535,
                                                                                             "suggested_step": 3200
                                                                                         } ],
                                                                              "outputs": [ {
                                                                                                 "address": 8234,
                                                                                             "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "_KNOB_POS",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                   "FRONT_SDG_MODE": {
                                                                                    "category": "GMK-1A",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore Gyro Mode MC/GC",
                                                                                  "identifier": "FRONT_SDG_MODE",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8224,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 512,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 9,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "limited_rotary"
                                                                     }
                                            },
                                  "Gauges": {
                                                      "FRONT_ACCEL_MAX": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Accelerometer Max",
                                                                               "identifier": "FRONT_ACCEL_MAX",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8272,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                      "FRONT_ACCEL_MIN": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Accelerometer Min",
                                                                               "identifier": "FRONT_ACCEL_MIN",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8270,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                   "FRONT_ACCEL_MINUTE": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Accelerometer Minute",
                                                                               "identifier": "FRONT_ACCEL_MINUTE",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8268,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "FRONT_AH_BANK": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Artificial Horizon Bank",
                                                                               "identifier": "FRONT_AH_BANK",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8308,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "FRONT_AH_PITCH": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Artificial Horizon Pitch",
                                                                               "identifier": "FRONT_AH_PITCH",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8310,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "FRONT_AH_SLIP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Artificial Horizon Sideslip",
                                                                               "identifier": "FRONT_AH_SLIP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8312,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "FRONT_AIRSPEED": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Airspeed Gauge",
                                                                               "identifier": "FRONT_AIRSPEED",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8280,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                         "FRONT_ALT100": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Altimeter 100",
                                                                               "identifier": "FRONT_ALT100",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8284,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "FRONT_ALT1000": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Altimeter 1000",
                                                                               "identifier": "FRONT_ALT1000",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8286,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                      "FRONT_ALT_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Altimeter Set Pressure",
                                                                               "identifier": "FRONT_ALT_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8288,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                   "FRONT_COMPASS_BANK": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Compass Bank",
                                                                               "identifier": "FRONT_COMPASS_BANK",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8368,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                    "FRONT_COMPASS_HDG": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Compass Heading",
                                                                               "identifier": "FRONT_COMPASS_HDG",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8370,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                  "FRONT_COMPASS_PITCH": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Compass Pitch",
                                                                               "identifier": "FRONT_COMPASS_PITCH",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8366,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "FRONT_CYL_TEMP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Cylinder Heads Temperature Gauge",
                                                                               "identifier": "FRONT_CYL_TEMP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8354,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                     "FRONT_FUEL_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Fuel Pressure Gauge",
                                                                               "identifier": "FRONT_FUEL_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8346,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                      "FRONT_OIL_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Oil Pressure Gauge",
                                                                               "identifier": "FRONT_OIL_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8342,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "FRONT_OIL_TEMP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Oil Temperature Gauge",
                                                                               "identifier": "FRONT_OIL_TEMP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8344,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                "FRONT_PNEU_MAIN_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Pneumatic Main Pressure Gauge",
                                                                               "identifier": "FRONT_PNEU_MAIN_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8358,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                "FRONT_PNEU_STBY_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Pneumatic Standby Pressure Gauge",
                                                                               "identifier": "FRONT_PNEU_STBY_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8360,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                           "FRONT_SLIP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Sideslip Gauge",
                                                                               "identifier": "FRONT_SLIP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8300,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                          "FRONT_TACHO": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Tachometer Gauge",
                                                                               "identifier": "FRONT_TACHO",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8320,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                           "FRONT_TURN": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Turn Gauge",
                                                                               "identifier": "FRONT_TURN",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8298,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                  "FRONT_UGR4K_BCN_CRS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore UGR-4K Beacon Course",
                                                                               "identifier": "FRONT_UGR4K_BCN_CRS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8334,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                 "FRONT_UGR4K_CURR_CRS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore UGR-4K Current Course",
                                                                               "identifier": "FRONT_UGR4K_CURR_CRS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8330,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                  "FRONT_UGR4K_SET_CRS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore UGR-4K Set Course",
                                                                               "identifier": "FRONT_UGR4K_SET_CRS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8332,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                     "FRONT_VARIOMETER": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Fore Variometer Gauge",
                                                                               "identifier": "FRONT_VARIOMETER",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8296,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "MANIFOLD_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Manifold Pressure Gauge",
                                                                               "identifier": "MANIFOLD_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8324,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "MANIFOLD_TEMP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Manifold Temperature Gauge",
                                                                               "identifier": "MANIFOLD_TEMP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8326,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "REAR_ACCEL_MAX": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Accelerometer Max",
                                                                               "identifier": "REAR_ACCEL_MAX",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8278,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "REAR_ACCEL_MIN": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Accelerometer Min",
                                                                               "identifier": "REAR_ACCEL_MIN",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8276,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                    "REAR_ACCEL_MINUTE": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Accelerometer Minute",
                                                                               "identifier": "REAR_ACCEL_MINUTE",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8274,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                         "REAR_AH_BANK": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Artificial Horizon Bank",
                                                                               "identifier": "REAR_AH_BANK",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8314,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "REAR_AH_PITCH": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Artificial Horizon Pitch",
                                                                               "identifier": "REAR_AH_PITCH",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8316,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                         "REAR_AH_SLIP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Artificial Horizon Sideslip",
                                                                               "identifier": "REAR_AH_SLIP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8318,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "REAR_AIRSPEED": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Airspeed Gauge",
                                                                               "identifier": "REAR_AIRSPEED",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8282,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                          "REAR_ALT100": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Altimeter 100",
                                                                               "identifier": "REAR_ALT100",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8290,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                         "REAR_ALT1000": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Altimeter 1000",
                                                                               "identifier": "REAR_ALT1000",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8292,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "REAR_ALT_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Altimeter Set Pressure",
                                                                               "identifier": "REAR_ALT_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8294,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                    "REAR_COMPASS_BANK": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Compass Bank",
                                                                               "identifier": "REAR_COMPASS_BANK",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8374,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                     "REAR_COMPASS_HDG": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Compass Heading",
                                                                               "identifier": "REAR_COMPASS_HDG",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8376,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                   "REAR_COMPASS_PITCH": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Compass Pitch",
                                                                               "identifier": "REAR_COMPASS_PITCH",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8372,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "REAR_CYL_TEMP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Cylinder Heads Temperature Gauge",
                                                                               "identifier": "REAR_CYL_TEMP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8356,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                      "REAR_FUEL_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Fuel Pressure Gauge",
                                                                               "identifier": "REAR_FUEL_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8352,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                       "REAR_OIL_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Oil Pressure Gauge",
                                                                               "identifier": "REAR_OIL_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8348,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                        "REAR_OIL_TEMP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Oil Temperature Gauge",
                                                                               "identifier": "REAR_OIL_TEMP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8350,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                 "REAR_PNEU_MAIN_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Pneumatic Main Pressure Gauge",
                                                                               "identifier": "REAR_PNEU_MAIN_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8362,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                 "REAR_PNEU_STBY_PRESS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Pneumatic Standby Pressure Gauge",
                                                                               "identifier": "REAR_PNEU_STBY_PRESS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8364,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                            "REAR_SLIP": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Sideslip Gauge",
                                                                               "identifier": "REAR_SLIP",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8306,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                           "REAR_TACHO": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Tachometer Gauge",
                                                                               "identifier": "REAR_TACHO",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8322,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                            "REAR_TURN": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Turn Gauge",
                                                                               "identifier": "REAR_TURN",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8304,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                   "REAR_UGR4K_BCN_CRS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear UGR-4K Beacon Course",
                                                                               "identifier": "REAR_UGR4K_BCN_CRS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8340,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                  "REAR_UGR4K_CURR_CRS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear UGR-4K Current Course",
                                                                               "identifier": "REAR_UGR4K_CURR_CRS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8336,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                   "REAR_UGR4K_SET_CRS": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear UGR-4K Set Course",
                                                                               "identifier": "REAR_UGR4K_SET_CRS",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8338,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                      "REAR_VARIOMETER": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Rear Variometer Gauge",
                                                                               "identifier": "REAR_VARIOMETER",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8302,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         },
                                                          "VOLTMETER_G": {
                                                                                 "category": "Gauges",
                                                                             "control_type": "analog_gauge",
                                                                              "description": "Volt Amperemeter Gauge",
                                                                               "identifier": "VOLTMETER_G",
                                                                                   "inputs": [  ],
                                                                                  "outputs": [ {
                                                                                                     "address": 8328,
                                                                                                 "description": "gauge position",
                                                                                                        "mask": 65535,
                                                                                                   "max_value": 65535,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ]
                                                                         }
                                            },
                        "Louvers Quadrant": {
                                                "FRONT_FRIC_R_LEVER": {
                                                                              "category": "Louvers Quadrant",
                                                                          "control_type": "limited_dial",
                                                                           "description": "Fore Right Frictioner Lever",
                                                                            "identifier": "FRONT_FRIC_R_LEVER",
                                                                                "inputs": [ {
                                                                                              "description": "set the position of the dial",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 65535
                                                                                          }, {
                                                                                                 "description": "turn the dial left or right",
                                                                                                   "interface": "variable_step",
                                                                                                   "max_value": 65535,
                                                                                              "suggested_step": 3200
                                                                                          } ],
                                                                               "outputs": [ {
                                                                                                  "address": 8230,
                                                                                              "description": "position of the potentiometer",
                                                                                                     "mask": 65535,
                                                                                                "max_value": 65535,
                                                                                                 "shift_by": 0,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "FRONT_ORADIATOR": {
                                                                              "category": "Louvers Quadrant",
                                                                          "control_type": "limited_dial",
                                                                           "description": "Fore Oil Radiator Lever",
                                                                            "identifier": "FRONT_ORADIATOR",
                                                                                "inputs": [ {
                                                                                              "description": "set the position of the dial",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 65535
                                                                                          }, {
                                                                                                 "description": "turn the dial left or right",
                                                                                                   "interface": "variable_step",
                                                                                                   "max_value": 65535,
                                                                                              "suggested_step": 3200
                                                                                          } ],
                                                                               "outputs": [ {
                                                                                                  "address": 8228,
                                                                                              "description": "position of the potentiometer",
                                                                                                     "mask": 65535,
                                                                                                "max_value": 65535,
                                                                                                 "shift_by": 0,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "FRONT_WRADIATOR": {
                                                                              "category": "Louvers Quadrant",
                                                                          "control_type": "limited_dial",
                                                                           "description": "Fore Cooling Flaps Lever",
                                                                            "identifier": "FRONT_WRADIATOR",
                                                                                "inputs": [ {
                                                                                              "description": "set the position of the dial",
                                                                                                "interface": "set_state",
                                                                                                "max_value": 65535
                                                                                          }, {
                                                                                                 "description": "turn the dial left or right",
                                                                                                   "interface": "variable_step",
                                                                                                   "max_value": 65535,
                                                                                              "suggested_step": 3200
                                                                                          } ],
                                                                               "outputs": [ {
                                                                                                  "address": 8226,
                                                                                              "description": "position of the potentiometer",
                                                                                                     "mask": 65535,
                                                                                                "max_value": 65535,
                                                                                                 "shift_by": 0,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      }
                                            },
                               "Port Wall": {
                                                 "FRONT_FUEL_COCK": {
                                                                                "api_variant": "momentary_last_position",
                                                                                   "category": "Port Wall",
                                                                               "control_type": "selector",
                                                                                "description": "Fore Fuel Cock",
                                                                                 "identifier": "FRONT_FUEL_COCK",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 8200,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 16384,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 14,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "push_button"
                                                                    },
                                                "FRONT_PNEM_VALVE": {
                                                                         "api_variant": "multiturn",
                                                                            "category": "Port Wall",
                                                                        "control_type": "analog_dial",
                                                                         "description": "Fore Pneumatic System Master Valve",
                                                                          "identifier": "FRONT_PNEM_VALVE",
                                                                              "inputs": [ {
                                                                                               "description": "turn the dial left or right",
                                                                                                 "interface": "variable_step",
                                                                                                 "max_value": 65535,
                                                                                            "suggested_step": 3200
                                                                                        } ],
                                                                             "outputs": [ {
                                                                                                "address": 8222,
                                                                                            "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                   "mask": 65535,
                                                                                              "max_value": 65535,
                                                                                               "shift_by": 0,
                                                                                                 "suffix": "_KNOB_POS",
                                                                                                   "type": "integer"
                                                                                        } ]
                                                                    },
                                                "FRONT_TRIM_WHEEL": {
                                                                         "api_variant": "multiturn",
                                                                            "category": "Port Wall",
                                                                        "control_type": "analog_dial",
                                                                         "description": "Fore Elevator Trim Wheel",
                                                                          "identifier": "FRONT_TRIM_WHEEL",
                                                                              "inputs": [ {
                                                                                               "description": "turn the dial left or right",
                                                                                                 "interface": "variable_step",
                                                                                                 "max_value": 65535,
                                                                                            "suggested_step": 3200
                                                                                        } ],
                                                                             "outputs": [ {
                                                                                                "address": 8220,
                                                                                            "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                   "mask": 65535,
                                                                                              "max_value": 65535,
                                                                                               "shift_by": 0,
                                                                                                 "suffix": "_KNOB_POS",
                                                                                                   "type": "integer"
                                                                                        } ]
                                                                    },
                                                  "REAR_FUEL_COCK": {
                                                                                "api_variant": "momentary_last_position",
                                                                                   "category": "Port Wall",
                                                                               "control_type": "selector",
                                                                                "description": "Rear Fuel Cock",
                                                                                 "identifier": "REAR_FUEL_COCK",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 8240,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 16384,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 14,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "push_button"
                                                                    },
                                                 "REAR_TRIM_WHEEL": {
                                                                         "api_variant": "multiturn",
                                                                            "category": "Port Wall",
                                                                        "control_type": "analog_dial",
                                                                         "description": "Rear Elevator Trim Wheel",
                                                                          "identifier": "REAR_TRIM_WHEEL",
                                                                              "inputs": [ {
                                                                                               "description": "turn the dial left or right",
                                                                                                 "interface": "variable_step",
                                                                                                 "max_value": 65535,
                                                                                            "suggested_step": 3200
                                                                                        } ],
                                                                             "outputs": [ {
                                                                                                "address": 8260,
                                                                                            "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                   "mask": 65535,
                                                                                              "max_value": 65535,
                                                                                               "shift_by": 0,
                                                                                                 "suffix": "_KNOB_POS",
                                                                                                   "type": "integer"
                                                                                        } ]
                                                                    }
                                            },
                         "Rear Main Panel": {
                                                     "REAR_ACCEL_BTN": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Accelerometer Button",
                                                                                    "identifier": "REAR_ACCEL_BTN",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8240,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 4,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 2,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                 "REAR_AHORIZON_LOCK": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Artificial Horizon LOCK Button",
                                                                                    "identifier": "REAR_AHORIZON_LOCK",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8240,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 8,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 3,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                 "REAR_AHORIZON_ZERO": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Rear Main Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Rear Artificial Horizon Zeroing",
                                                                             "identifier": "REAR_AHORIZON_ZERO",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8244,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                      "REAR_ALT_KNOB": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Rear Main Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Rear Altimeter Knob",
                                                                             "identifier": "REAR_ALT_KNOB",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8242,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                    "REAR_BRAKES_CUT": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Wheel Brakes Purge",
                                                                                    "identifier": "REAR_BRAKES_CUT",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8236,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 1024,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 10,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                  "REAR_CLOCK_PUSH_L": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Clock Left Push Button",
                                                                                    "identifier": "REAR_CLOCK_PUSH_L",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8240,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 4,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                  "REAR_CLOCK_PUSH_R": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Clock Right Push Button",
                                                                                    "identifier": "REAR_CLOCK_PUSH_R",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8240,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 5,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                "REAR_CLOCK_ROTATE_L": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Rear Main Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Rear Clock Left Rotate Knob",
                                                                             "identifier": "REAR_CLOCK_ROTATE_L",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8248,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                "REAR_CLOCK_ROTATE_R": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Rear Main Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Rear Clock Right Rotate Knob",
                                                                             "identifier": "REAR_CLOCK_ROTATE_R",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8250,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                      "REAR_HSI_KNOB": {
                                                                            "api_variant": "multiturn",
                                                                               "category": "Rear Main Panel",
                                                                           "control_type": "analog_dial",
                                                                            "description": "Rear HSI Knob",
                                                                             "identifier": "REAR_HSI_KNOB",
                                                                                 "inputs": [ {
                                                                                                  "description": "turn the dial left or right",
                                                                                                    "interface": "variable_step",
                                                                                                    "max_value": 65535,
                                                                                               "suggested_step": 3200
                                                                                           } ],
                                                                                "outputs": [ {
                                                                                                   "address": 8246,
                                                                                               "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                      "mask": 65535,
                                                                                                 "max_value": 65535,
                                                                                                  "shift_by": 0,
                                                                                                    "suffix": "_KNOB_POS",
                                                                                                      "type": "integer"
                                                                                           } ]
                                                                       },
                                                      "REAR_IGNITION": {
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Ignition Source Switch",
                                                                                    "identifier": "REAR_IGNITION",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8236,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 2048,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 11,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                     "REAR_LAMP_TEST": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Lamp Test Button",
                                                                                    "identifier": "REAR_LAMP_TEST",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8240,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 2,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 1,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                    "REAR_MAGNET_SEL": {
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Magnet Selector",
                                                                                    "identifier": "REAR_MAGNET_SEL",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 3
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8236,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 12288,
                                                                                                        "max_value": 3,
                                                                                                         "shift_by": 12,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "limited_rotary"
                                                                       },
                                                       "REAR_STARTER": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Starter Button",
                                                                                    "identifier": "REAR_STARTER",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8236,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 32768,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 15,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       },
                                                 "REAR_STARTER_COVER": {
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Starter Button Cover",
                                                                                    "identifier": "REAR_STARTER_COVER",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8236,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 16384,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 14,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                      "REAR_UCE_LOCK": {
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Undercarriage Extension Lock",
                                                                                    "identifier": "REAR_UCE_LOCK",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8240,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 1,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 0,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "toggle_switch"
                                                                       },
                                                  "REAR_WBRAKES_LOCK": {
                                                                                   "api_variant": "momentary_last_position",
                                                                                      "category": "Rear Main Panel",
                                                                                  "control_type": "selector",
                                                                                   "description": "Rear Wheel Brakes Lock",
                                                                                    "identifier": "REAR_WBRAKES_LOCK",
                                                                                        "inputs": [ {
                                                                                                      "description": "switch to previous or next state",
                                                                                                        "interface": "fixed_step"
                                                                                                  }, {
                                                                                                      "description": "set position",
                                                                                                        "interface": "set_state",
                                                                                                        "max_value": 1
                                                                                                  }, {
                                                                                                         "argument": "TOGGLE",
                                                                                                      "description": "Toggle switch state",
                                                                                                        "interface": "action"
                                                                                                  } ],
                                                                           "momentary_positions": "none",
                                                                                       "outputs": [ {
                                                                                                          "address": 8236,
                                                                                                      "description": "selector position",
                                                                                                             "mask": 512,
                                                                                                        "max_value": 1,
                                                                                                         "shift_by": 9,
                                                                                                           "suffix": "",
                                                                                                             "type": "integer"
                                                                                                  } ],
                                                                              "physical_variant": "push_button"
                                                                       }
                                            },
                                    "SPU9": {
                                                       "FRONT_ICOM_RDF_SW": {
                                                                                           "category": "SPU9",
                                                                                       "control_type": "selector",
                                                                                        "description": "Fore Intercom RDF Switch",
                                                                                         "identifier": "FRONT_ICOM_RDF_SW",
                                                                                             "inputs": [ {
                                                                                                           "description": "switch to previous or next state",
                                                                                                             "interface": "fixed_step"
                                                                                                       }, {
                                                                                                           "description": "set position",
                                                                                                             "interface": "set_state",
                                                                                                             "max_value": 1
                                                                                                       }, {
                                                                                                              "argument": "TOGGLE",
                                                                                                           "description": "Toggle switch state",
                                                                                                             "interface": "action"
                                                                                                       } ],
                                                                                "momentary_positions": "none",
                                                                                            "outputs": [ {
                                                                                                               "address": 8200,
                                                                                                           "description": "selector position",
                                                                                                                  "mask": 8,
                                                                                                             "max_value": 1,
                                                                                                              "shift_by": 3,
                                                                                                                "suffix": "",
                                                                                                                  "type": "integer"
                                                                                                       } ],
                                                                                   "physical_variant": "toggle_switch"
                                                                            },
                                                "FRONT_ICOM_STBY_DISTR_SW": {
                                                                                           "category": "SPU9",
                                                                                       "control_type": "selector",
                                                                                        "description": "Fore Intercom STBY Distributive Switch",
                                                                                         "identifier": "FRONT_ICOM_STBY_DISTR_SW",
                                                                                             "inputs": [ {
                                                                                                           "description": "switch to previous or next state",
                                                                                                             "interface": "fixed_step"
                                                                                                       }, {
                                                                                                           "description": "set position",
                                                                                                             "interface": "set_state",
                                                                                                             "max_value": 1
                                                                                                       }, {
                                                                                                              "argument": "TOGGLE",
                                                                                                           "description": "Toggle switch state",
                                                                                                             "interface": "action"
                                                                                                       } ],
                                                                                "momentary_positions": "none",
                                                                                            "outputs": [ {
                                                                                                               "address": 8200,
                                                                                                           "description": "selector position",
                                                                                                                  "mask": 4,
                                                                                                             "max_value": 1,
                                                                                                              "shift_by": 2,
                                                                                                                "suffix": "",
                                                                                                                  "type": "integer"
                                                                                                       } ],
                                                                                   "physical_variant": "toggle_switch"
                                                                            },
                                                          "FRONT_ICOM_VOL": {
                                                                                    "category": "SPU9",
                                                                                "control_type": "limited_dial",
                                                                                 "description": "Fore Intercom Volume Knob",
                                                                                  "identifier": "FRONT_ICOM_VOL",
                                                                                      "inputs": [ {
                                                                                                    "description": "set the position of the dial",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 65535
                                                                                                }, {
                                                                                                       "description": "turn the dial left or right",
                                                                                                         "interface": "variable_step",
                                                                                                         "max_value": 65535,
                                                                                                    "suggested_step": 3200
                                                                                                } ],
                                                                                     "outputs": [ {
                                                                                                        "address": 8206,
                                                                                                    "description": "position of the potentiometer",
                                                                                                           "mask": 65535,
                                                                                                      "max_value": 65535,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                         "FRONT_RADIO_VOL": {
                                                                                    "category": "SPU9",
                                                                                "control_type": "limited_dial",
                                                                                 "description": "Fore Radio Volume Knob",
                                                                                  "identifier": "FRONT_RADIO_VOL",
                                                                                      "inputs": [ {
                                                                                                    "description": "set the position of the dial",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 65535
                                                                                                }, {
                                                                                                       "description": "turn the dial left or right",
                                                                                                         "interface": "variable_step",
                                                                                                         "max_value": 65535,
                                                                                                    "suggested_step": 3200
                                                                                                } ],
                                                                                     "outputs": [ {
                                                                                                        "address": 8208,
                                                                                                    "description": "position of the potentiometer",
                                                                                                           "mask": 65535,
                                                                                                      "max_value": 65535,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                        "REAR_ICOM_RDF_SW": {
                                                                                           "category": "SPU9",
                                                                                       "control_type": "selector",
                                                                                        "description": "Rear Intercom RDF Switch",
                                                                                         "identifier": "REAR_ICOM_RDF_SW",
                                                                                             "inputs": [ {
                                                                                                           "description": "switch to previous or next state",
                                                                                                             "interface": "fixed_step"
                                                                                                       }, {
                                                                                                           "description": "set position",
                                                                                                             "interface": "set_state",
                                                                                                             "max_value": 1
                                                                                                       }, {
                                                                                                              "argument": "TOGGLE",
                                                                                                           "description": "Toggle switch state",
                                                                                                             "interface": "action"
                                                                                                       } ],
                                                                                "momentary_positions": "none",
                                                                                            "outputs": [ {
                                                                                                               "address": 8240,
                                                                                                           "description": "selector position",
                                                                                                                  "mask": 128,
                                                                                                             "max_value": 1,
                                                                                                              "shift_by": 7,
                                                                                                                "suffix": "",
                                                                                                                  "type": "integer"
                                                                                                       } ],
                                                                                   "physical_variant": "toggle_switch"
                                                                            },
                                                 "REAR_ICOM_STBY_DISTR_SW": {
                                                                                           "category": "SPU9",
                                                                                       "control_type": "selector",
                                                                                        "description": "Rear Intercom STBY Distributive Switch",
                                                                                         "identifier": "REAR_ICOM_STBY_DISTR_SW",
                                                                                             "inputs": [ {
                                                                                                           "description": "switch to previous or next state",
                                                                                                             "interface": "fixed_step"
                                                                                                       }, {
                                                                                                           "description": "set position",
                                                                                                             "interface": "set_state",
                                                                                                             "max_value": 1
                                                                                                       }, {
                                                                                                              "argument": "TOGGLE",
                                                                                                           "description": "Toggle switch state",
                                                                                                             "interface": "action"
                                                                                                       } ],
                                                                                "momentary_positions": "none",
                                                                                            "outputs": [ {
                                                                                                               "address": 8240,
                                                                                                           "description": "selector position",
                                                                                                                  "mask": 64,
                                                                                                             "max_value": 1,
                                                                                                              "shift_by": 6,
                                                                                                                "suffix": "",
                                                                                                                  "type": "integer"
                                                                                                       } ],
                                                                                   "physical_variant": "toggle_switch"
                                                                            },
                                                           "REAR_ICOM_VOL": {
                                                                                    "category": "SPU9",
                                                                                "control_type": "limited_dial",
                                                                                 "description": "Rear Intercom Volume Knob",
                                                                                  "identifier": "REAR_ICOM_VOL",
                                                                                      "inputs": [ {
                                                                                                    "description": "set the position of the dial",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 65535
                                                                                                }, {
                                                                                                       "description": "turn the dial left or right",
                                                                                                         "interface": "variable_step",
                                                                                                         "max_value": 65535,
                                                                                                    "suggested_step": 3200
                                                                                                } ],
                                                                                     "outputs": [ {
                                                                                                        "address": 8252,
                                                                                                    "description": "position of the potentiometer",
                                                                                                           "mask": 65535,
                                                                                                      "max_value": 65535,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            },
                                                          "REAR_RADIO_VOL": {
                                                                                    "category": "SPU9",
                                                                                "control_type": "limited_dial",
                                                                                 "description": "Rear Radio Volume Knob",
                                                                                  "identifier": "REAR_RADIO_VOL",
                                                                                      "inputs": [ {
                                                                                                    "description": "set the position of the dial",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 65535
                                                                                                }, {
                                                                                                       "description": "turn the dial left or right",
                                                                                                         "interface": "variable_step",
                                                                                                         "max_value": 65535,
                                                                                                    "suggested_step": 3200
                                                                                                } ],
                                                                                     "outputs": [ {
                                                                                                        "address": 8254,
                                                                                                    "description": "position of the potentiometer",
                                                                                                           "mask": 65535,
                                                                                                      "max_value": 65535,
                                                                                                       "shift_by": 0,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ]
                                                                            }
                                            },
                          "Starboard Wall": {
                                                "FRONT_EMER_VALVE": {
                                                                         "api_variant": "multiturn",
                                                                            "category": "Starboard Wall",
                                                                        "control_type": "analog_dial",
                                                                         "description": "Fore Pneumatic Emergency Valve 1",
                                                                          "identifier": "FRONT_EMER_VALVE",
                                                                              "inputs": [ {
                                                                                               "description": "turn the dial left or right",
                                                                                                 "interface": "variable_step",
                                                                                                 "max_value": 65535,
                                                                                            "suggested_step": 3200
                                                                                        } ],
                                                                             "outputs": [ {
                                                                                                "address": 8232,
                                                                                            "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                   "mask": 65535,
                                                                                              "max_value": 65535,
                                                                                               "shift_by": 0,
                                                                                                 "suffix": "_KNOB_POS",
                                                                                                   "type": "integer"
                                                                                        } ]
                                                                    },
                                                   "FRONT_MIXHEAT": {
                                                                                   "category": "Starboard Wall",
                                                                               "control_type": "selector",
                                                                                "description": "Fore Carburettor Heater Lever",
                                                                                 "identifier": "FRONT_MIXHEAT",
                                                                                     "inputs": [ {
                                                                                                   "description": "switch to previous or next state",
                                                                                                     "interface": "fixed_step"
                                                                                               }, {
                                                                                                   "description": "set position",
                                                                                                     "interface": "set_state",
                                                                                                     "max_value": 1
                                                                                               }, {
                                                                                                      "argument": "TOGGLE",
                                                                                                   "description": "Toggle switch state",
                                                                                                     "interface": "action"
                                                                                               } ],
                                                                        "momentary_positions": "none",
                                                                                    "outputs": [ {
                                                                                                       "address": 8224,
                                                                                                   "description": "selector position",
                                                                                                          "mask": 128,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 7,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ],
                                                                           "physical_variant": "toggle_switch"
                                                                    },
                                                 "REAR_EMER_VALVE": {
                                                                         "api_variant": "multiturn",
                                                                            "category": "Starboard Wall",
                                                                        "control_type": "analog_dial",
                                                                         "description": "Rear Pneumatic Emergency Valve 2",
                                                                          "identifier": "REAR_EMER_VALVE",
                                                                              "inputs": [ {
                                                                                               "description": "turn the dial left or right",
                                                                                                 "interface": "variable_step",
                                                                                                 "max_value": 65535,
                                                                                            "suggested_step": 3200
                                                                                        } ],
                                                                             "outputs": [ {
                                                                                                "address": 8262,
                                                                                            "description": "the rotation of the knob in the cockpit (not the value that is controlled by this knob!)",
                                                                                                   "mask": 65535,
                                                                                              "max_value": 65535,
                                                                                               "shift_by": 0,
                                                                                                 "suffix": "_KNOB_POS",
                                                                                                   "type": "integer"
                                                                                        } ]
                                                                    }
                                            },
                       "Throttle Quadrant": {
                                                 "FRONT_FRIC_LEVER": {
                                                                             "category": "Throttle Quadrant",
                                                                         "control_type": "limited_dial",
                                                                          "description": "Fore Left Frictioner Lever",
                                                                           "identifier": "FRONT_FRIC_LEVER",
                                                                               "inputs": [ {
                                                                                             "description": "set the position of the dial",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 65535
                                                                                         }, {
                                                                                                "description": "turn the dial left or right",
                                                                                                  "interface": "variable_step",
                                                                                                  "max_value": 65535,
                                                                                             "suggested_step": 3200
                                                                                         } ],
                                                                              "outputs": [ {
                                                                                                 "address": 8218,
                                                                                             "description": "position of the potentiometer",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                "FRONT_INTERCOM_TX": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "Throttle Quadrant",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore Intercom Button",
                                                                                  "identifier": "FRONT_INTERCOM_TX",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8200,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 8192,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 13,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     },
                                                 "FRONT_PROP_LEVER": {
                                                                             "category": "Throttle Quadrant",
                                                                         "control_type": "limited_dial",
                                                                          "description": "Fore Airscrew Lever",
                                                                           "identifier": "FRONT_PROP_LEVER",
                                                                               "inputs": [ {
                                                                                             "description": "set the position of the dial",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 65535
                                                                                         }, {
                                                                                                "description": "turn the dial left or right",
                                                                                                  "interface": "variable_step",
                                                                                                  "max_value": 65535,
                                                                                             "suggested_step": 3200
                                                                                         } ],
                                                                              "outputs": [ {
                                                                                                 "address": 8216,
                                                                                             "description": "position of the potentiometer",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                   "FRONT_RADIO_TX": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "Throttle Quadrant",
                                                                                "control_type": "selector",
                                                                                 "description": "Fore Radio Button",
                                                                                  "identifier": "FRONT_RADIO_TX",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8200,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 4096,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 12,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     },
                                                  "REAR_FRIC_LEVER": {
                                                                             "category": "Throttle Quadrant",
                                                                         "control_type": "limited_dial",
                                                                          "description": "Rear Left Frictioner Lever",
                                                                           "identifier": "REAR_FRIC_LEVER",
                                                                               "inputs": [ {
                                                                                             "description": "set the position of the dial",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 65535
                                                                                         }, {
                                                                                                "description": "turn the dial left or right",
                                                                                                  "interface": "variable_step",
                                                                                                  "max_value": 65535,
                                                                                             "suggested_step": 3200
                                                                                         } ],
                                                                              "outputs": [ {
                                                                                                 "address": 8258,
                                                                                             "description": "position of the potentiometer",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                 "REAR_INTERCOM_TX": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "Throttle Quadrant",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear Intercom Button",
                                                                                  "identifier": "REAR_INTERCOM_TX",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8240,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 8192,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 13,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     },
                                                  "REAR_PROP_LEVER": {
                                                                             "category": "Throttle Quadrant",
                                                                         "control_type": "limited_dial",
                                                                          "description": "Rear Airscrew Lever",
                                                                           "identifier": "REAR_PROP_LEVER",
                                                                               "inputs": [ {
                                                                                             "description": "set the position of the dial",
                                                                                               "interface": "set_state",
                                                                                               "max_value": 65535
                                                                                         }, {
                                                                                                "description": "turn the dial left or right",
                                                                                                  "interface": "variable_step",
                                                                                                  "max_value": 65535,
                                                                                             "suggested_step": 3200
                                                                                         } ],
                                                                              "outputs": [ {
                                                                                                 "address": 8256,
                                                                                             "description": "position of the potentiometer",
                                                                                                    "mask": 65535,
                                                                                               "max_value": 65535,
                                                                                                "shift_by": 0,
                                                                                                  "suffix": "",
                                                                                                    "type": "integer"
                                                                                         } ]
                                                                     },
                                                    "REAR_RADIO_TX": {
                                                                                 "api_variant": "momentary_last_position",
                                                                                    "category": "Throttle Quadrant",
                                                                                "control_type": "selector",
                                                                                 "description": "Rear Radio Button",
                                                                                  "identifier": "REAR_RADIO_TX",
                                                                                      "inputs": [ {
                                                                                                    "description": "switch to previous or next state",
                                                                                                      "interface": "fixed_step"
                                                                                                }, {
                                                                                                    "description": "set position",
                                                                                                      "interface": "set_state",
                                                                                                      "max_value": 1
                                                                                                }, {
                                                                                                       "argument": "TOGGLE",
                                                                                                    "description": "Toggle switch state",
                                                                                                      "interface": "action"
                                                                                                } ],
                                                                         "momentary_positions": "none",
                                                                                     "outputs": [ {
                                                                                                        "address": 8240,
                                                                                                    "description": "selector position",
                                                                                                           "mask": 4096,
                                                                                                      "max_value": 1,
                                                                                                       "shift_by": 12,
                                                                                                         "suffix": "",
                                                                                                           "type": "integer"
                                                                                                } ],
                                                                            "physical_variant": "push_button"
                                                                     }
                                            },
    "Warning, Caution and IndicatorLights": {
                                                     "F_ARC15_LIGHT": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front ARC-15 Signal Light (green)",
                                                                            "identifier": "F_ARC15_LIGHT",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8384,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 3,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                      "F_FLAPS_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Flaps DOWN Lamp (yellow)",
                                                                            "identifier": "F_FLAPS_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 256,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 8,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                        "F_FLAPS_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Flaps UP Lamp (green)",
                                                                            "identifier": "F_FLAPS_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 128,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 7,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "F_GEN_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Generator Fault Warning Lamp (red)",
                                                                            "identifier": "F_GEN_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16384,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 14,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                      "F_GYRO_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Gyro Compass Warning Lamp (yellow)",
                                                                            "identifier": "F_GYRO_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 1,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 0,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "F_L_GEAR_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Left Gear DOWN Lamp (green)",
                                                                            "identifier": "F_L_GEAR_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8264,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16384,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 14,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "F_L_GEAR_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Left Gear UP Lamp (red)",
                                                                            "identifier": "F_L_GEAR_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8264,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2048,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 11,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                      "F_MAXG_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Max G Warning Lamp (red)",
                                                                            "identifier": "F_MAXG_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 32768,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 15,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "F_METAL_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Metal Chips Warning Lamp (yellow)",
                                                                            "identifier": "F_METAL_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8192,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 13,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "F_N_GEAR_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Nose Gear DOWN Lamp (green)",
                                                                            "identifier": "F_N_GEAR_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8264,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 32768,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 15,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "F_N_GEAR_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Nose Gear UP Lamp (red)",
                                                                            "identifier": "F_N_GEAR_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8264,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4096,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 12,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                "F_PITOT_HEAT_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Pitot-Tube Heat Warning Lamp (green)",
                                                                            "identifier": "F_PITOT_HEAT_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 2,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "F_R_GEAR_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Right Gear DOWN Lamp (green)",
                                                                            "identifier": "F_R_GEAR_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 1,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 0,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "F_R_GEAR_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Right Gear UP Lamp (red)",
                                                                            "identifier": "F_R_GEAR_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8264,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8192,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 13,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "F_SPEED_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Danger Speed Warning Lamp (yellow)",
                                                                            "identifier": "F_SPEED_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4096,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 12,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                "F_STALL_HEAT_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Stall Heat Warning Lamp (green)",
                                                                            "identifier": "F_STALL_HEAT_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 1,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "F_STALL_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Front Stall Warning Lamp (red)",
                                                                            "identifier": "F_STALL_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2048,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 11,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_12_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 12L Warning Lamp (red)",
                                                                            "identifier": "L_FUEL_12_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 512,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 9,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_15_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 15L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_15_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 1024,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 10,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_20_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 20L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_20_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2048,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 11,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_25_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 25L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_25_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4096,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 12,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_30_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 30L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_30_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8192,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 13,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_35_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 35L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_35_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16384,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 14,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_40_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 40L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_40_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 32768,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 15,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_45_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 45L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_45_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8384,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 1,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 0,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_50_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 50L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_50_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8384,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 1,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "L_FUEL_60_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Left Fueltank 60L Warning Lamp (white)",
                                                                            "identifier": "L_FUEL_60_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8384,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 2,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_ARC15_LIGHT": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear ARC-15 Signal Light (green)",
                                                                            "identifier": "R_ARC15_LIGHT",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8384,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 4,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                      "R_BATT_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Battery ON Warning Lamp (green)",
                                                                            "identifier": "R_BATT_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 512,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 9,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_EMPTY_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Empty Warning Lamp (green)",
                                                                            "identifier": "R_EMPTY_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16384,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 14,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                      "R_FLAPS_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Flaps DOWN Lamp (yellow)",
                                                                            "identifier": "R_FLAPS_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 1024,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 10,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                        "R_FLAPS_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Flaps UP Lamp (green)",
                                                                            "identifier": "R_FLAPS_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 512,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 9,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_12_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 12L Warning Lamp (red)",
                                                                            "identifier": "R_FUEL_12_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 32768,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 15,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_15_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 15L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_15_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 1,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 0,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_20_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 20L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_20_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 1,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_25_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 25L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_25_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 2,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_30_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 30L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_30_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 3,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_35_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 35L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_35_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 4,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_40_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 40L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_40_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 32,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 5,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_45_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 45L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_45_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 64,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 6,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_50_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 50L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_50_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 128,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 7,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                   "R_FUEL_60_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Right Fueltank 60L Warning Lamp (white)",
                                                                            "identifier": "R_FUEL_60_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8382,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 256,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 8,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                    "R_FUEL_L_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Fuel 12L Left Warning Lamp (red)",
                                                                            "identifier": "R_FUEL_L_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 128,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 7,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                    "R_FUEL_R_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Fuel 12L Right Warning Lamp (red)",
                                                                            "identifier": "R_FUEL_R_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 256,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 8,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "R_GEN_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Generator Fault Warning Lamp (red)",
                                                                            "identifier": "R_GEN_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 64,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 6,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                      "R_GYRO_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Gyro Compass Warning Lamp (yellow)",
                                                                            "identifier": "R_GYRO_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 1024,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 10,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_L_GEAR_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Left Gear DOWN Lamp (green)",
                                                                            "identifier": "R_L_GEAR_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 4,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "R_L_GEAR_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Left Gear UP Lamp (red)",
                                                                            "identifier": "R_L_GEAR_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 1,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                      "R_MAXG_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Max G Warning Lamp (red)",
                                                                            "identifier": "R_MAXG_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 3,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_METAL_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Metal Chips Warning Lamp (yellow)",
                                                                            "identifier": "R_METAL_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 2048,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 11,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_N_GEAR_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Nose Gear DOWN Lamp (green)",
                                                                            "identifier": "R_N_GEAR_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 32,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 5,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "R_N_GEAR_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Nose Gear UP Lamp (red)",
                                                                            "identifier": "R_N_GEAR_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 2,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                "R_PITOT_HEAT_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Pitot-Tube Heat Warning Lamp (green)",
                                                                            "identifier": "R_PITOT_HEAT_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 4096,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 12,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_R_GEAR_DOWN": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Right Gear DOWN Lamp (green)",
                                                                            "identifier": "R_R_GEAR_DOWN",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 64,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 6,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                       "R_R_GEAR_UP": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Right Gear UP Lamp (red)",
                                                                            "identifier": "R_R_GEAR_UP",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8378,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 3,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_SPEED_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Danger Speed Warning Lamp (yellow)",
                                                                            "identifier": "R_SPEED_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 32,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 5,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                "R_STALL_HEAT_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Stall Heat Warning Lamp (green)",
                                                                            "identifier": "R_STALL_HEAT_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 8192,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 13,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      },
                                                     "R_STALL_WARNL": {
                                                                              "category": "Warning, Caution and IndicatorLights",
                                                                          "control_type": "led",
                                                                           "description": "Rear Stall Warning Lamp (red)",
                                                                            "identifier": "R_STALL_WARNL",
                                                                                "inputs": [  ],
                                                                               "outputs": [ {
                                                                                                  "address": 8380,
                                                                                              "description": "0 if light is off, 1 if light is on",
                                                                                                     "mask": 16,
                                                                                                "max_value": 1,
                                                                                                 "shift_by": 4,
                                                                                                   "suffix": "",
                                                                                                     "type": "integer"
                                                                                          } ]
                                                                      }
                                            }
};
