1966->[I] i
1970->[I] ret 0
1972->[I] ret 0
1972->[I] ret 0
1974->[E] I2C2 Slave addr 0x7C, task app display tas code 4
1976->[I] ret 0
1978->[I] ret 0
1978->[I] ret 0
1998->[I] i
app_start_thread wait nrf usb ready try_cnt:8.
2518->[E] I2C3 Slave addr 0x72, task app display tas code 1
2518->[E] retry cnt 1 ret 1
2529->[I] codec_suspend s:1 reset:1


2529->[I] state 1 => 5
2558->[I] codec_power spk:0 1788:1797


4402->[I] Codec init done cnt:1.
4402->[I] sync_codec_power_state s_o:0, s:3
4551->[I] cmd 86 opt 5 datalen 1
4551->[I] cmd 86 opt 5 datalen 1
4551->[I] etp_sts exp_fw:2
4555->[I] cmd 91 opt 5 datalen 2
4555->[I] ept_w_s write cmd:2 val:2

4557->[I] cmd 86 opt 5 datalen 4
4557->[I] cmd 86 opt 5 datalen 4
4558->[I] cmd 3 opt 6 datalen 0
4561->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


4561->[I] etp chip act_s:1 


4563->[I] etp chip ept_s:1 app_s:1


4563->[I] Panel off unlocked!!!
4565->[I] ept_r_ept expand:0 1 268442544
4571->[I] cmd 86 opt 5 datalen 4
4571->[I] cmd 86 opt 5 datalen 4
4572->[I] ept_r_ept expand:2 1 268442544
4833->[I] cmd 26 opt 5 datalen 10
4833->[I] eSpiCmdVideoCtrl cmd 1
4833->[I] video set work mode 0
4833->[I] eSpiCmdVideoCtrl cmd 1 return 1
4838->[I] cmd 26 opt 5 datalen 10
4838->[I] eSpiCmdVideoCtrl cmd 2
4838->[I] open video prepare
4838->[I] requiredFps 90
4838->[I] set upscale mode: 1
4841->[I] dsc mode not match
4845->[I] eSpiCmdVideoCtrl cmd 2 return 2
4850->[I] cmd 26 opt 5 datalen 10
4850->[I] eSpiCmdVideoCtrl cmd 3
4850->[I] video reset
4850->[I] eSpiCmdVideoCtrl cmd 3 return 1
4928->[I] i
4931->[I] i
5256->[I] cmd 86 opt 5 datalen 1
5256->[I] cmd 86 opt 5 datalen 1
5259->[I] cmd 86 opt 5 datalen 1
5259->[I] cmd 86 opt 5 datalen 1
5262->[I] cmd 86 opt 5 datalen 1
5262->[I] cmd 86 opt 5 datalen 1
5262->[I] etp_sts ept_s:1


5268->[I] cmd 10 opt 5 datalen 4
5268->[I] cmd 10 opt 5 datalen 4
5273->[I] ept_vef_sig in scr_len:35 key_id:1

5295->[I] cmd 10 opt 5 datalen 4
5295->[I] cmd 10 opt 5 datalen 4
5306->[I] cmd 10 opt 5 datalen 4
5306->[I] cmd 10 opt 5 datalen 4
5318->[I] cmd 10 opt 5 datalen 4
5318->[I] cmd 10 opt 5 datalen 4
5329->[I] cmd 10 opt 5 datalen 4
5329->[I] cmd 10 opt 5 datalen 4
5340->[I] cmd 10 opt 5 datalen 4
5340->[I] cmd 10 opt 5 datalen 4
5347->[I] requiredFps 0
5347->[I] codec_i2s connect reset_flag:1


5351->[I] cmd 10 opt 5 datalen 4
5351->[I] cmd 10 opt 5 datalen 4
5362->[I] cmd 10 opt 5 datalen 4
5362->[I] cmd 10 opt 5 datalen 4
5373->[I] cmd 10 opt 5 datalen 4
5373->[I] cmd 10 opt 5 datalen 4
5386->[I] cmd 10 opt 5 datalen 4
5386->[I] cmd 10 opt 5 datalen 4
5395->[I] cmd 86 opt 5 datalen 1
5395->[I] cmd 86 opt 5 datalen 1
5395->[I] etp_sts exp_fw:2
5399->[I] cmd 91 opt 5 datalen 2
5399->[I] ept_w_s write cmd:2 val:2

5402->[I] cmd 91 opt 5 datalen 3
5402->[I] ept_w_s write cmd:2 val:2

5405->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


5405->[I] etp chip act_s:1 


5407->[I] cmd 86 opt 5 datalen 4
5407->[I] cmd 86 opt 5 datalen 4
5407->[I] etp chip ept_s:1 app_s:1


5413->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


5413->[I] etp chip act_s:1 


5415->[I] etp chip ept_s:1 app_s:1


5417->[I] ept_r_ept expand:0 32 268442544
5502->[E] codec_reset_flag wait:3
5502->[I] sync_codec_power_state s_o:3, s:2
5502->[I] codec_vol val:0 vol_bk:170 force:1 p_s:1


5502->[I] codec_power s:1 bk_s:2
5502->[E] codec_off flag:0
5502->[I] codec_vol val:0 vol_bk:170 force:1 p_s:1


7430->[I] i
7434->[I] ret 0
7436->[I] ret 0
7436->[I] ret 0
7438->[I] ret 0
7440->[I] ret 0
7440->[I] ret 0
7460->[I] i
7990->[I] dsc mode not match
7994->[I] hard reset
8332->[I] cmd 26 opt 5 datalen 10
8332->[I] eSpiCmdVideoCtrl cmd 1
8332->[I] video set work mode 0
8332->[I] eSpiCmdVideoCtrl cmd 1 return 1
8337->[I] cmd 26 opt 5 datalen 10
8337->[I] eSpiCmdVideoCtrl cmd 2
8337->[I] open video prepare
8337->[I] requiredFps 90
8337->[I] keep upscale mode: 1
8337->[I] eSpiCmdVideoCtrl cmd 2 return 1
8368->[I] requiredFps 0
8384->[I] requiredFps 90
8429->[I] cmd 26 opt 5 datalen 10
8429->[I] eSpiCmdVideoCtrl cmd 2
8429->[I] open video prepare
8429->[I] keep upscale mode: 1
8429->[I] eSpiCmdVideoCtrl cmd 2 return 1
9476->[I] cmd 26 opt 5 datalen 10
9476->[I] eSpiCmdVideoCtrl cmd 2
9476->[I] open video prepare
9476->[I] keep upscale mode: 1
9476->[I] eSpiCmdVideoCtrl cmd 2 return 1
10497->[I] cmd 26 opt 5 datalen 10
10497->[I] eSpiCmdVideoCtrl c