112379->[I] cmd 86 opt 5 datalen 1
112379->[I] cmd 86 opt 5 datalen 1
112379->[I] etp_sts exp_fw:2
112383->[I] cmd 91 opt 5 datalen 2
112383->[I] ept_w_s write cmd:2 val:2

112385->[I] cmd 86 opt 5 datalen 4
112385->[I] cmd 86 opt 5 datalen 4
112385->[I] cmd 3 opt 6 datalen 0
112390->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


112390->[I] etp chip act_s:1 


112392->[I] etp chip ept_s:1 app_s:1


112394->[I] ept_r_ept expand:0 1 268442544
112399->[I] cmd 86 opt 5 datalen 4
112399->[I] cmd 86 opt 5 datalen 4
112401->[I] ept_r_ept expand:2 1 268442544
112483->[I] i
112487->[I] ret 0
112489->[I] ret 0
112489->[I] ret 0
112491->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112493->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112495->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112497->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112499->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112501->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112503->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112505->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112507->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112509->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112511->[I] ret 1
112513->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112515->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112517->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112519->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112521->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112523->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112525->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112527->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112529->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112531->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112533->[I] ret 1
112533->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112535->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112537->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112539->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112541->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112543->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112545->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112547->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112549->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112551->[E] I2C2 Slave addr 0x7C, task app display tas code 4
112553->[I] ret 1
112573->[I] i
113104->[I] codec_suspend s:1 reset:0


113104->[I] sync_codec_power_state s_o:1, s:1
113104->[I] codec_power s:1 bk_s:1
113104->[E] codec_off flag:1
113104->[I] state 1 => 5
113199->[I] cmd 86 opt 5 datalen 1
113199->[I] cmd 86 opt 5 datalen 1
113202->[I] cmd 86 opt 5 datalen 1
113202->[I] cmd 86 opt 5 datalen 1
113204->[I] cmd 86 opt 5 datalen 1
113204->[I] cmd 86 opt 5 datalen 1
113204->[I] etp_sts ept_s:1


113212->[I] cmd 10 opt 5 datalen 4
113212->[I] cmd 10 opt 5 datalen 4
113218->[I] ept_vef_sig in scr_len:35 key_id:1

113239->[I] cmd 10 opt 5 datalen 4
113239->[I] cmd 10 opt 5 datalen 4
113252->[I] cmd 10 opt 5 datalen 4
113252->[I] cmd 10 opt 5 datalen 4
113264->[I] cmd 10 opt 5 datalen 4
113265->[I] cmd 10 opt 5 datalen 4
113277->[I] cmd 10 opt 5 datalen 4
113277->[I] cmd 10 opt 5 datalen 4
113289->[I] cmd 10 opt 5 datalen 4
113289->[I] cmd 10 opt 5 datalen 4
113302->[I] cmd 10 opt 5 datalen 4
113302->[I] cmd 10 opt 5 datalen 4
113314->[I] cmd 10 opt 5 datalen 4
113314->[I] cmd 10 opt 5 datalen 4
113326->[I] cmd 10 opt 5 datalen 4
113326->[I] cmd 10 opt 5 datalen 4
113338->[I] cmd 10 opt 5 datalen 4
113338->[I] cmd 10 opt 5 datalen 4
113348->[I] cmd 86 opt 5 datalen 1
113348->[I] cmd 86 opt 5 datalen 1
113348->[I] etp_sts exp_fw:2
113352->[I] cmd 91 opt 5 datalen 2
113352->[I] ept_w_s write cmd:2 val:2

113354->[I] cmd 91 opt 5 datalen 3
113354->[I] ept_w_s write cmd:2 val:2

113358->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


113358->[I] etp chip act_s:1 


113360->[I] etp chip ept_s:1 app_s:1


113360->[I] cmd 86 opt 5 datalen 4
113360->[I] cmd 86 opt 5 datalen 4
113366->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


113366->[I] etp chip act_s:1 


113368->[I] etp chip ept_s:1 app_s:1


113371->[I] ept_r_ept expand:0 32 268442544
113434->[I] cmd 26 opt 5 datalen 10
113434->[I] eSpiCmdVideoCtrl cmd 1
113434->[I] video set work mode 0
113434->[I] eSpiCmdVideoCtrl cmd 1 return 1
113440->[I] cmd 26 opt 5 datalen 10
113440->[I] eSpiCmdVideoCtrl cmd 2
113440->[I] open video prepare
113440->[I] requiredFps 90
113440->[I] set upscale mode: 1
113443->[I] dsc mode not match
113447->[I] eSpiCmdVideoCtrl cmd 2 return 2
113452->[I] cmd 26 opt 5 datalen 10
113452->[I] eSpiCmdVideoCtrl cmd 3
113452->[I] video reset
113452->[I] eSpiCmdVideoCtrl cmd 3 return 1
113503->[I] i
113506->[I] i
113979->[I] requiredFps 0
116005->[I] i
116009->[I] ret 0
116011->[I] ret 0
116011->[I] ret 0
116013->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116015->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116017->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116019->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116021->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116023->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116025->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116027->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116029->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116031->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116033->[I] ret 1
116035->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116037->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116039->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116041->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116043->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116045->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116047->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116049->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116051->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116053->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116055->[I] ret 1
116055->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116057->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116059->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116061->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116063->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116065->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116067->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116069->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116071->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116073->[E] I2C2 Slave addr 0x7C, task app display tas code 4
116075->[I] ret 1
116095->[I] i
116626->[I] dsc mode not match
116629->[I] hard reset
116955->[I] cmd 26 opt 5 datalen 10
116955->[I] eSpiCmdVideoCtrl cmd 1
116955->[I] video set work mode 0
116955->[I] eSpiCmdVideoCtrl cmd 1 return 1
116960->[I] cmd 26 opt 5 datalen 10
116960->[I] eSpiCmdVideoCtrl cmd 2
116960->[I] open video prepare
116960->[I] requiredFps 90
116960->[I] keep upscale mode: 1
116960->[I] eSpiCmdVideoCtrl cmd 2 return 1
117000->[I] requiredFps 0
117112->[I] requiredFps 90
117870->[I] cmd 86 opt 5 datalen 1
117870->[I] cmd 86 opt 5 datalen 1
117877->[I] cmd 86 opt 5 datalen 1
117877->[I] cmd 86 opt 5 datalen 1
117894->[I] cmd 10 opt 5 datalen 4
117896->[I] cmd 10 opt 5 datalen 4
117902->[I] ept_vef_sig in scr_len:35 key_id:1

117926->[I] cmd 10 opt 5 datalen 4
117926->[I] cmd 10 opt 5 datalen 4
117940->[I] cmd 10 opt 5 datalen 4
117941->[I] cmd 10 opt 5 datalen 4
117953->[I] cmd 10 opt 5 datalen 4
117953->[I] cmd 10 opt 5 datalen 4
117965->[I] cmd 10 opt 5 datalen 4
117965->[I] cmd 10 opt 5 datalen 4
117978->[I] cmd 10 opt 5 datalen 4
117978->[I] cmd 10 opt 5 datalen 4
117988->[I] cmd 86 opt 5 datalen 4
117989->[I] cmd 86 opt 5 datalen 4
117991->[I] cmd 10 opt 5 datalen 4
117991->[I] ept_r_ept expand:0 1 268442544
117991->[I] cmd 10 opt 5 datalen 4
117997->[I] cmd 86 opt 5 datalen 4
117997->[I] cmd 86 opt 5 datalen 4
118000->[I] ept_r_ept expand:2 1 268442544
118005->[I] cmd 10 opt 5 datalen 4
118005->[I] cmd 10 opt 5 datalen 4
118018->[I] cmd 10 opt 5 datalen 4
118018->[I] cmd 10 opt 5 datalen 4
118031->[I] cmd 10 opt 5 datalen 4
118031->[I] cmd 10 opt 5 datalen 4
118041->[I] cmd 86 opt 5 datalen 1
118041->[I] cmd 86 opt 5 datalen 1
118041->[I] etp_sts exp_fw:2
118046->[I] cmd 91 opt 5 datalen 2
118046->[I] ept_w_s write cmd:2 val:2

118049->[I] cmd 91 opt 5 datalen 3
118049->[I] ept_w_s write cmd:2 val:2

118052->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


118052->[I] etp chip act_s:1 


118053->[I] cmd 86 opt 5 datalen 4
118053->[I] cmd 86 opt 5 datalen 4
118054->[I] etp chip ept_s:1 app_s:1


118060->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


118060->[I] etp chip act_s:1 


118062->[I] etp chip ept_s:1 app_s:1


118065->[I] ept_r_ept expand:0 32 268442544
118333->[I] calc fps 0 => 90
119881->[I] cmd 86 opt 5 datalen 1
119881->[I] cmd 86 opt 5 datalen 1
119884->[I] cmd 86 opt 5 datalen 1
119885->[I] cmd 86 opt 5 datalen 1
119888->[I] cmd 86 opt 5 datalen 1
119888->[I] cmd 86 opt 5 datalen 1
119888->[I] etp_sts ept_s:1


119893->[I] cmd 86 opt 5 datalen 1
119894->[I] cmd 86 opt 5 datalen 1
119906->[I] cmd 10 opt 5 datalen 4
119907->[I] cmd 10 opt 5 datalen 4
119913->[I] ept_vef_sig in scr_len:35 key_id:1

119935->[I] cmd 10 opt 5 datalen 4
119935->[I] cmd 10 opt 5 datalen 4
119947->[I] cmd 10 opt 5 datalen 4
119947->[I] cmd 10 opt 5 datalen 4
119960->[I] cmd 10 opt 5 datalen 4
119962->[I] cmd 10 opt 5 datalen 4
119974->[I] cmd 10 opt 5 datalen 4
119974->[I] cmd 10 opt 5 datalen 4
119987->[I] cmd 10 opt 5 datalen 4
119989->[I] cmd 10 opt 5 datalen 4
120001->[I] cmd 10 opt 5 datalen 4
120001->[I] cmd 10 opt 5 datalen 4
120013->[I] cmd 10 opt 5 datalen 4
120013->[I] cmd 10 opt 5 datalen 4
120025->[I] cmd 10 opt 5 datalen 4
120025->[I] cmd 10 opt 5 datalen 4
120038->[I] cmd 10 opt 5 datalen 4
120040->[I] cmd 10 opt 5 datalen 4
120050->[I] cmd 86 opt 5 datalen 1
120051->[I] cmd 86 opt 5 datalen 1
120051->[I] etp_sts exp_fw:2
120055->[I] cmd 91 opt 5 datalen 2
120055->[I] ept_w_s write cmd:2 val:2

120057->[I] cmd 91 opt 5 datalen 3
120057->[I] ept_w_s write cmd:2 val:2

120061->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


120061->[I] etp chip act_s:1 


120062->[I] cmd 86 opt 5 datalen 4
120063->[I] etp chip ept_s:1 app_s:1


120064->[I] cmd 86 opt 5 datalen 4
120069->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


120069->[I] etp chip act_s:1 


120071->[I] etp chip ept_s:1 app_s:1


120075->[I] ept_r_ept expand:0 32 268442544
121897->[I] cmd 86 opt 5 datalen 1
121897->[I] cmd 86 opt 5 datalen 1
121899->[I] cmd 86 opt 5 datalen 1
121899->[I] cmd 86 opt 5 datalen 1
121899->[I] etp_sts ept_s:1


121904->[I] cmd 86 opt 5 datalen 1
121904->[I] cmd 86 opt 5 datalen 1
121904->[I] etp_sts exp_fw:2
121908->[I] cmd 91 opt 5 datalen 2
121908->[I] ept_w_s write cmd:2 val:2

121911->[I] cmd 91 opt 5 datalen 3
121911->[I] ept_w_s write cmd:2 val:2

121914->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


121914->[I] etp chip act_s:1 


121915->[I] cmd 86 opt 5 datalen 4
121916->[I] cmd 86 opt 5 datalen 4
121916->[I] etp chip ept_s:1 app_s:1


121922->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


121922->[I] etp chip act_s:1 


121924->[I] etp chip ept_s:1 app_s:1


121927->[I] ept_r_ept expand:0 32 268442544
122277->[I] i
122307->[I] i
122312->[I] boe_localdimming_on

122511->[I] Panel: 0
122512->[I] Panel: 1
122517->[I] Panel: 0 ok!

122517->[I] BOE_DataInit B2 4,
122517->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
122518->[I] Panel: 1 ok!

122518->[I] BOE_DataInit B2 4,
122518->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
122531->[I] codec_suspend s:1 reset:0


122531->[I] sync_codec_power_state s_o:1, s:1
122531->[I] codec_power s:1 bk_s:1
122531->[E] codec_off flag:1
122531->[I] video stable
122531->[I] state 5 => 7
122531->[I] rx0 0x08E00960 Htotal=2400, Vtotal=2272
122532->[I] rx1 0x08E00960 Htotal=2400, Vtotal=2272
122532->[I] dp_rx_timming_check Ok
122621->[W] pps OK.
122621->[I] codec_resume s:1 reset:0


122621->[I] codec_power s:2 bk_s:1
122621->[E] codec_on flag:1
122630->[I] state 7 => 8
122630->[I] Panel ON
124530->[E] I2C3 Slave addr 0x72, task app display tas code 1
124530->[E] retry cnt 1 ret 1
124531->[E] I2C3 Slave addr 0x72, task app display tas code 4
124531->[E] retry cnt 2 ret 1
125707->[I] Codec init done cnt:1.
125707->[E] codec_reset_flag wait:0
125707->[I] sync_codec_power_state s_o:1, s:2
125707->[I] codec_vol val:2 vol_bk:170 force:1 p_s:2


125707->[I] codec_unmute codec_s:1


125710->[I] codec_vol_mute 1


125710->[I] vol_ctl vol_bk:168 s:1


