41340->[I] cmd 86 opt 5 datalen 1
41340->[I] cmd 86 opt 5 datalen 1
41340->[I] etp_sts exp_fw:2
41344->[I] cmd 91 opt 5 datalen 2
41344->[I] ept_w_s write cmd:2 val:2

41346->[I] cmd 86 opt 5 datalen 4
41346->[I] cmd 86 opt 5 datalen 4
41346->[I] cmd 3 opt 6 datalen 0
41351->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


41351->[I] etp chip act_s:1 


41353->[I] etp chip ept_s:1 app_s:1


41355->[I] ept_r_ept expand:0 1 268442544
41359->[I] cmd 86 opt 5 datalen 4
41360->[I] cmd 86 opt 5 datalen 4
41361->[I] ept_r_ept expand:2 1 268442544
41418->[I] requiredFps 0
41514->[I] i
41518->[I] ret 0
41520->[I] ret 0
41520->[I] ret 0
41522->[I] ret 0
41524->[I] ret 0
41524->[I] ret 0
41544->[I] i
42074->[I] dsc mode not match
42078->[I] codec_suspend s:1 reset:0


42078->[I] sync_codec_power_state s_o:1, s:1
42078->[I] codec_power s:1 bk_s:1
42078->[E] codec_off flag:1
42078->[I] state 1 => 5
42370->[I] cmd 86 opt 5 datalen 1
42370->[I] cmd 86 opt 5 datalen 1
42372->[I] cmd 86 opt 5 datalen 1
42372->[I] cmd 86 opt 5 datalen 1
42374->[I] cmd 86 opt 5 datalen 1
42374->[I] cmd 86 opt 5 datalen 1
42374->[I] etp_sts ept_s:1


42381->[I] cmd 10 opt 5 datalen 4
42381->[I] cmd 10 opt 5 datalen 4
42387->[I] ept_vef_sig in scr_len:35 key_id:1

42403->[I] cmd 26 opt 5 datalen 10
42403->[I] eSpiCmdVideoCtrl cmd 1
42403->[I] video set work mode 0
42403->[I] eSpiCmdVideoCtrl cmd 1 return 1
42408->[I] cmd 26 opt 5 datalen 10
42408->[I] eSpiCmdVideoCtrl cmd 2
42408->[I] open video prepare
42408->[I] requiredFps 90
42408->[I] keep upscale mode: 1
42408->[I] eSpiCmdVideoCtrl cmd 2 return 1
42409->[I] cmd 10 opt 5 datalen 4
42409->[I] cmd 10 opt 5 datalen 4
42422->[I] cmd 10 opt 5 datalen 4
42422->[I] cmd 10 opt 5 datalen 4
42435->[I] cmd 10 opt 5 datalen 4
42435->[I] cmd 10 opt 5 datalen 4
42447->[I] cmd 10 opt 5 datalen 4
42447->[I] cmd 10 opt 5 datalen 4
42459->[I] cmd 10 opt 5 datalen 4
42459->[I] cmd 10 opt 5 datalen 4
42471->[I] cmd 10 opt 5 datalen 4
42471->[I] cmd 10 opt 5 datalen 4
42484->[I] cmd 10 opt 5 datalen 4
42484->[I] cmd 10 opt 5 datalen 4
42496->[I] cmd 10 opt 5 datalen 4
42497->[I] cmd 10 opt 5 datalen 4
42509->[I] cmd 10 opt 5 datalen 4
42509->[I] cmd 10 opt 5 datalen 4
42518->[I] cmd 86 opt 5 datalen 1
42518->[I] cmd 86 opt 5 datalen 1
42518->[I] etp_sts exp_fw:2
42522->[I] cmd 91 opt 5 datalen 2
42522->[I] ept_w_s write cmd:2 val:2

42525->[I] cmd 91 opt 5 datalen 3
42525->[I] ept_w_s write cmd:2 val:2

42528->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


42528->[I] etp chip act_s:1 


42530->[I] cmd 86 opt 5 datalen 4
42530->[I] cmd 86 opt 5 datalen 4
42530->[I] etp chip ept_s:1 app_s:1


42536->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


42536->[I] etp chip act_s:1 


42538->[I] etp chip ept_s:1 app_s:1


42540->[I] ept_r_ept expand:0 32 268442544
42560->[I] cmd 26 opt 5 datalen 10
42560->[I] eSpiCmdVideoCtrl cmd 2
42560->[I] open video prepare
42560->[I] keep upscale mode: 1
42560->[I] eSpiCmdVideoCtrl cmd 2 return 1
43576->[I] cmd 26 opt 5 datalen 10
43576->[I] eSpiCmdVideoCtrl cmd 2
43576->[I] open video prepare
43576->[I] keep upscale mode: 1
43576->[I] eSpiCmdVideoCtrl cmd 2 return 1
44592->[I] cmd 26 opt 5 datalen 10
44592->[I] eSpiCmdVideoCtrl cmd 2
44592->[I] open video prepare
44592->[I] keep upscale mode: 1
44592->[I] eSpiCmdVideoCtrl cmd 2 return 1
45607->[I] cmd 26 opt 5 datalen 10
45607->[I] eSpiCmdVideoCtrl cmd 2
45607->[I] open video prepare
45607->[I] keep upscale mode: 1
45607->[I] eSpiCmdVideoCtrl cmd 2 return 1
57604->[I] cmd 26 opt 5 datalen 10
57604->[I] eSpiCmdVideoCtrl cmd 3
57604->[I] video reset
57604->[I] eSpiCmdVideoCtrl cmd 3 return 1
57678->[I] i
57681->[I] i
60180->[I] i
60184->[I] ret 0
60186->[I] ret 0
60186->[I] ret 0
60188->[I] ret 0
60190->[I] ret 0
60190->[I] ret 0
60210->[I] i
60740->[I] dsc mode not match
60744->[I] hard reset
61080->[I] cmd 26 opt 5 datalen 10
61081->[I] eSpiCmdVideoCtrl cmd 1
61081->[I] video set work mode 0
61081->[I] eSpiCmdVideoCtrl cmd 1 return 1
61085->[I] cmd 26 opt 5 datalen 10
61085->[I] eSpiCmdVideoCtrl cmd 2
61085->[I] open video prepare
61085->[I] keep upscale mode: 1
61085->[I] eSpiCmdVideoCtrl cmd 2 return 1
61179->[I] cmd 26 opt 5 datalen 10
61179->[I] eSpiCmdVideoCtrl cmd 2
61179->[I] open video prepare
61179->[I] keep upscale mode: 1
61179->[I] eSpiCmdVideoCtrl cmd 2 return 1
62193->[I] cmd 26 opt 5 datalen 10
62193->[I] eSpiCmdVideoCtrl cmd 2
62193->[I] open video prepare
62193->[I] keep upscale mode: 1
62193->[I] eSpiCmdVideoCtrl cmd 2 return 1
63215->[I] cmd 26 opt 5 datalen 10
63215->[I] eSpiCmdVideoCtrl cmd 2
63215->[I] open video prepare
63215->[I] keep upscale mode: 1
63215->[I] eSpiCmdVideoCtrl cmd 2 return 1
64236->[I] cmd 26 opt 5 datalen 10
64236->[I] eSpiCmdVideoCtrl cmd 2
64236->[I] open video prepare
64236->[I] keep upscale mode: 1
64236->[I] eSpiCmdVideoCtrl cmd 2 return 1
76233->[I] cmd 26 opt 5 datalen 10
76233->[I] eSpiCmdVideoCtrl cmd 3
76233->[I] video reset
76233->[I] eSpiCmdVideoCtrl cmd 3 return 1
76244->[I] i
76247->[I] i
78746->[I] i
78750->[I] ret 0
78752->[I] ret 0
78752->[I] ret 0
78754->[E] I2C2 Slave addr 0x7C, task app display tas code 4
78756->[I] ret 0
78758->[I] ret 0
78758->[I] ret 0
78778->[I] i
79308->[I] dsc mode not match
79312->[I] hard reset
79635->[I] cmd 26 opt 5 datalen 10
79635->[I] eSpiCmdVideoCtrl cmd 1
79635->[I] video set work mode 0
79635->[I] eSpiCmdVideoCtrl cmd 1 return 1
79640->[I] cmd 26 opt 5 datalen 10
79640->[I] eSpiCmdVideoCtrl cmd 2
79640->[I] open video prepare
79640->[I] keep upscale mode: 1
79640->[I] eSpiCmdVideoCtrl cmd 2 return 1
79696->[I] cmd 26 opt 5 datalen 10
79696->[I] eSpiCmdVideoCtrl cmd 2
79696->[I] open video prepare
79696->[I] keep upscale mode: 1
79696->[I] eSpiCmdVideoCtrl cmd 2 return 1
80711->[I] cmd 26 opt 5 datalen 10
80711->[I] eSpiCmdVideoCtrl cmd 2
80711->[I] open video prepare
80711->[I] keep upscale mode: 1
80711->[I] eSpiCmdVideoCtrl cmd 2 return 1
81726->[I] cmd 26 opt 5 datalen 10
81726->[I] eSpiCmdVideoCtrl c