33489->[I] cmd 86 opt 5 datalen 1
33489->[I] cmd 86 opt 5 datalen 1
33489->[I] etp_sts exp_fw:2
33493->[I] cmd 91 opt 5 datalen 2
33493->[I] ept_w_s write cmd:2 val:2

33494->[I] cmd 86 opt 5 datalen 4
33494->[I] cmd 86 opt 5 datalen 4
33495->[I] cmd 3 opt 6 datalen 0
33499->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


33499->[I] etp chip act_s:1 


33501->[I] etp chip ept_s:1 app_s:1


33501->[I] Panel off unlocked!!!
33503->[I] ept_r_ept expand:0 1 268442544
33508->[I] cmd 86 opt 5 datalen 4
33508->[I] cmd 86 opt 5 datalen 4
33510->[I] ept_r_ept expand:2 1 268442544
33586->[I] i
33590->[I] ret 0
33592->[I] ret 0
33592->[I] ret 0
33594->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33596->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33598->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33600->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33602->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33604->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33606->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33608->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33610->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33612->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33614->[I] ret 1
33616->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33618->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33620->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33622->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33624->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33626->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33628->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33630->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33632->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33634->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33636->[I] ret 1
33636->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33638->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33640->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33642->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33644->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33646->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33648->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33650->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33652->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33654->[E] I2C2 Slave addr 0x7C, task app display tas code 4
33656->[I] ret 1
33676->[I] i
34207->[I] codec_suspend s:1 reset:0


34207->[I] sync_codec_power_state s_o:2, s:1
34207->[I] codec_power s:1 bk_s:1
34207->[E] codec_off flag:1
34207->[I] state 1 => 5
36116->[I] cmd 3 opt 6 datalen 0
37115->[I] cmd 86 opt 5 datalen 1
37115->[I] cmd 86 opt 5 datalen 1
37118->[I] cmd 86 opt 5 datalen 1
37118->[I] cmd 86 opt 5 datalen 1
37120->[I] cmd 86 opt 5 datalen 1
37120->[I] cmd 86 opt 5 datalen 1
37120->[I] etp_sts ept_s:1


37126->[I] cmd 10 opt 5 datalen 4
37126->[I] cmd 10 opt 5 datalen 4
37132->[I] ept_vef_sig in scr_len:35 key_id:1

37154->[I] cmd 10 opt 5 datalen 4
37154->[I] cmd 10 opt 5 datalen 4
37166->[I] cmd 10 opt 5 datalen 4
37166->[I] cmd 10 opt 5 datalen 4
37179->[I] cmd 10 opt 5 datalen 4
37179->[I] cmd 10 opt 5 datalen 4
37191->[I] cmd 10 opt 5 datalen 4
37191->[I] cmd 10 opt 5 datalen 4
37203->[I] cmd 10 opt 5 datalen 4
37203->[I] cmd 10 opt 5 datalen 4
37216->[I] cmd 10 opt 5 datalen 4
37216->[I] cmd 10 opt 5 datalen 4
37229->[I] cmd 10 opt 5 datalen 4
37229->[I] cmd 10 opt 5 datalen 4
37242->[I] cmd 10 opt 5 datalen 4
37242->[I] cmd 10 opt 5 datalen 4
37254->[I] cmd 10 opt 5 datalen 4
37254->[I] cmd 10 opt 5 datalen 4
37265->[I] cmd 86 opt 5 datalen 1
37265->[I] cmd 86 opt 5 datalen 1
37265->[I] etp_sts exp_fw:2
37269->[I] cmd 91 opt 5 datalen 2
37269->[I] ept_w_s write cmd:2 val:2

37271->[I] cmd 91 opt 5 datalen 3
37271->[I] ept_w_s write cmd:2 val:2

37274->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


37274->[I] etp chip act_s:1 


37276->[I] cmd 86 opt 5 datalen 4
37276->[I] cmd 86 opt 5 datalen 4
37276->[I] etp chip ept_s:1 app_s:1


37282->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


37282->[I] etp chip act_s:1 


37284->[I] etp chip ept_s:1 app_s:1


37287->[I] ept_r_ept expand:0 32 268442544
94680->[I] i
94683->[I] No video input, power off panel!!!!
