51427->[I] cmd 86 opt 5 datalen 1
51427->[I] cmd 86 opt 5 datalen 1
51427->[I] etp_sts exp_fw:2
51431->[I] cmd 91 opt 5 datalen 2
51431->[I] ept_w_s write cmd:2 val:2

51433->[I] cmd 86 opt 5 datalen 4
51433->[I] cmd 86 opt 5 datalen 4
51433->[I] cmd 3 opt 6 datalen 0
51438->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


51438->[I] etp chip act_s:1 


51440->[I] etp chip ept_s:1 app_s:1


51442->[I] ept_r_ept expand:0 1 268442544
51447->[I] cmd 86 opt 5 datalen 4
51448->[I] cmd 86 opt 5 datalen 4
51449->[I] ept_r_ept expand:2 1 268442544
51496->[I] requiredFps 0
51578->[I] i
51582->[I] ret 0
51584->[I] ret 0
51584->[I] ret 0
51586->[E] I2C2 Slave addr 0x7C, task app display tas code 4
51588->[I] ret 0
51590->[I] ret 0
51590->[I] ret 0
51610->[I] i
52026->[I] cmd 86 opt 5 datalen 1
52026->[I] cmd 86 opt 5 datalen 1
52029->[I] cmd 86 opt 5 datalen 1
52029->[I] cmd 86 opt 5 datalen 1
52030->[I] cmd 86 opt 5 datalen 1
52030->[I] cmd 86 opt 5 datalen 1
52030->[I] etp_sts ept_s:1


52037->[I] cmd 10 opt 5 datalen 4
52037->[I] cmd 10 opt 5 datalen 4
52043->[I] ept_vef_sig in scr_len:35 key_id:1

52064->[I] cmd 10 opt 5 datalen 4
52064->[I] cmd 10 opt 5 datalen 4
52075->[I] cmd 10 opt 5 datalen 4
52075->[I] cmd 10 opt 5 datalen 4
52086->[I] cmd 10 opt 5 datalen 4
52086->[I] cmd 10 opt 5 datalen 4
52097->[I] cmd 10 opt 5 datalen 4
52097->[I] cmd 10 opt 5 datalen 4
52108->[I] cmd 10 opt 5 datalen 4
52108->[I] cmd 10 opt 5 datalen 4
52120->[I] cmd 10 opt 5 datalen 4
52120->[I] cmd 10 opt 5 datalen 4
52131->[I] cmd 10 opt 5 datalen 4
52131->[I] cmd 10 opt 5 datalen 4
52141->[I] dsc mode not match
52142->[I] cmd 10 opt 5 datalen 4
52142->[I] cmd 10 opt 5 datalen 4
52144->[I] codec_suspend s:1 reset:0


52144->[I] sync_codec_power_state s_o:1, s:1
52144->[I] codec_power s:1 bk_s:1
52145->[E] codec_off flag:1
52145->[I] state 1 => 5
52154->[I] cmd 10 opt 5 datalen 4
52154->[I] cmd 10 opt 5 datalen 4
52164->[I] cmd 86 opt 5 datalen 1
52164->[I] cmd 86 opt 5 datalen 1
52164->[I] etp_sts exp_fw:2
52168->[I] cmd 91 opt 5 datalen 2
52168->[I] ept_w_s write cmd:2 val:2

52170->[I] cmd 91 opt 5 datalen 3
52170->[I] ept_w_s write cmd:2 val:2

52174->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


52174->[I] etp chip act_s:1 


52174->[I] cmd 86 opt 5 datalen 4
52174->[I] cmd 86 opt 5 datalen 4
52176->[I] etp chip ept_s:1 app_s:1


52182->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


52182->[I] etp chip act_s:1 


52184->[I] etp chip ept_s:1 app_s:1


52187->[I] ept_r_ept expand:0 32 268442544
52486->[I] cmd 26 opt 5 datalen 10
52486->[I] eSpiCmdVideoCtrl cmd 1
52486->[I] video set work mode 0
52486->[I] eSpiCmdVideoCtrl cmd 1 return 1
52491->[I] cmd 26 opt 5 datalen 10
52491->[I] eSpiCmdVideoCtrl cmd 2
52491->[I] open video prepare
52491->[I] requiredFps 90
52491->[I] set upscale mode: 0
52494->[I] dsc mode not match
52498->[I] eSpiCmdVideoCtrl cmd 2 return 2
52503->[I] cmd 26 opt 5 datalen 10
52503->[I] eSpiCmdVideoCtrl cmd 3
52503->[I] video reset
52503->[I] eSpiCmdVideoCtrl cmd 3 return 1
52544->[I] i
52547->[I] i
52680->[I] requiredFps 0
55046->[I] i
55050->[I] ret 0
55052->[I] ret 0
55052->[I] ret 0
55054->[E] I2C2 Slave addr 0x7C, task app display tas code 4
55056->[I] ret 0
55058->[I] ret 0
55058->[I] ret 0
55078->[I] i
55609->[I] hard reset
55976->[I] cmd 26 opt 5 datalen 10
55976->[I] eSpiCmdVideoCtrl cmd 1
55976->[I] video set work mode 0
55976->[I] eSpiCmdVideoCtrl cmd 1 return 1
55981->[I] cmd 26 opt 5 datalen 10
55981->[I] eSpiCmdVideoCtrl cmd 2
55981->[I] open video prepare
55981->[I] requiredFps 90
55981->[I] keep upscale mode: 0
55981->[I] eSpiCmdVideoCtrl cmd 2 return 1
57155->[I] calc fps 0 => 90
59144->[I] cmd 86 opt 5 datalen 1
59145->[I] cmd 86 opt 5 datalen 1
59147->[I] cmd 86 opt 5 datalen 1
59147->[I] cmd 86 opt 5 datalen 1
59159->[I] cmd 10 opt 5 datalen 4
59159->[I] cmd 10 opt 5 datalen 4
59165->[I] ept_vef_sig in scr_len:35 key_id:1

59186->[I] cmd 10 opt 5 datalen 4
59186->[I] cmd 10 opt 5 datalen 4
59198->[I] cmd 10 opt 5 datalen 4
59200->[I] cmd 10 opt 5 datalen 4
59213->[I] cmd 10 opt 5 datalen 4
59213->[I] cmd 10 opt 5 datalen 4
59227->[I] cmd 10 opt 5 datalen 4
59227->[I] cmd 10 opt 5 datalen 4
59239->[I] cmd 10 opt 5 datalen 4
59239->[I] cmd 10 opt 5 datalen 4
59252->[I] cmd 10 opt 5 datalen 4
59252->[I] cmd 10 opt 5 datalen 4
59264->[I] cmd 10 opt 5 datalen 4
59266->[I] cmd 10 opt 5 datalen 4
59278->[I] cmd 10 opt 5 datalen 4
59278->[I] cmd 10 opt 5 datalen 4
59291->[I] cmd 10 opt 5 datalen 4
59291->[I] cmd 10 opt 5 datalen 4
59301->[I] cmd 86 opt 5 datalen 1
59301->[I] cmd 86 opt 5 datalen 1
59301->[I] etp_sts exp_fw:2
59305->[I] cmd 91 opt 5 datalen 2
59305->[I] ept_w_s write cmd:2 val:2

59308->[I] cmd 91 opt 5 datalen 3
59308->[I] ept_w_s write cmd:2 val:2

59310->[I] cmd 86 opt 5 datalen 4
59311->[I] cmd 86 opt 5 datalen 4
59311->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


59311->[I] etp chip act_s:1 


59313->[I] etp chip ept_s:1 app_s:1


59314->[I] cmd 86 opt 5 datalen 4
59319->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


59319->[I] etp chip act_s:1 


59321->[I] etp chip ept_s:1 app_s:1


59323->[I] ept_r_ept expand:0 1 268442544
59323->[I] cmd 86 opt 5 datalen 4
59325->[I] ept_r_ept expand:0 32 268442544
59328->[I] cmd 86 opt 5 datalen 4
59328->[I] cmd 86 opt 5 datalen 4
59330->[I] ept_r_ept expand:2 1 268442544
60771->[I] i
60789->[I] i
60794->[I] boe_localdimming_on

60989->[I] Panel: 0
60990->[I] Panel: 1
60995->[I] Panel: 0 ok!

60995->[I] BOE_DataInit B2 4,
60995->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
60996->[I] Panel: 1 ok!

60996->[I] BOE_DataInit B2 4,
60996->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
61008->[I] codec_suspend s:1 reset:0


61008->[I] sync_codec_power_state s_o:1, s:1
61008->[I] codec_power s:1 bk_s:1
61008->[E] codec_off flag:1
61008->[I] video stable
61008->[I] state 5 => 7
61008->[I] rx0 0x0BB003D0 Htotal=976, Vtotal=2992
61009->[I] rx1 0x0BB003D0 Htotal=976, Vtotal=2992
61009->[I] dp_rx_timming_check Ok
61087->[W] pps OK.
61088->[I] codec_resume s:1 reset:0


61088->[I] codec_power s:2 bk_s:1
61088->[E] codec_on flag:1
61097->[I] state 7 => 8
61107->[I] Panel ON
61151->[I] cmd 86 opt 5 datalen 1
61151->[I] cmd 86 opt 5 datalen 1
61153->[I] cmd 86 opt 5 datalen 1
61153->[I] cmd 86 opt 5 datalen 1
61157->[I] cmd 86 opt 5 datalen 1
61157->[I] cmd 86 opt 5 datalen 1
61157->[I] etp_sts ept_s:1


61162->[I] cmd 86 opt 5 datalen 1
61162->[I] cmd 86 opt 5 datalen 1
61173->[I] cmd 10 opt 5 datalen 4
61173->[I] cmd 10 opt 5 datalen 4
61179->[I] ept_vef_sig in scr_len:35 key_id:1

61201->[I] cmd 10 opt 5 datalen 4
61201->[I] cmd 10 opt 5 datalen 4
61213->[I] cmd 10 opt 5 datalen 4
61213->[I] cmd 10 opt 5 datalen 4
61225->[I] cmd 10 opt 5 datalen 4
61225->[I] cmd 10 opt 5 datalen 4
61237->[I] cmd 10 opt 5 datalen 4
61237->[I] cmd 10 opt 5 datalen 4
61250->[I] cmd 10 opt 5 datalen 4
61250->[I] cmd 10 opt 5 datalen 4
61262->[I] cmd 10 opt 5 datalen 4
61262->[I] cmd 10 opt 5 datalen 4
61275->[I] cmd 10 opt 5 datalen 4
61275->[I] cmd 10 opt 5 datalen 4
61289->[I] cmd 10 opt 5 datalen 4
61289->[I] cmd 10 opt 5 datalen 4
61301->[I] cmd 10 opt 5 datalen 4
61301->[I] cmd 10 opt 5 datalen 4
61308->[I] cmd 86 opt 5 datalen 4
61308->[I] cmd 86 opt 5 datalen 4
61310->[I] ept_r_ept expand:0 1 268442544
61311->[I] cmd 86 opt 5 datalen 1
61311->[I] cmd 86 opt 5 datalen 1
61311->[I] etp_sts exp_fw:2
61315->[I] cmd 86 opt 5 datalen 4
61315->[I] cmd 86 opt 5 datalen 4
61316->[I] cmd 91 opt 5 datalen 2
61316->[I] ept_w_s write cmd:2 val:2

61317->[I] ept_r_ept expand:2 1 268442544
61322->[I] cmd 91 opt 5 datalen 3
61322->[I] ept_w_s write cmd:2 val:2

61323->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


61323->[I] etp chip act_s:1 


61325->[I] etp chip ept_s:1 app_s:1


61327->[I] cmd 86 opt 5 datalen 4
61327->[I] cmd 86 opt 5 datalen 4
61331->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


61331->[I] etp chip act_s:1 


61333->[I] etp chip ept_s:1 app_s:1


61336->[I] ept_r_ept expand:0 32 268442544
63007->[E] I2C3 Slave addr 0x72, task app display tas code 1
63007->[E] retry cnt 1 ret 1
63166->[I] cmd 86 opt 5 datalen 1
63166->[I] cmd 86 opt 5 datalen 1
63168->[I] cmd 86 opt 5 datalen 1
63168->[I] cmd 86 opt 5 datalen 1
63168->[I] etp_sts ept_s:1


63171->[I] cmd 86 opt 5 datalen 1
63171->[I] cmd 86 opt 5 datalen 1
63171->[I] etp_sts exp_fw:2
63175->[I] cmd 91 opt 5 datalen 2
63175->[I] ept_w_s write cmd:2 val:2

63178->[I] cmd 91 opt 5 datalen 3
63178->[I] ept_w_s write cmd:2 val:2

63181->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


63181->[I] etp chip act_s:1 


63183->[I] etp chip ept_s:1 app_s:1


63183->[I] cmd 86 opt 5 datalen 4
63183->[I] cmd 86 opt 5 datalen 4
63189->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


63189->[I] etp chip act_s:1 


63191->[I] etp chip ept_s:1 app_s:1


63193->[I] ept_r_ept expand:0 32 268442544
64131->[I] Codec init done cnt:1.
64131->[E] codec_reset_flag wait:0
64131->[I] sync_codec_power_state s_o:1, s:2
64131->[I] codec_vol val:2 vol_bk:170 force:1 p_s:2


64131->[I] codec_unmute codec_s:1


64134->[I] codec_vol_mute 1


64134->[I] vol_ctl vol_bk:168 s:1


64152->[I] codec_jack n:0 o:170
64183->[I] codec_jack s:2
64183->[I] codec_vol val:2 vol_bk:2 force:0 p_s:2


66234->[I] vol_ctl end


81457->[I] cmd 86 opt 5 datalen 1
81457->[I] cmd 86 opt 5 datalen 1
82707->[I] boe_localdimming_off

82707->[I] i
82712->[I] i
82739->[I] codec_suspend s:2 reset:0


82740->[I] sync_codec_power_state s_o:2, s:1
82740->[I] codec_power s:1 bk_s:2
82740->[E] codec_off flag:0
82740->[I] codec_vol val:0 vol_bk:2 force:1 p_s:1


82740->[I] codec_vol_mute 0


82740->[I] state 8 => 9
82740->[I] codec_classd 0


82807->[I] Panel OFF
83866->[I] cmd 86 opt 5 datalen 1
83866->[I] cmd 86 opt 5 datalen 1
83869->[I] cmd 86 opt 5 datalen 1
83869->[I] cmd 86 opt 5 datalen 1
83869->[I] etp_sts ept_s:1


83875->[I] cmd 86 opt 5 datalen 1
83875->[I] cmd 86 opt 5 datalen 1
83875->[I] etp_sts exp_fw:2
83879->[I] cmd 91 opt 5 datalen 2
83879->[I] ept_w_s write cmd:2 val:2

83883->[I] cmd 91 opt 5 datalen 3
83883->[I] ept_w_s write cmd:2 val:2

83886->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


83886->[I] etp chip act_s:1 


83888->[I] etp chip ept_s:1 app_s:1


83888->[I] cmd 86 opt 5 datalen 4
83889->[I] cmd 86 opt 5 datalen 4
83894->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


83894->[I] etp chip act_s:1 


83896->[I] etp chip ept_s:1 app_s:1


83899->[I] ept_r_ept expand:0 32 268442544
101440->[I] cmd 86 opt 5 datalen 1
101440->[I] cmd 86 opt 5 datalen 1
101745->[I] cmd 85 opt 5 datalen 54
101759->[I] cmd 85 opt 5 datalen 54
101773->[I] cmd 85 opt 5 datalen 54
101787->[I] cmd 85 opt 5 datalen 54
101800->[I] cmd 85 opt 5 datalen 54
101815->[I] cmd 85 opt 5 datalen 54
101815->[I] ept_hid encpt_actv size:[293]


101815->[I] ept_act sn:P33000P1174A1400164 act_s:1 tm:1733808832

101815->[I] ept_vef_sig in scr_len:256 key_id:1

101826->[I] ept_vef_sig sha256 sus

101853->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


101853->[I] etp chip act_s:1 


101855->[I] etp chip ept_s:1 app_s:1


103868->[I] cmd 86 opt 5 datalen 1
103868->[I] cmd 86 opt 5 datalen 1
103871->[I] cmd 86 opt 5 datalen 1
103871->[I] cmd 86 opt 5 datalen 1
103871->[I] etp_sts ept_s:1


103873->[I] cmd 86 opt 5 datalen 1
103873->[I] cmd 86 opt 5 datalen 1
103873->[I] etp_sts exp_fw:2
103877->[I] cmd 91 opt 5 datalen 2
103877->[I] ept_w_s write cmd:2 val:2

103882->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


103882->[I] etp chip act_s:1 


103884->[I] etp chip ept_s:1 app_s:1


104315->[I] cmd 91 opt 5 datalen 3
104315->[I] ept_w_s write cmd:1 len:100 max:100

104325->[I] cmd 85 opt 5 datalen 54
104832->[I] cmd 86 opt 5 datalen 1
104832->[I] cmd 86 opt 5 datalen 1
104839->[I] cmd 91 opt 5 datalen 3
104839->[I] ept_w_s write cmd:2 val:2

104844->[I] cmd 86 opt 5 datalen 4
104844->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


104844->[I] etp chip act_s:1 


104844->[I] cmd 86 opt 5 datalen 4
104846->[I] etp chip ept_s:1 app_s:1


104848->[I] ept_r_ept expand:0 32 268442544
104860->[I] cmd 85 opt 5 datalen 54
104861->[I] cmd 86 opt 5 datalen 1
104861->[I] cmd 86 opt 5 datalen 1
104882->[I] cmd 85 opt 5 datalen 54
104894->[I] cmd 85 opt 5 datalen 54
104908->[I] cmd 85 opt 5 datalen 54
104923->[I] cmd 85 opt 5 datalen 54
104937->[I] cmd 85 opt 5 datalen 54
104951->[I] cmd 85 opt 5 datalen 54
104951->[I] ept_hid encpt_ept size:[401]


104951->[I] ept_eqt sn:P33000P1174A1400164 [1733106426][1733808834][2145916800] ept_s:1 exp_len:100

104951->[I] ept_vef_sig in scr_len:256 key_id:1

104962->[I] ept_vef_sig sha256 sus

104986->[I] ept_eqt ept_s:1

105011->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


105011->[I] etp chip act_s:1 


105013->[I] etp chip ept_s:1 app_s:1


107975->[I] cmd 86 opt 5 datalen 0
107975->[I] cmd 86 opt 5 datalen 0
107984->[I] cmd 86 opt 5 datalen 1
107984->[I] cmd 86 opt 5 datalen 1
107986->[I] cmd 86 opt 5 datalen 1
107986->[I] cmd 86 opt 5 datalen 1
107986->[I] etp_sts ept_s:1


109330->[I] cmd 86 opt 5 datalen 1
109330->[I] cmd 86 opt 5 datalen 1
109330->[I] etp_sts exp_fw:2
109335->[I] cmd 91 opt 5 datalen 2
109335->[I] ept_w_s write cmd:2 val:2

109337->[I] cmd 91 opt 5 datalen 3
109337->[I] ept_w_s write cmd:2 val:2

109341->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


109341->[I] etp chip act_s:1 


109342->[I] cmd 86 opt 5 datalen 4
109342->[I] cmd 86 opt 5 datalen 4
109343->[I] etp chip ept_s:1 app_s:1


109349->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


109349->[I] etp chip act_s:1 


109351->[I] etp chip ept_s:1 app_s:1


109353->[I] ept_r_ept expand:0 32 268442544
111740->[I] cmd 86 opt 5 datalen 1
111740->[I] cmd 86 opt 5 datalen 1
114322->[I] cmd 86 opt 5 datalen 1
114322->[I] cmd 86 opt 5 datalen 1
114324->[I] cmd 86 opt 5 datalen 1
114324->[I] cmd 86 opt 5 datalen 1
114324->[I] etp_sts ept_s:1


114328->[I] cmd 86 opt 5 datalen 1
114328->[I] cmd 86 opt 5 datalen 1
114328->[I] etp_sts exp_fw:2
114332->[I] cmd 91 opt 5 datalen 2
114332->[I] ept_w_s write cmd:2 val:2

114334->[I] cmd 86 opt 5 datalen 1
114334->[I] cmd 86 opt 5 datalen 1
114334->[I] etp_sts exp_fw:2
114337->[I] cmd 91 opt 5 datalen 3
114337->[I] ept_w_s write cmd:2 val:2

114338->[I] cmd 91 opt 5 datalen 2
114338->[I] ept_w_s write cmd:2 val:2

114338->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


114338->[I] etp chip act_s:1 


114340->[I] etp chip ept_s:1 app_s:1


114341->[I] cmd 86 opt 5 datalen 4
114341->[I] cmd 86 opt 5 datalen 4
114346->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


114346->[I] etp chip act_s:1 


114348->[I] etp chip ept_s:1 app_s:1


114354->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


114354->[I] etp chip act_s:1 


114356->[I] etp chip ept_s:1 app_s:1


114358->[I] ept_r_ept expand:0 32 268442544
116269->[I] requiredFps 0
117024->[I] frame changed
117024->[I] codec_suspend s:1 reset:0


117024->[I] sync_codec_power_state s_o:1, s:1
117025->[I] codec_power s:1 bk_s:1
117025->[E] codec_off flag:1
117025->[I] state 9 => 5
117025->[I] aw2013_blinking_details 2

118266->[I] cmd 26 opt 5 datalen 10
118266->[I] eSpiCmdVideoCtrl cmd 1
118266->[I] video set work mode 0
118266->[I] eSpiCmdVideoCtrl cmd 1 return 1
118271->[I] cmd 26 opt 5 datalen 10
118271->[I] eSpiCmdVideoCtrl cmd 2
118271->[I] open video prepare
118271->[I] requiredFps 90
118271->[I] set upscale mode: 1
118274->[I] dsc mode not match
118277->[I] eSpiCmdVideoCtrl cmd 2 return 2
118284->[I] cmd 26 opt 5 datalen 10
118284->[I] eSpiCmdVideoCtrl cmd 3
118284->[I] video reset
118284->[I] eSpiCmdVideoCtrl cmd 3 return 1
118307->[I] i
118310->[I] i
119146->[I] requiredFps 0
120809->[I] i
120813->[I] ret 0
120815->[I] ret 0
120815->[I] ret 0
120817->[I] ret 0
120819->[I] ret 0
120819->[I] ret 0
120839->[I] i
121370->[I] dsc mode not match
121373->[I] hard reset
121731->[I] cmd 26 opt 5 datalen 10
121731->[I] eSpiCmdVideoCtrl cmd 1
121731->[I] video set work mode 0
121731->[I] eSpiCmdVideoCtrl cmd 1 return 1
121736->[I] cmd 26 opt 5 datalen 10
121736->[I] eSpiCmdVideoCtrl cmd 2
121736->[I] open video prepare
121736->[I] requiredFps 90
121736->[I] keep upscale mode: 1
121736->[I] eSpiCmdVideoCtrl cmd 2 return 1
121795->[I] cmd 26 opt 5 datalen 10
121795->[I] eSpiCmdVideoCtrl cmd 2
121795->[I] open video prepare
121795->[I] keep upscale mode: 1
121795->[I] eSpiCmdVideoCtrl cmd 2 return 1
122824->[I] cmd 26 opt 5 datalen 10
122824->[I] eSpiCmdVideoCtrl cmd 2
122824->[I] open video prepare
122824->[I] keep upscale mode: 1
122824->[I] eSpiCmdVideoCtrl cmd 2 return 1
123853->[I] cmd 26 opt 5 datalen 10
123853->[I] eSpiCmdVideoCtrl cmd 2
123853->[I] open video prepare
123853->[I] keep upscale mode: 1
123853->[I] eSpiCmdVideoCtrl cmd 2 return 1
124882->[I] cmd 26 opt 5 datalen 10
124882->[I] eSpiCmdVideoCtrl cmd 2
124882->[I] open video prepare
124882->[I] keep upscale mode: 1
124882->[I] eSpiCmdVideoCtrl cmd 2 return 1
136895->[I] cmd 26 opt 5 datalen 10
136895->[I] eSpiCmdVideoCtrl cmd 3
136895->[I] video reset
136895->[I] eSpiCmdVideoCtrl cmd 3 return 1
136973->[I] i
136976->[I] i
139475->[I] i
139479->[I] ret 0
139481->[I] ret 0
139481->[I] ret 0
139483->[I] ret 0
139485->[I] ret 0
139485->[I] ret 0
139505->[I] i
140036->[I] dsc mode not match
140039->[I] hard reset
140379->[I] cmd 26 opt 5 datalen 10
140379->[I] eSpiCmdVideoCtrl cmd 1
140379->[I] video set work mode 0
140379->[I] eSpiCmdVideoCtrl cmd 1 return 1
140384->[I] cmd 26 opt 5 datalen 10
140384->[I] eSpiCmdVideoCtrl cmd 2
140384->[I] open video prepare
140384->[I] keep upscale mode: 1
140384->[I] eSpiCmdVideoCtrl cmd 2 return 1
140439->[I] cmd 26 opt 5 datalen 10
140439->[I] eSpiCmdVideoCtrl cmd 2
140439->[I] open video prepare
140439->[I] keep upscale mode: 1
140440->[I] eSpiCmdVideoCtrl cmd 2 return 1
141471->[I] cmd 26 opt 5 datalen 10
141471->[I] eSpiCmdVideoCtrl cmd 2
141471->[I] open video prepare
141471->[I] keep upscale mode: 1
141471->[I] eSpiCmdVideoCtrl cmd 2 return 1
142500->[I] cmd 26 opt 5 datalen 10
142500->[I] eSpiCmdVideoCtrl cmd 2
142500->[I] open video prepare
142500->[I] keep upscale mode: 1
142500->[I] eSpiCmdVideoCtrl cmd 2 return 1
143526->[I] cmd 26 opt 5 datalen 10
143526->[I] eSpiCmdVideoCtrl cmd 2
143526->[I] open video prepare
143526->[I] keep upscale mode: 1
143526->[I] eSpiCmdVideoCtrl cmd 2 return 1
