715252->[I] cmd 86 opt 5 datalen 1
715252->[I] cmd 86 opt 5 datalen 1
715252->[I] etp_sts exp_fw:2
715256->[I] cmd 91 opt 5 datalen 2
715256->[I] ept_w_s write cmd:2 val:2

715258->[I] cmd 86 opt 5 datalen 4
715258->[I] cmd 86 opt 5 datalen 4
715259->[I] cmd 3 opt 6 datalen 0
715263->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


715263->[I] etp chip act_s:1 


715265->[I] etp chip ept_s:1 app_s:1


715267->[I] ept_r_ept expand:0 1 268442544
715273->[I] cmd 86 opt 5 datalen 4
715273->[I] cmd 86 opt 5 datalen 4
715274->[I] ept_r_ept expand:2 1 268442544
715341->[I] requiredFps 0
715435->[I] i
715439->[I] ret 0
715441->[I] ret 0
715442->[I] ret 0
715443->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715445->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715447->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715449->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715451->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715453->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715455->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715457->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715459->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715461->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715463->[I] ret 1
715465->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715467->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715469->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715471->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715473->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715475->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715477->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715479->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715481->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715483->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715485->[I] ret 1
715485->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715487->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715489->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715491->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715493->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715495->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715497->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715499->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715501->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715503->[E] I2C2 Slave addr 0x7C, task app display tas code 4
715505->[I] ret 1
715525->[I] i
715989->[I] cmd 86 opt 5 datalen 1
715989->[I] cmd 86 opt 5 datalen 1
715991->[I] cmd 86 opt 5 datalen 1
715991->[I] cmd 86 opt 5 datalen 1
715993->[I] cmd 86 opt 5 datalen 1
715993->[I] cmd 86 opt 5 datalen 1
715993->[I] etp_sts ept_s:1


716000->[I] cmd 10 opt 5 datalen 4
716001->[I] cmd 10 opt 5 datalen 4
716006->[I] ept_vef_sig in scr_len:35 key_id:1

716027->[I] cmd 10 opt 5 datalen 4
716028->[I] cmd 10 opt 5 datalen 4
716039->[I] cmd 10 opt 5 datalen 4
716040->[I] cmd 10 opt 5 datalen 4
716052->[I] cmd 10 opt 5 datalen 4
716052->[I] cmd 10 opt 5 datalen 4
716056->[I] codec_suspend s:1 reset:0


716056->[I] sync_codec_power_state s_o:1, s:1
716056->[I] codec_power s:1 bk_s:1
716056->[E] codec_off flag:1
716056->[I] state 1 => 5
716064->[I] cmd 10 opt 5 datalen 4
716064->[I] cmd 10 opt 5 datalen 4
716076->[I] cmd 10 opt 5 datalen 4
716076->[I] cmd 10 opt 5 datalen 4
716089->[I] cmd 10 opt 5 datalen 4
716089->[I] cmd 10 opt 5 datalen 4
716102->[I] cmd 10 opt 5 datalen 4
716102->[I] cmd 10 opt 5 datalen 4
716113->[I] cmd 10 opt 5 datalen 4
716113->[I] cmd 10 opt 5 datalen 4
716125->[I] cmd 10 opt 5 datalen 4
716125->[I] cmd 10 opt 5 datalen 4
716135->[I] cmd 86 opt 5 datalen 1
716135->[I] cmd 86 opt 5 datalen 1
716135->[I] etp_sts exp_fw:2
716139->[I] cmd 91 opt 5 datalen 2
716139->[I] ept_w_s write cmd:2 val:2

716141->[I] cmd 91 opt 5 datalen 3
716141->[I] ept_w_s write cmd:2 val:2

716145->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


716145->[I] etp chip act_s:1 


716146->[I] cmd 86 opt 5 datalen 4
716147->[I] cmd 86 opt 5 datalen 4
716147->[I] etp chip ept_s:1 app_s:1


716153->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


716153->[I] etp chip act_s:1 


716155->[I] etp chip ept_s:1 app_s:1


716158->[I] ept_r_ept expand:0 32 268442544
717070->[I] cmd 26 opt 5 datalen 10
717070->[I] eSpiCmdVideoCtrl cmd 1
717070->[I] video set work mode 0
717070->[I] eSpiCmdVideoCtrl cmd 1 return 1
717075->[I] cmd 26 opt 5 datalen 10
717075->[I] eSpiCmdVideoCtrl cmd 2
717075->[I] open video prepare
717075->[I] requiredFps 90
717075->[I] set upscale mode: 1
717078->[I] dsc mode not match
717082->[I] eSpiCmdVideoCtrl cmd 2 return 2
717087->[I] cmd 26 opt 5 datalen 10
717087->[I] eSpiCmdVideoCtrl cmd 3
717087->[I] video reset
717087->[I] eSpiCmdVideoCtrl cmd 3 return 1
717181->[I] i
717184->[I] i
717235->[I] requiredFps 0
719683->[I] i
719687->[I] ret 0
719689->[I] ret 0
719690->[I] ret 0
719691->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719693->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719695->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719697->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719699->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719701->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719703->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719705->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719707->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719709->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719711->[I] ret 1
719713->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719715->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719717->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719719->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719721->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719723->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719725->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719727->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719729->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719731->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719733->[I] ret 1
719733->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719735->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719737->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719739->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719741->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719743->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719745->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719747->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719749->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719751->[E] I2C2 Slave addr 0x7C, task app display tas code 4
719753->[I] ret 1
719773->[I] i
720304->[I] dsc mode not match
720307->[I] hard reset
720668->[I] cmd 26 opt 5 datalen 10
720668->[I] eSpiCmdVideoCtrl cmd 1
720668->[I] video set work mode 0
720668->[I] eSpiCmdVideoCtrl cmd 1 return 1
720673->[I] cmd 26 opt 5 datalen 10
720673->[I] eSpiCmdVideoCtrl cmd 2
720673->[I] open video prepare
720673->[I] requiredFps 90
720673->[I] keep upscale mode: 1
720673->[I] eSpiCmdVideoCtrl cmd 2 return 1
721828->[I] calc fps 0 => 90
721851->[I] cmd 86 opt 5 datalen 1
721851->[I] cmd 86 opt 5 datalen 1
721860->[I] cmd 86 opt 5 datalen 1
721860->[I] cmd 86 opt 5 datalen 1
721876->[I] cmd 10 opt 5 datalen 4
721878->[I] cmd 10 opt 5 datalen 4
721883->[I] ept_vef_sig in scr_len:35 key_id:1

721908->[I] cmd 10 opt 5 datalen 4
721908->[I] cmd 10 opt 5 datalen 4
721922->[I] cmd 10 opt 5 datalen 4
721922->[I] cmd 10 opt 5 datalen 4
721927->[I] cmd 86 opt 5 datalen 4
721927->[I] cmd 86 opt 5 datalen 4
721928->[I] ept_r_ept expand:0 1 268442544
721933->[I] cmd 86 opt 5 datalen 4
721934->[I] cmd 86 opt 5 datalen 4
721935->[I] cmd 10 opt 5 datalen 4
721935->[I] ept_r_ept expand:2 1 268442544
721936->[I] cmd 10 opt 5 datalen 4
721949->[I] cmd 10 opt 5 datalen 4
721949->[I] cmd 10 opt 5 datalen 4
721961->[I] cmd 10 opt 5 datalen 4
721961->[I] cmd 10 opt 5 datalen 4
721973->[I] cmd 10 opt 5 datalen 4
721974->[I] cmd 10 opt 5 datalen 4
721986->[I] cmd 10 opt 5 datalen 4
721988->[I] cmd 10 opt 5 datalen 4
722000->[I] cmd 10 opt 5 datalen 4
722000->[I] cmd 10 opt 5 datalen 4
722012->[I] cmd 10 opt 5 datalen 4
722013->[I] cmd 10 opt 5 datalen 4
722023->[I] cmd 86 opt 5 datalen 1
722023->[I] cmd 86 opt 5 datalen 1
722023->[I] etp_sts exp_fw:2
722027->[I] cmd 91 opt 5 datalen 2
722027->[I] ept_w_s write cmd:2 val:2

722030->[I] cmd 91 opt 5 datalen 3
722030->[I] ept_w_s write cmd:2 val:2

722033->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


722033->[I] etp chip act_s:1 


722035->[I] cmd 86 opt 5 datalen 4
722035->[I] cmd 86 opt 5 datalen 4
722035->[I] etp chip ept_s:1 app_s:1


722041->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


722041->[I] etp chip act_s:1 


722043->[I] etp chip ept_s:1 app_s:1


722047->[I] ept_r_ept expand:0 32 268442544
723864->[I] cmd 86 opt 5 datalen 1
723866->[I] cmd 86 opt 5 datalen 1
723867->[I] cmd 86 opt 5 datalen 1
723867->[I] cmd 86 opt 5 datalen 1
723870->[I] cmd 86 opt 5 datalen 1
723870->[I] cmd 86 opt 5 datalen 1
723870->[I] etp_sts ept_s:1


723872->[I] cmd 86 opt 5 datalen 1
723872->[I] cmd 86 opt 5 datalen 1
723883->[I] cmd 10 opt 5 datalen 4
723883->[I] cmd 10 opt 5 datalen 4
723890->[I] ept_vef_sig in scr_len:35 key_id:1

723911->[I] cmd 10 opt 5 datalen 4
723911->[I] cmd 10 opt 5 datalen 4
723924->[I] cmd 10 opt 5 datalen 4
723924->[I] cmd 10 opt 5 datalen 4
723936->[I] cmd 10 opt 5 datalen 4
723936->[I] cmd 10 opt 5 datalen 4
723948->[I] cmd 10 opt 5 datalen 4
723949->[I] cmd 10 opt 5 datalen 4
723961->[I] cmd 10 opt 5 datalen 4
723961->[I] cmd 10 opt 5 datalen 4
723973->[I] cmd 10 opt 5 datalen 4
723973->[I] cmd 10 opt 5 datalen 4
723986->[I] cmd 10 opt 5 datalen 4
723986->[I] cmd 10 opt 5 datalen 4
723998->[I] cmd 10 opt 5 datalen 4
724000->[I] cmd 10 opt 5 datalen 4
724012->[I] cmd 10 opt 5 datalen 4
724013->[I] cmd 10 opt 5 datalen 4
724023->[I] cmd 86 opt 5 datalen 1
724023->[I] cmd 86 opt 5 datalen 1
724023->[I] etp_sts exp_fw:2
724027->[I] cmd 91 opt 5 datalen 2
724027->[I] ept_w_s write cmd:2 val:2

724030->[I] cmd 91 opt 5 datalen 3
724030->[I] ept_w_s write cmd:2 val:2

724033->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


724033->[I] etp chip act_s:1 


724035->[I] cmd 86 opt 5 datalen 4
724035->[I] cmd 86 opt 5 datalen 4
724035->[I] etp chip ept_s:1 app_s:1


724041->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


724041->[I] etp chip act_s:1 


724043->[I] etp chip ept_s:1 app_s:1


724046->[I] ept_r_ept expand:0 32 268442544
725876->[I] cmd 86 opt 5 datalen 1
725878->[I] cmd 86 opt 5 datalen 1
725879->[I] cmd 86 opt 5 datalen 1
725879->[I] cmd 86 opt 5 datalen 1
725879->[I] etp_sts ept_s:1


725881->[I] cmd 86 opt 5 datalen 1
725881->[I] cmd 86 opt 5 datalen 1
725881->[I] etp_sts exp_fw:2
725885->[I] cmd 91 opt 5 datalen 2
725886->[I] ept_w_s write cmd:2 val:2

725889->[I] cmd 91 opt 5 datalen 3
725889->[I] ept_w_s write cmd:2 val:2

725891->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


725891->[I] etp chip act_s:1 


725893->[I] etp chip ept_s:1 app_s:1


725895->[I] cmd 86 opt 5 datalen 4
725896->[I] cmd 86 opt 5 datalen 4
725899->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


725899->[I] etp chip act_s:1 


725901->[I] etp chip ept_s:1 app_s:1


725904->[I] ept_r_ept expand:0 32 268442544
725925->[I] i
725941->[I] i
725946->[I] boe_localdimming_on

726137->[I] Panel: 0
726138->[I] Panel: 1
726143->[I] Panel: 0 ok!

726143->[I] BOE_DataInit B2 4,
726143->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
726144->[I] Panel: 1 ok!

726144->[I] BOE_DataInit B2 4,
726144->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
726158->[I] codec_suspend s:1 reset:0


726158->[I] sync_codec_power_state s_o:1, s:1
726158->[I] codec_power s:1 bk_s:1
726158->[E] codec_off flag:1
726158->[I] video stable
726158->[I] state 5 => 7
726158->[I] rx0 0x08E00960 Htotal=2400, Vtotal=2272
726159->[I] rx1 0x08E00960 Htotal=2400, Vtotal=2272
726159->[I] dp_rx_timming_check Ok
726249->[W] pps OK.
726249->[I] codec_resume s:1 reset:0


726249->[I] codec_power s:2 bk_s:1
726249->[E] codec_on flag:1
726255->[I] state 7 => 8
726257->[I] Panel ON
728159->[E] I2C3 Slave addr 0x72, task app display tas code 1
728159->[E] retry cnt 1 ret 1
729335->[I] Codec init done cnt:1.
729335->[E] codec_reset_flag wait:0
729335->[I] sync_codec_power_state s_o:1, s:2
729335->[I] codec_vol val:2 vol_bk:0 force:1 p_s:2


729335->[I] codec_unmute codec_s:1


729338->[I] codec_vol_mute 1


729338->[I] vol_ctl vol_bk:168 s:1


729366->[I] codec_jack n:0 o:170
729398->[I] codec_jack s:2
729398->[I] codec_vol val:2 vol_bk:2 force:0 p_s:2


731439->[I] vol_ctl end


743872->[I] cmd 86 opt 5 datalen 1
743872->[I] cmd 86 opt 5 datalen 1
744246->[I] cmd 85 opt 5 datalen 54
744260->[I] cmd 85 opt 5 datalen 54
744274->[I] cmd 85 opt 5 datalen 54
744288->[I] cmd 85 opt 5 datalen 54
744304->[I] cmd 85 opt 5 datalen 54
744318->[I] cmd 85 opt 5 datalen 54
744318->[I] ept_hid encpt_actv size:[293]


744319->[I] ept_act sn:P33000P1174A1400164 act_s:1 tm:1733775497

744319->[I] ept_vef_sig in scr_len:256 key_id:1

744332->[I] ept_vef_sig sha256 sus

744359->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


744359->[I] etp chip act_s:1 


744361->[I] etp chip ept_s:1 app_s:1


745881->[I] cmd 86 opt 5 datalen 1
745881->[I] cmd 86 opt 5 datalen 1
745882->[I] cmd 86 opt 5 datalen 1
745882->[I] cmd 86 opt 5 datalen 1
745882->[I] etp_sts ept_s:1


745885->[I] cmd 86 opt 5 datalen 1
745885->[I] cmd 86 opt 5 datalen 1
745885->[I] etp_sts exp_fw:2
745889->[I] cmd 91 opt 5 datalen 2
745889->[I] ept_w_s write cmd:2 val:2

745896->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


745896->[I] etp chip act_s:1 


745897->[I] etp chip ept_s:1 app_s:1


746359->[I] boe_localdimming_off

746359->[I] i
746366->[I] i
746394->[I] codec_suspend s:2 reset:0


746394->[I] sync_codec_power_state s_o:2, s:1
746394->[I] codec_power s:1 bk_s:2
746394->[E] codec_off flag:0
746394->[I] codec_vol val:0 vol_bk:2 force:1 p_s:1


746394->[I] codec_vol_mute 0


746394->[I] state 8 => 9
746394->[I] codec_classd 0


746459->[I] Panel OFF
747341->[I] cmd 86 opt 5 datalen 1
747341->[I] cmd 86 opt 5 datalen 1
747350->[I] cmd 91 opt 5 datalen 3
747350->[I] ept_w_s write cmd:2 val:2

747354->[I] cmd 86 opt 5 datalen 4
747355->[I] cmd 86 opt 5 datalen 4
747355->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


747355->[I] etp chip act_s:1 


747357->[I] etp chip ept_s:1 app_s:1


747360->[I] ept_r_ept expand:0 32 268442544
747360->[I] cmd 86 opt 5 datalen 1
747360->[I] cmd 86 opt 5 datalen 1
754248->[I] cmd 86 opt 5 datalen 1
754248->[I] cmd 86 opt 5 datalen 1
765870->[I] cmd 86 opt 5 datalen 1
765870->[I] cmd 86 opt 5 datalen 1
765872->[I] cmd 86 opt 5 datalen 1
765872->[I] cmd 86 opt 5 datalen 1
765872->[I] etp_sts ept_s:1


765874->[I] cmd 86 opt 5 datalen 1
765874->[I] cmd 86 opt 5 datalen 1
765874->[I] etp_sts exp_fw:2
765878->[I] cmd 91 opt 5 datalen 2
765878->[I] ept_w_s write cmd:2 val:2

765882->[I] cmd 91 opt 5 datalen 3
765882->[I] ept_w_s write cmd:2 val:2

765885->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


765885->[I] etp chip act_s:1 


765886->[I] cmd 86 opt 5 datalen 4
765887->[I] etp chip ept_s:1 app_s:1


765889->[I] cmd 86 opt 5 datalen 4
765893->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


765893->[I] etp chip act_s:1 


765895->[I] etp chip ept_s:1 app_s:1


765899->[I] ept_r_ept expand:0 32 268442544
766250->[I] cmd 91 opt 5 datalen 3
766250->[I] ept_w_s write cmd:1 len:100 max:100

766259->[I] cmd 85 opt 5 datalen 54
766273->[I] cmd 85 opt 5 datalen 54
766288->[I] cmd 85 opt 5 datalen 54
766302->[I] cmd 85 opt 5 datalen 54
766316->[I] cmd 85 opt 5 datalen 54
766331->[I] cmd 85 opt 5 datalen 54
766345->[I] cmd 85 opt 5 datalen 54
766359->[I] cmd 85 opt 5 datalen 54
766359->[I] ept_hid encpt_ept size:[401]


766359->[I] ept_eqt sn:P33000P1174A1400164 [1733106426][1733775519][2145916800] ept_s:1 exp_len:100

766359->[I] ept_vef_sig in scr_len:256 key_id:1

766371->[I] ept_vef_sig sha256 sus

766394->[I] ept_eqt ept_s:1

766419->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


766419->[I] etp chip act_s:1 


766421->[I] etp chip ept_s:1 app_s:1


769369->[I] cmd 86 opt 5 datalen 0
769369->[I] cmd 86 opt 5 datalen 0
769378->[I] cmd 86 opt 5 datalen 1
769378->[I] cmd 86 opt 5 datalen 1
769380->[I] cmd 86 opt 5 datalen 1
769380->[I] cmd 86 opt 5 datalen 1
769380->[I] etp_sts ept_s:1


771253->[I] cmd 86 opt 5 datalen 1
771255->[I] cmd 86 opt 5 datalen 1
771255->[I] etp_sts exp_fw:2
771259->[I] cmd 91 opt 5 datalen 2
771259->[I] ept_w_s write cmd:2 val:2

771262->[I] cmd 91 opt 5 datalen 3
771262->[I] ept_w_s write cmd:2 val:2

771266->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


771266->[I] etp chip act_s:1 


771267->[I] cmd 86 opt 5 datalen 4
771267->[I] cmd 86 opt 5 datalen 4
771268->[I] etp chip ept_s:1 app_s:1


771274->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


771274->[I] etp chip act_s:1 


771276->[I] etp chip ept_s:1 app_s:1


771280->[I] ept_r_ept expand:0 32 268442544
776246->[I] cmd 86 opt 5 datalen 1
776246->[I] cmd 86 opt 5 datalen 1
776248->[I] cmd 86 opt 5 datalen 1
776248->[I] cmd 86 opt 5 datalen 1
776248->[I] etp_sts ept_s:1


776250->[I] cmd 86 opt 5 datalen 1
776250->[I] cmd 86 opt 5 datalen 1
776250->[I] etp_sts exp_fw:2
776254->[I] cmd 91 opt 5 datalen 2
776254->[I] ept_w_s write cmd:2 val:2

776255->[I] cmd 86 opt 5 datalen 1
776256->[I] cmd 86 opt 5 datalen 1
776256->[I] etp_sts exp_fw:2
776260->[I] cmd 91 opt 5 datalen 3
776260->[I] ept_w_s write cmd:2 val:2

776260->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


776260->[I] etp chip act_s:1 


776261->[I] cmd 91 opt 5 datalen 2
776261->[I] ept_w_s write cmd:2 val:2

776262->[I] etp chip ept_s:1 app_s:1


776264->[I] cmd 86 opt 5 datalen 4
776264->[I] cmd 86 opt 5 datalen 4
776268->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


776268->[I] etp chip act_s:1 


776270->[I] etp chip ept_s:1 app_s:1


776276->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


776276->[I] etp chip act_s:1 


776278->[I] etp chip ept_s:1 app_s:1


776281->[I] ept_r_ept expand:0 32 268442544
831562->[I] i
831567->[I] boe_localdimming_on

832568->[I] i
832585->[I] codec_resume s:1 reset:0


832585->[I] codec_power s:2 bk_s:1
832585->[E] codec_on flag:1
832585->[I] state 9 => 8
832585->[I] Panel ON
832585->[I] boe_localdimming_off

832585->[I] i
832590->[I] i
832590->[E] I2C3 Slave addr 0x72, task app display tas code 1
832590->[E] retry cnt 1 ret 1
832618->[I] i
832622->[I] boe_localdimming_on

832837->[I] Panel: 0
832837->[I] Panel: 1
832843->[I] Panel: 0 ok!

832843->[I] BOE_DataInit B2 4,
832843->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
832843->[I] Panel: 1 ok!

832843->[I] BOE_DataInit B2 4,
832843->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
835672->[I] Codec init done cnt:1.
835672->[E] codec_reset_flag wait:0
835672->[I] sync_codec_power_state s_o:1, s:2
835672->[I] codec_vol val:2 vol_bk:0 force:1 p_s:2


835672->[I] codec_unmute codec_s:1


835675->[I] codec_vol_mute 1


835677->[I] vol_ctl vol_bk:168 s:1


835704->[I] codec_jack n:0 o:170
835736->[I] codec_jack s:2
835736->[I] codec_vol val:2 vol_bk:2 force:0 p_s:2


837777->[I] vol_ctl end


2802478->[I] boe_localdimming_off

2802478->[I] i
2802484->[I] i