13998328->[I] cmd 86 opt 5 datalen 1
13998328->[I] cmd 86 opt 5 datalen 1
13998328->[I] etp_sts exp_fw:2
13998331->[I] cmd 3 opt 6 datalen 0
13998333->[I] cmd 91 opt 5 datalen 2
13998333->[I] ept_w_s write cmd:2 val:2

13998334->[I] cmd 86 opt 5 datalen 4
13998334->[I] cmd 86 opt 5 datalen 4
13998339->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


13998339->[I] etp chip act_s:1 


13998341->[I] etp chip ept_s:1 app_s:1


13998343->[I] ept_r_ept expand:0 1 268442544
13998348->[I] cmd 86 opt 5 datalen 4
13998348->[I] cmd 86 opt 5 datalen 4
13998349->[I] ept_r_ept expand:2 1 268442544
13998520->[I] requiredFps 0
13998598->[I] i
13998602->[I] ret 0
13998604->[I] ret 0
13998605->[I] ret 0
13998606->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998608->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998610->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998612->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998614->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998616->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998618->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998620->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998622->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998624->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998626->[I] ret 1
13998628->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998630->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998632->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998634->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998636->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998638->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998640->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998642->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998644->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998646->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998648->[I] ret 1
13998648->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998650->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998652->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998654->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998656->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998658->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998660->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998662->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998664->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998666->[E] I2C2 Slave addr 0x7C, task app display tas code 4
13998668->[I] ret 1
13998688->[I] i
13999161->[I] cmd 86 opt 5 datalen 1
13999161->[I] cmd 86 opt 5 datalen 1
13999166->[I] cmd 86 opt 5 datalen 1
13999166->[I] cmd 86 opt 5 datalen 1
13999172->[I] cmd 86 opt 5 datalen 1
13999173->[I] cmd 86 opt 5 datalen 1
13999173->[I] etp_sts ept_s:1


13999180->[I] cmd 10 opt 5 datalen 4
13999180->[I] cmd 10 opt 5 datalen 4
13999185->[I] ept_vef_sig in scr_len:35 key_id:1

13999212->[I] cmd 10 opt 5 datalen 4
13999212->[I] cmd 10 opt 5 datalen 4
13999219->[I] dsc mode not match
13999222->[I] codec_suspend s:1 reset:0


13999222->[I] sync_codec_power_state s_o:1, s:1
13999222->[I] codec_power s:1 bk_s:1
13999222->[E] codec_off flag:1
13999223->[I] state 1 => 5
13999229->[I] cmd 10 opt 5 datalen 4
13999229->[I] cmd 10 opt 5 datalen 4
13999246->[I] cmd 10 opt 5 datalen 4
13999246->[I] cmd 10 opt 5 datalen 4
13999263->[I] cmd 10 opt 5 datalen 4
13999263->[I] cmd 10 opt 5 datalen 4
13999282->[I] cmd 10 opt 5 datalen 4
13999282->[I] cmd 10 opt 5 datalen 4
13999299->[I] cmd 10 opt 5 datalen 4
13999299->[I] cmd 10 opt 5 datalen 4
13999316->[I] cmd 10 opt 5 datalen 4
13999316->[I] cmd 10 opt 5 datalen 4
13999333->[I] cmd 10 opt 5 datalen 4
13999333->[I] cmd 10 opt 5 datalen 4
13999351->[I] cmd 10 opt 5 datalen 4
13999351->[I] cmd 10 opt 5 datalen 4
13999366->[I] cmd 86 opt 5 datalen 1
13999367->[I] cmd 86 opt 5 datalen 1
13999367->[I] etp_sts exp_fw:2
13999371->[I] cmd 91 opt 5 datalen 2
13999371->[I] ept_w_s write cmd:2 val:2

13999376->[I] cmd 91 opt 5 datalen 3
13999376->[I] ept_w_s write cmd:2 val:2

13999376->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


13999376->[I] etp chip act_s:1 


13999378->[I] etp chip ept_s:1 app_s:1


13999384->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


13999384->[I] etp chip act_s:1 


13999386->[I] cmd 86 opt 5 datalen 4
13999386->[I] cmd 86 opt 5 datalen 4
13999386->[I] etp chip ept_s:1 app_s:1


13999389->[I] ept_r_ept expand:0 32 268442544
14000394->[I] cmd 26 opt 5 datalen 10
14000394->[I] eSpiCmdVideoCtrl cmd 1
14000394->[I] video set work mode 0
14000394->[I] eSpiCmdVideoCtrl cmd 1 return 1
14000399->[I] cmd 26 opt 5 datalen 10
14000399->[I] eSpiCmdVideoCtrl cmd 2
14000400->[I] open video prepare
14000400->[I] requiredFps 90
14000400->[I] keep upscale mode: 1
14000400->[I] eSpiCmdVideoCtrl cmd 2 return 1
14000493->[I] requiredFps 0
14000593->[I] requiredFps 90
14000619->[I] cmd 26 opt 5 datalen 10
14000619->[I] eSpiCmdVideoCtrl cmd 2
14000619->[I] open video prepare
14000619->[I] keep upscale mode: 1
14000619->[I] eSpiCmdVideoCtrl cmd 2 return 1
14001648->[I] cmd 26 opt 5 datalen 10
14001648->[I] eSpiCmdVideoCtrl cmd 2
14001648->[I] open video prepare
14001649->[I] keep upscale mode: 1
14001649->[I] eSpiCmdVideoCtrl cmd 2 return 1
14002673->[I] cmd 26 opt 5 datalen 10
14002673->[I] eSpiCmdVideoCtrl cmd 2
14002673->[I] open video prepare
14002673->[I] keep upscale mode: 1
14002673->[I] eSpiCmdVideoCtrl cmd 2 return 1
14003709->[I] cmd 26 opt 5 datalen 10
14003709->[I] eSpiCmdVideoCtrl cmd 2
14003709->[I] open video prepare
14003709->[I] keep upscale mode: 1
14003709->[I] eSpiCmdVideoCtrl cmd 2 return 1
14015685->[I] cmd 26 opt 5 datalen 10
14015685->[I] eSpiCmdVideoCtrl cmd 3
14015685->[I] video reset
14015685->[I] eSpiCmdVideoCtrl cmd 3 return 1
14015776->[I] i
14015779->[I] i
14018278->[I] i
14018282->[I] ret 0
14018284->[I] ret 0
14018285->[I] ret 0
14018286->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018288->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018290->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018292->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018294->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018296->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018298->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018300->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018302->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018304->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018306->[I] ret 1
14018308->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018310->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018312->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018314->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018316->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018318->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018320->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018322->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018324->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018326->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018328->[I] ret 1
14018328->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018330->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018332->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018334->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018336->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018338->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018340->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018342->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018344->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018346->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14018348->[I] ret 1
14018368->[I] i
14018899->[I] dsc mode not match
14018902->[I] hard reset
14019487->[I] cmd 26 opt 5 datalen 10
14019487->[I] eSpiCmdVideoCtrl cmd 1
14019487->[I] video set work mode 0
14019487->[I] eSpiCmdVideoCtrl cmd 1 return 1
14019492->[I] cmd 26 opt 5 datalen 10
14019492->[I] eSpiCmdVideoCtrl cmd 2
14019492->[I] open video prepare
14019492->[I] keep upscale mode: 1
14019492->[I] eSpiCmdVideoCtrl cmd 2 return 1
14021113->[I] cmd 86 opt 5 datalen 1
14021113->[I] cmd 86 opt 5 datalen 1
14021119->[I] cmd 86 opt 5 datalen 1
14021120->[I] cmd 86 opt 5 datalen 1
14021138->[I] cmd 10 opt 5 datalen 4
14021138->[I] cmd 10 opt 5 datalen 4
14021145->[I] ept_vef_sig in scr_len:35 key_id:1

14021173->[I] cmd 10 opt 5 datalen 4
14021174->[I] cmd 10 opt 5 datalen 4
14021192->[I] cmd 10 opt 5 datalen 4
14021192->[I] cmd 10 opt 5 datalen 4
14021212->[I] cmd 10 opt 5 datalen 4
14021212->[I] cmd 10 opt 5 datalen 4
14021231->[I] cmd 10 opt 5 datalen 4
14021231->[I] cmd 10 opt 5 datalen 4
14021247->[I] cmd 86 opt 5 datalen 4
14021247->[I] cmd 86 opt 5 datalen 4
14021248->[I] ept_r_ept expand:0 1 268442544
14021249->[I] cmd 10 opt 5 datalen 4
14021249->[I] cmd 10 opt 5 datalen 4
14021253->[I] cmd 86 opt 5 datalen 4
14021253->[I] cmd 86 opt 5 datalen 4
14021254->[I] ept_r_ept expand:2 1 268442544
14021270->[I] cmd 10 opt 5 datalen 4
14021270->[I] cmd 10 opt 5 datalen 4
14021288->[I] cmd 10 opt 5 datalen 4
14021288->[I] cmd 10 opt 5 datalen 4
14021307->[I] cmd 10 opt 5 datalen 4
14021307->[I] cmd 10 opt 5 datalen 4
14021327->[I] cmd 10 opt 5 datalen 4
14021327->[I] cmd 10 opt 5 datalen 4
14021343->[I] cmd 86 opt 5 datalen 1
14021343->[I] cmd 86 opt 5 datalen 1
14021343->[I] etp_sts exp_fw:2
14021348->[I] cmd 91 opt 5 datalen 2
14021348->[I] ept_w_s write cmd:2 val:2

14021353->[I] cmd 91 opt 5 datalen 3
14021353->[I] ept_w_s write cmd:2 val:2

14021353->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14021353->[I] etp chip act_s:1 


14021355->[I] etp chip ept_s:1 app_s:1


14021361->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14021361->[I] etp chip act_s:1 


14021363->[I] etp chip ept_s:1 app_s:1


14021365->[I] cmd 86 opt 5 datalen 4
14021365->[I] cmd 86 opt 5 datalen 4
14021367->[I] ept_r_ept expand:0 32 268442544
14023138->[I] cmd 86 opt 5 datalen 1
14023140->[I] cmd 86 opt 5 datalen 1
14023149->[I] cmd 86 opt 5 datalen 1
14023151->[I] cmd 86 opt 5 datalen 1
14023171->[I] cmd 86 opt 5 datalen 1
14023171->[I] cmd 86 opt 5 datalen 1
14023171->[I] etp_sts ept_s:1


14023182->[I] cmd 86 opt 5 datalen 1
14023182->[I] cmd 86 opt 5 datalen 1
14023201->[I] cmd 10 opt 5 datalen 4
14023201->[I] cmd 10 opt 5 datalen 4
14023207->[I] ept_vef_sig in scr_len:35 key_id:1

14023260->[I] cmd 10 opt 5 datalen 4
14023260->[I] cmd 10 opt 5 datalen 4
14023295->[I] cmd 10 opt 5 datalen 4
14023296->[I] cmd 10 opt 5 datalen 4
14023322->[I] cmd 10 opt 5 datalen 4
14023322->[I] cmd 10 opt 5 datalen 4
14023356->[I] cmd 10 opt 5 datalen 4
14023356->[I] cmd 10 opt 5 datalen 4
14023407->[I] cmd 10 opt 5 datalen 4
14023408->[I] cmd 10 opt 5 datalen 4
14023430->[I] cmd 10 opt 5 datalen 4
14023430->[I] cmd 10 opt 5 datalen 4
14023453->[I] cmd 10 opt 5 datalen 4
14023453->[I] cmd 10 opt 5 datalen 4
14023478->[I] cmd 10 opt 5 datalen 4
14023478->[I] cmd 10 opt 5 datalen 4
14023502->[I] cmd 10 opt 5 datalen 4
14023502->[I] cmd 10 opt 5 datalen 4
14023520->[I] cmd 86 opt 5 datalen 1
14023520->[I] cmd 86 opt 5 datalen 1
14023521->[I] etp_sts exp_fw:2
14023524->[I] cmd 91 opt 5 datalen 2
14023525->[I] ept_w_s write cmd:2 val:2

14023530->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14023530->[I] etp chip act_s:1 


14023532->[I] etp chip ept_s:1 app_s:1


14023535->[I] cmd 91 opt 5 datalen 3
14023535->[I] ept_w_s write cmd:2 val:2

14023540->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14023540->[I] etp chip act_s:1 


14023542->[I] etp chip ept_s:1 app_s:1


14023548->[I] cmd 86 opt 5 datalen 4
14023548->[I] cmd 86 opt 5 datalen 4
14023551->[I] ept_r_ept expand:0 32 268442544
14025192->[I] cmd 86 opt 5 datalen 1
14025192->[I] cmd 86 opt 5 datalen 1
14025199->[I] cmd 86 opt 5 datalen 1
14025200->[I] cmd 86 opt 5 datalen 1
14025200->[I] etp_sts ept_s:1


14025210->[I] cmd 86 opt 5 datalen 1
14025211->[I] cmd 86 opt 5 datalen 1
14025211->[I] etp_sts exp_fw:2
14025215->[I] cmd 91 opt 5 datalen 2
14025215->[I] ept_w_s write cmd:2 val:2

14025220->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14025220->[I] etp chip act_s:1 


14025221->[I] cmd 91 opt 5 datalen 3
14025221->[I] ept_w_s write cmd:2 val:2

14025222->[I] etp chip ept_s:1 app_s:1


14025228->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14025228->[I] etp chip act_s:1 


14025230->[I] etp chip ept_s:1 app_s:1


14025232->[I] cmd 86 opt 5 datalen 4
14025232->[I] cmd 86 opt 5 datalen 4
14025234->[I] ept_r_ept expand:0 32 268442544
14029565->[I] requiredFps 0
14031558->[I] cmd 26 opt 5 datalen 10
14031558->[I] eSpiCmdVideoCtrl cmd 3
14031558->[I] video reset
14031558->[I] eSpiCmdVideoCtrl cmd 3 return 1
14031583->[I] i
14031586->[I] i
14034085->[I] i
14034089->[I] ret 0
14034091->[I] ret 0
14034092->[I] ret 0
14034093->[I] ret 0
14034095->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034097->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034099->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034101->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034103->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034105->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034107->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034109->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034111->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034113->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034115->[I] ret 1
14034115->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034117->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034119->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034121->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034123->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034125->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034127->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034129->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034131->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034133->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14034135->[I] ret 1
14034155->[I] i
14034686->[I] dsc mode not match
14034689->[I] hard reset
14035858->[I] cmd 26 opt 5 datalen 10
14035858->[I] eSpiCmdVideoCtrl cmd 1
14035858->[I] video set work mode 0
14035858->[I] eSpiCmdVideoCtrl cmd 1 return 1
14035863->[I] cmd 26 opt 5 datalen 10
14035863->[I] eSpiCmdVideoCtrl cmd 2
14035863->[I] open video prepare
14035863->[I] requiredFps 90
14035863->[I] keep upscale mode: 1
14035864->[I] eSpiCmdVideoCtrl cmd 2 return 1
14035962->[I] cmd 26 opt 5 datalen 10
14035962->[I] eSpiCmdVideoCtrl cmd 2
14035962->[I] open video prepare
14035962->[I] keep upscale mode: 1
14035962->[I] eSpiCmdVideoCtrl cmd 2 return 1
14037004->[I] cmd 26 opt 5 datalen 10
14037004->[I] eSpiCmdVideoCtrl cmd 2
14037004->[I] open video prepare
14037004->[I] keep upscale mode: 1
14037004->[I] eSpiCmdVideoCtrl cmd 2 return 1
14038040->[I] cmd 26 opt 5 datalen 10
14038040->[I] eSpiCmdVideoCtrl cmd 2
14038041->[I] open video prepare
14038041->[I] keep upscale mode: 1
14038041->[I] eSpiCmdVideoCtrl cmd 2 return 1
14039090->[I] cmd 26 opt 5 datalen 10
14039090->[I] eSpiCmdVideoCtrl cmd 2
14039090->[I] open video prepare
14039090->[I] keep upscale mode: 1
14039090->[I] eSpiCmdVideoCtrl cmd 2 return 1
14051074->[I] cmd 26 opt 5 datalen 10
14051074->[I] eSpiCmdVideoCtrl cmd 3
14051074->[I] video reset
14051074->[I] eSpiCmdVideoCtrl cmd 3 return 1
14051105->[I] i
14051108->[I] i
14053607->[I] i
14053611->[I] ret 0
14053613->[I] ret 0
14053614->[I] ret 0
14053615->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053617->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053619->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053621->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053623->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053625->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053627->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053629->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053631->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053633->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053635->[I] ret 1
14053637->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053639->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053641->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053643->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053645->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053647->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053649->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053651->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053653->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053655->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053657->[I] ret 1
14053657->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053659->[E] I2C2 Slave addr 0x7C, task app display tas code 4
14053661->[I] ret 0
14053681->[I] i
14054212->[I] dsc mode not match
14054215->[I] hard reset
14054610->[I] cmd 26 opt 5 datalen 10
14054610->[I] eSpiCmdVideoCtrl cmd 1
14054610->[I] video set work mode 0
14054610->[I] eSpiCmdVideoCtrl cmd 1 return 1
14054615->[I] cmd 26 opt 5 datalen 10
14054615->[I] eSpiCmdVideoCtrl cmd 2
14054615->[I] open video prepare
14054615->[I] keep upscale mode: 1
14054616->[I] eSpiCmdVideoCtrl cmd 2 return 1
14055172->[I] calc fps 0 => 90
14056724->[I] cmd 86 opt 5 datalen 1
14056726->[I] cmd 86 opt 5 datalen 1
14056727->[I] cmd 86 opt 5 datalen 1
14056727->[I] cmd 86 opt 5 datalen 1
14056739->[I] cmd 10 opt 5 datalen 4
14056739->[I] cmd 10 opt 5 datalen 4
14056740->[I] cmd 86 opt 5 datalen 4
14056744->[I] ept_vef_sig in scr_len:35 key_id:1

14056755->[I] cmd 86 opt 5 datalen 4
14056756->[I] ept_r_ept expand:0 1 268442544
14056764->[I] cmd 86 opt 5 datalen 4
14056764->[I] cmd 86 opt 5 datalen 4
14056765->[I] ept_r_ept expand:2 1 268442544
14056769->[I] cmd 10 opt 5 datalen 4
14056771->[I] cmd 10 opt 5 datalen 4
14056783->[I] cmd 10 opt 5 datalen 4
14056783->[I] cmd 10 opt 5 datalen 4
14056796->[I] cmd 10 opt 5 datalen 4
14056796->[I] cmd 10 opt 5 datalen 4
14056809->[I] cmd 10 opt 5 datalen 4
14056809->[I] cmd 10 opt 5 datalen 4
14056822->[I] cmd 10 opt 5 datalen 4
14056822->[I] cmd 10 opt 5 datalen 4
14056835->[I] cmd 10 opt 5 datalen 4
14056835->[I] cmd 10 opt 5 datalen 4
14056850->[I] cmd 10 opt 5 datalen 4
14056850->[I] cmd 10 opt 5 datalen 4
14056863->[I] cmd 10 opt 5 datalen 4
14056863->[I] cmd 10 opt 5 datalen 4
14056876->[I] cmd 10 opt 5 datalen 4
14056876->[I] cmd 10 opt 5 datalen 4
14056886->[I] cmd 86 opt 5 datalen 1
14056887->[I] cmd 86 opt 5 datalen 1
14056887->[I] etp_sts exp_fw:2
14056891->[I] cmd 91 opt 5 datalen 2
14056891->[I] ept_w_s write cmd:2 val:2

14056893->[I] cmd 91 opt 5 datalen 3
14056893->[I] ept_w_s write cmd:2 val:2

14056896->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14056896->[I] etp chip act_s:1 


14056898->[I] cmd 86 opt 5 datalen 4
14056898->[I] cmd 86 opt 5 datalen 4
14056898->[I] etp chip ept_s:1 app_s:1


14056904->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14056904->[I] etp chip act_s:1 


14056906->[I] etp chip ept_s:1 app_s:1


14056909->[I] ept_r_ept expand:0 32 268442544
14058731->[I] cmd 86 opt 5 datalen 1
14058731->[I] cmd 86 opt 5 datalen 1
14058735->[I] cmd 86 opt 5 datalen 1
14058735->[I] cmd 86 opt 5 datalen 1
14058737->[I] cmd 86 opt 5 datalen 1
14058738->[I] cmd 86 opt 5 datalen 1
14058738->[I] etp_sts ept_s:1


14058741->[I] cmd 86 opt 5 datalen 1
14058741->[I] cmd 86 opt 5 datalen 1
14058752->[I] cmd 10 opt 5 datalen 4
14058752->[I] cmd 10 opt 5 datalen 4
14058757->[I] ept_vef_sig in scr_len:35 key_id:1

14058780->[I] cmd 10 opt 5 datalen 4
14058780->[I] cmd 10 opt 5 datalen 4
14058792->[I] cmd 10 opt 5 datalen 4
14058793->[I] cmd 10 opt 5 datalen 4
14058806->[I] cmd 10 opt 5 datalen 4
14058806->[I] cmd 10 opt 5 datalen 4
14058818->[I] cmd 10 opt 5 datalen 4
14058818->[I] cmd 10 opt 5 datalen 4
14058831->[I] cmd 10 opt 5 datalen 4
14058831->[I] cmd 10 opt 5 datalen 4
14058843->[I] cmd 10 opt 5 datalen 4
14058843->[I] cmd 10 opt 5 datalen 4
14058855->[I] cmd 10 opt 5 datalen 4
14058855->[I] cmd 10 opt 5 datalen 4
14058867->[I] cmd 10 opt 5 datalen 4
14058867->[I] cmd 10 opt 5 datalen 4
14058879->[I] cmd 10 opt 5 datalen 4
14058879->[I] cmd 10 opt 5 datalen 4
14058888->[I] cmd 86 opt 5 datalen 1
14058889->[I] cmd 86 opt 5 datalen 1
14058889->[I] etp_sts exp_fw:2
14058893->[I] cmd 91 opt 5 datalen 2
14058893->[I] ept_w_s write cmd:2 val:2

14058895->[I] cmd 91 opt 5 datalen 3
14058895->[I] ept_w_s write cmd:2 val:2

14058898->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14058898->[I] etp chip act_s:1 


14058900->[I] cmd 86 opt 5 datalen 4
14058900->[I] cmd 86 opt 5 datalen 4
14058900->[I] etp chip ept_s:1 app_s:1


14058906->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14058906->[I] etp chip act_s:1 


14058908->[I] etp chip ept_s:1 app_s:1


14058911->[I] ept_r_ept expand:0 32 268442544
14059519->[I] i
14059546->[I] i
14059550->[I] boe_localdimming_on

14059742->[I] Panel: 0
14059742->[I] Panel: 1
14059748->[I] Panel: 0 ok!

14059748->[I] BOE_DataInit B2 4,
14059748->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14059748->[I] Panel: 1 ok!

14059748->[I] BOE_DataInit B2 4,
14059748->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14059761->[I] codec_suspend s:1 reset:0


14059761->[I] sync_codec_power_state s_o:1, s:1
14059762->[I] codec_power s:1 bk_s:1
14059762->[E] codec_off flag:1
14059762->[I] video stable
14059762->[I] sta14059762->[I] rx0 0x08E00960 Htotal=2400, Vtotal=2272
14059763->[I] rx1 0x08E00960 Htotal=2400, Vtotal=2272
14059763->[I] dp_rx_timming_check Ok
14059851->[W] pps OK.
14059851->[I] codec_resume s:1 reset:0


14059851->[I] codec_power s:2 bk_s:1
14059851->[E] codec_on flag:1
14059856->[I] state 7 => 8
14059861->[I] Panel ON
14060743->[I] cmd 86 opt 5 datalen 1
14060744->[I] cmd 86 opt 5 datalen 1
14060747->[I] cmd 86 opt 5 datalen 1
14060748->[I] cmd 86 opt 5 datalen 1
14060749->[I] cmd 86 opt 5 datalen 1
14060749->[I] etp_sts ept_s:1


14060749->[I] cmd 86 opt 5 datalen 1
14060749->[I] etp_sts exp_fw:2
14060756->[I] cmd 91 opt 5 datalen 2
14060756->[I] ept_w_s write cmd:2 val:2

14060759->[I] cmd 91 opt 5 datalen 3
14060759->[I] ept_w_s write cmd:2 val:2

14060762->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14060762->[I] etp chip act_s:1 


14060764->[I] cmd 86 opt 5 datalen 4
14060764->[I] cmd 86 opt 5 datalen 4
14060764->[I] etp chip ept_s:1 app_s:1


14060771->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14060771->[I] etp chip act_s:1 


14060773->[I] etp chip ept_s:1 app_s:1


14060776->[I] ept_r_ept expand:0 32 268442544
14061762->[E] I2C3 Slave addr 0x72, task app display tas code 1
14061762->[E] retry cnt 1 ret 1
14062940->[I] Codec init done cnt:1.
14062940->[E] codec_reset_flag wait:0
14062940->[I] sync_codec_power_state s_o:1, s:2
14062940->[I] codec_vol val:2 vol_bk:0 force:1 p_s:2


14062940->[I] codec_unmute codec_s:1


14062943->[I] codec_vol_mute 1


14062943->[I] vol_ctl vol_bk:168 s:1


14062987->[I] codec_jack n:0 o:170
14063018->[I] codec_jack s:2
14063018->[I] codec_vol val:2 vol_bk:2 force:0 p_s:2


14065043->[I] vol_ctl end


14078745->[I] cmd 86 opt 5 datalen 1
14078745->[I] cmd 86 opt 5 datalen 1
14079066->[I] cmd 85 opt 5 datalen 54
14079080->[I] cmd 85 opt 5 datalen 54
14079095->[I] cmd 85 opt 5 datalen 54
14079109->[I] cmd 85 opt 5 datalen 54
14079123->[I] cmd 85 opt 5 datalen 54
14079137->[I] cmd 85 opt 5 datalen 54
14079137->[I] ept_hid encpt_actv size:[293]


14079137->[I] ept_act sn:P33000P1174A1400164 act_s:1 tm:1733788832

14079138->[I] ept_vef_sig in scr_len:256 key_id:1

14079150->[I] ept_vef_sig sha256 sus

14079176->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14079176->[I] etp chip act_s:1 


14079180->[I] etp chip ept_s:1 app_s:1


14079963->[I] boe_localdimming_off

14079963->[I] i
14079968->[I] i
14079998->[I] codec_suspend s:2 reset:0


14079998->[I] sync_codec_power_state s_o:2, s:1
14079998->[I] codec_power s:1 bk_s:2
14079998->[E] codec_off flag:0
14079998->[I] codec_vol val:0 vol_bk:2 force:1 p_s:1


14079998->[I] codec_vol_mute 0


14079998->[I] state 8 => 9
14079998->[I] codec_classd 0


14080063->[I] Panel OFF
14080746->[I] cmd 86 opt 5 datalen 1
14080748->[I] cmd 86 opt 5 datalen 1
14080747->[I] cmd 86 opt 5 datalen 1
14080749->[I] cmd 86 opt 5 datalen 1
14080749->[I] etp_sts ept_s:1


14080751->[I] cmd 86 opt 5 datalen 1
14080751->[I] cmd 86 opt 5 datalen 1
14080751->[I] etp_sts exp_fw:2
14080757->[I] cmd 91 opt 5 datalen 2
14080757->[I] ept_w_s write cmd:2 val:2

14080762->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14080762->[I] etp chip act_s:1 


14080764->[I] etp chip ept_s:1 app_s:1


14082150->[I] cmd 86 opt 5 datalen 1
14082151->[I] cmd 86 opt 5 datalen 1
14082158->[I] cmd 91 opt 5 datalen 3
14082158->[I] ept_w_s write cmd:2 val:2

14082163->[I] cmd 86 opt 5 datalen 4
14082163->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14082163->[I] etp chip act_s:1 


14082164->[I] cmd 86 opt 5 datalen 4
14082165->[I] etp chip ept_s:1 app_s:1


14082168->[I] ept_r_ept expand:0 32 268442544
14082170->[I] cmd 86 opt 5 datalen 1
14082170->[I] cmd 86 opt 5 datalen 1
14089059->[I] cmd 86 opt 5 datalen 1
14089060->[I] cmd 86 opt 5 datalen 1
14100755->[I] cmd 86 opt 5 datalen 1
14100756->[I] cmd 86 opt 5 datalen 1
14100759->[I] cmd 86 opt 5 datalen 1
14100760->[I] cmd 86 opt 5 datalen 1
14100760->[I] etp_sts ept_s:1


14100762->[I] cmd 86 opt 5 datalen 1
14100762->[I] cmd 86 opt 5 datalen 1
14100762->[I] etp_sts exp_fw:2
14100766->[I] cmd 91 opt 5 datalen 2
14100766->[I] ept_w_s write cmd:2 val:2

14100771->[I] cmd 91 opt 5 datalen 3
14100771->[I] ept_w_s write cmd:2 val:2

14100772->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14100772->[I] etp chip act_s:1 


14100774->[I] etp chip ept_s:1 app_s:1


14100776->[I] cmd 86 opt 5 datalen 4
14100776->[I] cmd 86 opt 5 datalen 4
14100780->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14100780->[I] etp chip act_s:1 


14100782->[I] etp chip ept_s:1 app_s:1


14100785->[I] ept_r_ept expand:0 32 268442544
14101076->[I] cmd 91 opt 5 datalen 3
14101076->[I] ept_w_s write cmd:1 len:100 max:100

14101085->[I] cmd 85 opt 5 datalen 54
14101099->[I] cmd 85 opt 5 datalen 54
14101113->[I] cmd 85 opt 5 datalen 54
14101128->[I] cmd 85 opt 5 datalen 54
14101142->[I] cmd 85 opt 5 datalen 54
14101156->[I] cmd 85 opt 5 datalen 54
14101170->[I] cmd 85 opt 5 datalen 54
14101185->[I] cmd 85 opt 5 datalen 54
14101185->[I] ept_hid encpt_ept size:[401]


14101185->[I] ept_eqt sn:P33000P1174A1400164 [1733106426][1733788854][2145916800] ept_s:1 exp_len:100

14101185->[I] ept_vef_sig in scr_len:256 key_id:1

14101198->[I] ept_vef_sig sha256 sus

14101221->[I] ept_eqt ept_s:1

14101246->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14101246->[I] etp chip act_s:1 


14101248->[I] etp chip ept_s:1 app_s:1


14104208->[I] cmd 86 opt 5 datalen 0
14104208->[I] cmd 86 opt 5 datalen 0
14104216->[I] cmd 86 opt 5 datalen 1
14104216->[I] cmd 86 opt 5 datalen 1
14104218->[I] cmd 86 opt 5 datalen 1
14104219->[I] cmd 86 opt 5 datalen 1
14104219->[I] etp_sts ept_s:1


14106091->[I] cmd 86 opt 5 datalen 1
14106091->[I] cmd 86 opt 5 datalen 1
14106091->[I] etp_sts exp_fw:2
14106095->[I] cmd 91 opt 5 datalen 2
14106095->[I] ept_w_s write cmd:2 val:2

14106098->[I] cmd 91 opt 5 datalen 3
14106098->[I] ept_w_s write cmd:2 val:2

14106101->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14106101->[I] etp chip act_s:1 


14106103->[I] cmd 86 opt 5 datalen 4
14106103->[I] etp chip ept_s:1 app_s:1


14106105->[I] cmd 86 opt 5 datalen 4
14106109->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14106109->[I] etp chip act_s:1 


14106111->[I] etp chip ept_s:1 app_s:1


14106115->[I] ept_r_ept expand:0 32 268442544
14111082->[I] cmd 86 opt 5 datalen 1
14111083->[I] cmd 86 opt 5 datalen 1
14111085->[I] cmd 86 opt 5 datalen 1
14111086->[I] cmd 86 opt 5 datalen 1
14111086->[I] etp_sts ept_s:1


14111089->[I] cmd 86 opt 5 datalen 1
14111090->[I] cmd 86 opt 5 datalen 1
14111090->[I] etp_sts exp_fw:2
14111094->[I] cmd 86 opt 5 datalen 1
14111094->[I] cmd 86 opt 5 datalen 1
14111094->[I] etp_sts exp_fw:2
14111095->[I] cmd 91 opt 5 datalen 2
14111095->[I] ept_w_s write cmd:2 val:2

14111098->[I] cmd 91 opt 5 datalen 3
14111098->[I] ept_w_s write cmd:2 val:2

14111099->[I] cmd 91 opt 5 datalen 2
14111099->[I] ept_w_s write cmd:2 val:2

14111101->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14111101->[I] etp chip act_s:1 


14111103->[I] cmd 86 opt 5 datalen 4
14111103->[I] etp chip ept_s:1 app_s:1


14111105->[I] cmd 86 opt 5 datalen 4
14111109->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14111109->[I] etp chip act_s:1 


14111111->[I] etp chip ept_s:1 app_s:1


14111117->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


14111117->[I] etp chip act_s:1 


14111119->[I] etp chip ept_s:1 app_s:1


14111122->[I] ept_r_ept expand:0 32 268442544
14119064->[I] i
14119071->[I] boe_localdimming_on

14120071->[I] i
14120098->[I] codec_resume s:1 reset:0


14120098->[I] codec_power s:2 bk_s:1
14120098->[E] codec_on flag:1
14120098->[I] state 9 => 8
14120098->[I] Panel ON
14120098->[I] boe_localdimming_off

14120098->[I] i
14120104->[I] i
14120104->[E] I2C3 Slave addr 0x72, task app display tas code 1
14120104->[E] retry cnt 1 ret 1
14120132->[I] i
14120137->[I] boe_localdimming_on

14120342->[I] Panel: 0
14120342->[I] Panel: 1
14120348->[I] Panel: 0 ok!

14120348->[I] BOE_DataInit B2 4,
14120348->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14120348->[I] Panel: 1 ok!

14120348->[I] BOE_DataInit B2 4,
14120348->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14123185->[I] Codec init done cnt:1.
14123185->[E] codec_reset_flag wait:0
14123185->[I] sync_codec_power_state s_o:1, s:2
14123185->[I] codec_vol val:2 vol_bk:0 force:1 p_s:2


14123185->[I] codec_unmute codec_s:1


14123188->[I] codec_vol_mute 1


14123188->[I] vol_ctl vol_bk:168 s:1


14123228->[I] codec_jack n:0 o:170
14123260->[I] codec_jack s:2
14123260->[I] codec_vol val:2 vol_bk:2 force:0 p_s:2


14125288->[I] vol_ctl end


14564966->[I] boe_localdimming_off

14564966->[I] i
14564971->[I] i
14564999->[I] codec_suspend s:2 reset:0


14564999->[I] sync_codec_power_state s_o:2, s:1
14564999->[I] codec_power s:1 bk_s:2
14564999->[E] codec_off flag:0
14564999->[I] codec_vol val:0 vol_bk:2 force:1 p_s:1


14564999->[I] codec_vol_mute 0


14564999->[I] state 8 => 9
14564999->[I] codec_classd 0


14565066->[I] Panel OFF
14599266->[I] i
14599271->[I] boe_localdimming_on

14600272->[I] i
14600300->[I] codec_resume s:1 reset:0


14600300->[I] codec_power s:2 bk_s:1
14600300->[E] codec_on flag:1
14600300->[I] state 9 => 8
14600300->[I] Panel ON
14600300->[I] boe_localdimming_off

14600300->[I] i
14600304->[I] i
14600304->[E] I2C3 Slave addr 0x72, task app display tas code 1
14600304->[E] retry cnt 1 ret 1
14600332->[I] i
14600337->[I] boe_localdimming_on

14600541->[I] Panel: 0
14600542->[I] Panel: 1
14600547->[I] Panel: 0 ok!

14600547->[I] BOE_DataInit B2 4,
14600547->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14600548->[I] Panel: 1 ok!

14600548->[I] BOE_DataInit B2 4,
14600548->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14603385->[I] Codec init done cnt:1.
14603385->[E] codec_reset_flag wait:0
14603385->[I] sync_codec_power_state s_o:1, s:2
14603385->[I] codec_vol val:2 vol_bk:0 force:1 p_s:2


14603385->[I] codec_unmute codec_s:1


14603388->[I] codec_vol_mute 1


14603389->[I] vol_ctl vol_bk:168 s:1


14603430->[I] codec_jack n:0 o:170
14603462->[I] codec_jack s:2
14603462->[I] codec_vol val:2 vol_bk:2 force:0 p_s:2


14605489->[I] vol_ctl end


14871265->[I] boe_localdimming_off

14871265->[I] i
14871270->[I] i
14871298->[I] codec_suspend s:2 reset:0


14871298->[I] sync_codec_power_state s_o:2, s:1
14871298->[I] codec_power s:1 bk_s:2
14871298->[E] codec_off flag:0
14871298->[I] codec_vol val:0 vol_bk:2 force:1 p_s:1


14871298->[I] codec_vol_mute 0


14871298->[I] state 8 => 9
14871298->[I] codec_classd 0


14871365->[I] Panel OFF
14877765->[I] i
14877770->[I] boe_localdimming_on

14878771->[I] i
14878799->[I] codec_resume s:1 reset:0


14878799->[I] codec_power s:2 bk_s:1
14878799->[E] codec_on flag:1
14878799->[I] state 9 => 8
14878799->[I] Panel ON
14878799->[I] boe_localdimming_off

14878799->[I] i
14878803->[I] i
14878803->[E] I2C3 Slave addr 0x72, task app display tas code 1
14878803->[E] retry cnt 1 ret 1
14878831->[I] i
14878836->[I] boe_localdimming_on

14879041->[I] Panel: 0
14879041->[I] Panel: 1
14879047->[I] Panel: 0 ok!

14879047->[I] BOE_DataInit B2 4,
14879047->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14879047->[I] Panel: 1 ok!

14879047->[I] BOE_DataInit B2 4,
14879047->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
14881886->[I] Codec init done cnt:1.
14881886->[E] codec_reset_flag wait:0
14881886->[I] sync_codec_power_state s_o:1, s:2
14881886->[I] codec_vol val:2 vol_bk:0 force:1 p_s:2


14881886->[I] codec_unmute codec_s:1


14881889->[I] codec_vol_mute 1


14881889->[I] vol_ctl vol_bk:168 s:1


14881912->[I] codec_jack n:0 o:170
14881945->[I] codec_jack s:2
14881945->[I] codec_vol val:2 vol_bk:2 force:0 p_s:2


14883989->[I] vol_ctl end


15137164->[I] boe_localdimming_off

15137164->[I] i
15137169->[I] i
15137197->[I] codec_suspend s:2 reset:0


15137197->[I] sync_codec_power_state s_o:2, s:1
15137197->[I] codec_power s:1 bk_s:2
15137197->[E] codec_off flag:0
15137197->[I] codec_vol val:0 vol_bk:2 force:1 p_s:1


15137197->[I] codec_vol_mute 0


15137197->[I] state 8 => 9
15137197->[I] codec_classd 0


15137264->[I] Panel OFF
15191864->[I] i
15191869->[I] boe_localdimming_on

15192870->[I] i
15192898->[I] codec_resume s:1 reset:0


15192898->[I] codec_power s:2 bk_s:1
15192898->[E] codec_on flag:1
15192898->[I] state 9 => 8
15192898->[I] Panel ON
15192898->[I] boe_localdimming_off

15192898->[I] i
15192902->[I] i
15192902->[E] I2C3 Slave addr 0x72, task app display tas code 1
15192902->[E] retry cnt 1 ret 1
15192930->[I] i
15192935->[I] boe_localdimming_on

15193140->[I] Panel: 0
15193140->[I] Panel: 1
15193146->[I] Panel: 0 ok!

15193146->[I] BOE_DataInit B2 4,
15193146->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
15193146->[I] Panel: 1 ok!

15193146->[I] BOE_DataInit B2 4,
15193146->[I] BOE_DataInit mux_time_us: 455, t_porch_us: 296, t_gap_us: 56,spi_transfer_v: 1228, t_delay_us: 5000, real delay_us: 2566
15195978->[I] Codec init done cnt:1.
15195978->[E] codec_reset_flag wait:0
15195978->[I] sync_codec_power_state s_o:1, s:2
15195978->[I] codec_vol val:2 vol_bk:0 force:1 p_s:2


15195978->[I] codec_unmute codec_s:1


15195982->[I] codec_vol_mute 1


151959