1966->[I] i
1970->[I] ret 0
1972->[I] ret 0
1972->[I] ret 0
1974->[I] ret 0
1976->[I] ret 0
1976->[I] ret 0
1996->[I] i
app_start_thread wait nrf usb ready try_cnt:8.
2516->[E] I2C3 Slave addr 0x72, task app display tas code 1
2516->[E] retry cnt 1 ret 1
2527->[I] codec_suspend s:1 reset:1


2527->[I] state 1 => 5
2558->[I] codec_power spk:0 1797:1788


4402->[I] Codec init done cnt:1.
4402->[I] sync_codec_power_state s_o:0, s:3
4530->[I] cmd 86 opt 5 datalen 1
4530->[I] cmd 86 opt 5 datalen 1
4530->[I] etp_sts exp_fw:2
4534->[I] cmd 91 opt 5 datalen 2
4534->[I] ept_w_s write cmd:2 val:2

4536->[I] cmd 86 opt 5 datalen 4
4536->[I] cmd 86 opt 5 datalen 4
4537->[I] cmd 3 opt 6 datalen 0
4540->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


4540->[I] etp chip act_s:1 


4542->[I] etp chip ept_s:1 app_s:1


4542->[I] Panel off unlocked!!!
4544->[I] ept_r_ept expand:0 1 268442544
4549->[I] cmd 86 opt 5 datalen 4
4549->[I] cmd 86 opt 5 datalen 4
4550->[I] ept_r_ept expand:2 1 268442544
4826->[I] cmd 26 opt 5 datalen 10
4826->[I] eSpiCmdVideoCtrl cmd 1
4826->[I] video set work mode 0
4826->[I] eSpiCmdVideoCtrl cmd 1 return 1
4831->[I] cmd 26 opt 5 datalen 10
4831->[I] eSpiCmdVideoCtrl cmd 2
4831->[I] open video prepare
4831->[I] requiredFps 90
4831->[I] set upscale mode: 1
4834->[I] dsc mode not match
4838->[I] eSpiCmdVideoCtrl cmd 2 return 2
4843->[I] cmd 26 opt 5 datalen 10
4843->[I] eSpiCmdVideoCtrl cmd 3
4843->[I] video reset
4843->[I] eSpiCmdVideoCtrl cmd 3 return 1
4926->[I] i
4929->[I] i
5329->[I] cmd 86 opt 5 datalen 1
5329->[I] cmd 86 opt 5 datalen 1
5332->[I] cmd 86 opt 5 datalen 1
5332->[I] cmd 86 opt 5 datalen 1
5334->[I] cmd 86 opt 5 datalen 1
5334->[I] cmd 86 opt 5 datalen 1
5334->[I] etp_sts ept_s:1


5341->[I] cmd 10 opt 5 datalen 4
5341->[I] cmd 10 opt 5 datalen 4
5346->[I] ept_vef_sig in scr_len:35 key_id:1

5347->[I] requiredFps 0
5347->[I] codec_i2s connect reset_flag:1


5366->[I] cmd 10 opt 5 datalen 4
5366->[I] cmd 10 opt 5 datalen 4
5378->[I] cmd 10 opt 5 datalen 4
5379->[I] cmd 10 opt 5 datalen 4
5390->[I] cmd 10 opt 5 datalen 4
5390->[I] cmd 10 opt 5 datalen 4
5402->[I] cmd 10 opt 5 datalen 4
5402->[I] cmd 10 opt 5 datalen 4
5413->[I] cmd 10 opt 5 datalen 4
5413->[I] cmd 10 opt 5 datalen 4
5424->[I] cmd 10 opt 5 datalen 4
5424->[I] cmd 10 opt 5 datalen 4
5435->[I] cmd 10 opt 5 datalen 4
5435->[I] cmd 10 opt 5 datalen 4
5446->[I] cmd 10 opt 5 datalen 4
5446->[I] cmd 10 opt 5 datalen 4
5458->[I] cmd 10 opt 5 datalen 4
5458->[I] cmd 10 opt 5 datalen 4
5467->[I] cmd 86 opt 5 datalen 1
5467->[I] cmd 86 opt 5 datalen 1
5467->[I] etp_sts exp_fw:2
5471->[I] cmd 91 opt 5 datalen 2
5471->[I] ept_w_s write cmd:2 val:2

5474->[I] cmd 91 opt 5 datalen 3
5474->[I] ept_w_s write cmd:2 val:2

5477->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


5477->[I] etp chip act_s:1 


5479->[I] cmd 86 opt 5 datalen 4
5479->[I] cmd 86 opt 5 datalen 4
5479->[I] etp chip ept_s:1 app_s:1


5485->[I] etp_ld ld_en:1 ld_s:161 app_unlock:1


5485->[I] etp chip act_s:1 


5487->[I] etp chip ept_s:1 app_s:1


5489->[I] ept_r_ept expand:0 32 268442544
5502->[E] codec_reset_flag wait:3
5502->[I] sync_codec_power_state s_o:3, s:2
5502->[I] codec_vol val:0 vol_bk:170 force:1 p_s:1


5502->[I] codec_power s:1 bk_s:2
5502->[E] codec_off flag:0
5502->[I] codec_vol val:0 vol_bk:170 force:1 p_s:1


7428->[I] i
7432->[I] ret 0
7434->[I] ret 0
7434->[I] ret 0
7436->[I] ret 0
7438->[I] ret 0
7438->[I] ret 0
7458->[I] i
7989->[I] dsc mode not match
7992->[I] hard reset
8341->[I] cmd 26 opt 5 datalen 10
8341->[I] eSpiCmdVideoCtrl cmd 1
8341->[I] video set work mode 0
8341->[I] eSpiCmdVideoCtrl cmd 1 return 1
8346->[I] cmd 26 opt 5 datalen 10
8346->[I] eSpiCmdVideoCtrl cmd 2
8346->[I] open video prepare
8346->[I] requiredFps 90
8346->[I] keep upscale mode: 1
8346->[I] eSpiCmdVideoCtrl cmd 2 return 1
8410->[I] cmd 26 opt 5 datalen 10
8410->[I] eSpiCmdVideoCtrl cmd 2
8410->[I] open video prepare
8410->[I] keep upscale mode: 1
8410->[I] eSpiCmdVideoCtrl cmd 2 return 1
9426->[I] cmd 26 opt 5 datalen 10
9426->[I] eSpiCmdVideoCtrl cmd 2
9426->[I] open video prepare
9426->[I] keep upscale mode: 1
9426->[I] eSpiCmdVideoCtrl cmd 2 return 1
10442->[I] cmd 26 opt 5 datalen 10
10442->[I] eSpiCmdVideoCtrl cmd 2
10442->[I] open video prepare
10442->[I] keep upscale mode: 1
10442->[I] eSpiCmdVideoCtrl cmd 2 return 1
11458->[I] cmd 26 opt 5 datalen 10
11458->[I] eSpiCmdVideoCtrl cmd 2
11458->[I] open video prepare
11458->[I] keep upscale mode: 1
11458->[I] eSpiCmdVideoCtrl cmd 2 return 1
23458->[I] cmd 26 opt 5 datalen 10
23458->[I] eSpiCmdVideoCtrl cmd 3
23458->[I] video reset
23458->[I] eSpiCmdVideoCtrl cmd 3 return 1
23492->[I] i
23495->[I] i
25994->[I] i
25998->[I] ret 0
26000->[I] ret 0
26000->[I] ret 0
26002->[I] ret 0
26004->[I] ret 0
26004->[I] ret 0
26024->[I] i
26555->[I] dsc mode not match
26558->[I] hard reset
26912->[I] cmd 26 opt 5 datalen 10
26912->[I] eSpiCmdVideoCtrl cmd 1
26912->[I] video set work mode 0
26912->[I] eSpiCmdVideoCtrl cmd 1 return 1
26917->[I] cmd 26 opt 5 datalen 10
26917->[I] eSpiCmdVideoCtrl cmd 2
26917->[I] open video prepare
26917->[I] keep upscale mode: 1
26917->[I] eSpiCmdVideoCtrl cmd 2 return 1
26977->[I] cmd 26 opt 5 datalen 10
26977->[I] eSpiCmdVideoCtrl cmd 2
26977->[I] open video prepare
26977->[I] keep upscale mode: 1
26977->[I] eSpiCmdVideoCtrl cmd 2 return 1
28009->[I] cmd 26 opt 5 datalen 10
28009->[I] eSpiCmdVideoCtrl cmd 2
28009->[I] open video prepare
28009->[I] keep upscale mode: 1
28009->[I] eSpiCmdVideoCtrl cmd 2 return 1
29026->[I] cmd 26 opt 5 datalen 10
29026->[I] eSpiCmdVideoCtrl cmd 2
29026->[I] open video prepare
29026->[I] keep upscale mode: