docdata["Hercules"] =
{
                               "APU Panel": {
                                                "APU_START_SW": {
                                                                               "category": "APU Panel",
                                                                           "control_type": "selector",
                                                                            "description": "APU Stop/Run/Start Selector",
                                                                             "identifier": "APU_START_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 2
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26122,
                                                                                               "description": "selector position",
                                                                                                      "mask": 48,
                                                                                                 "max_value": 2,
                                                                                                  "shift_by": 4,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "limited_rotary"
                                                                }
                                            },
                          "Electric Panel": {
                                                  "BATTERY_SW": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "Battery Switch",
                                                                             "identifier": "BATTERY_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 4,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 2,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                 "BATTERY_SW1": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "Battery Switch1",
                                                                             "identifier": "BATTERY_SW1",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 8,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 3,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                "BATT_TEST_SW": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "Battery Test Switch",
                                                                             "identifier": "BATT_TEST_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 2
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 3072,
                                                                                                 "max_value": 2,
                                                                                                  "shift_by": 10,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "3_position_switch"
                                                                },
                                                   "EXT_PW_SW": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "External Power/OFF/APU Switch",
                                                                             "identifier": "EXT_PW_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 2
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 48,
                                                                                                 "max_value": 2,
                                                                                                  "shift_by": 4,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "3_position_switch"
                                                                },
                                                     "GEN1_SW": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "Generator 1 Switch",
                                                                             "identifier": "GEN1_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 64,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 6,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                     "GEN2_SW": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "Generator 2 Switch",
                                                                             "identifier": "GEN2_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 128,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 7,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                     "GEN3_SW": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "Generator 3 Switch",
                                                                             "identifier": "GEN3_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 256,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 8,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                },
                                                     "GEN4_SW": {
                                                                               "category": "Electric Panel",
                                                                           "control_type": "selector",
                                                                            "description": "Generator 4 Switch",
                                                                             "identifier": "GEN4_SW",
                                                                                 "inputs": [ {
                                                                                               "description": "switch to previous or next state",
                                                                                                 "interface": "fixed_step"
                                                                                           }, {
                                                                                               "description": "set position",
                                                                                                 "interface": "set_state",
                                                                                                 "max_value": 1
                                                                                           }, {
                                                                                                  "argument": "TOGGLE",
                                                                                               "description": "Toggle switch state",
                                                                                                 "interface": "action"
                                                                                           } ],
                                                                    "momentary_positions": "none",
                                                                                "outputs": [ {
                                                                                                   "address": 26112,
                                                                                               "description": "selector position",
                                                                                                      "mask": 512,
                                                                                                 "max_value": 1,
                                                                                                  "shift_by": 9,
                                                                                                    "suffix": "",
                                                                                                      "type": "integer"
                                                                                           } ],
                                                                       "physical_variant": "toggle_switch"
                                                                }
                                            },
                      "Engine Start Panel": {
                                                "ENG1_START_SW": {
                                                                                "category": "Engine Start Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Engine 1 Stop/Run/Start Selector",
                                                                              "identifier": "ENG1_START_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 3
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 26112,
                                                                                                "description": "selector position",
                                                                                                       "mask": 12288,
                                                                                                  "max_value": 3,
                                                                                                   "shift_by": 12,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "limited_rotary"
                                                                 },
                                                "ENG2_START_SW": {
                                                                                "category": "Engine Start Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Engine 2 Stop/Run/Start Selector",
                                                                              "identifier": "ENG2_START_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 3
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 26112,
                                                                                                "description": "selector position",
                                                                                                       "mask": 49152,
                                                                                                  "max_value": 3,
                                                                                                   "shift_by": 14,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "limited_rotary"
                                                                 },
                                                "ENG3_START_SW": {
                                                                                "category": "Engine Start Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Engine 3 Stop/Run/Start Selector",
                                                                              "identifier": "ENG3_START_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 3
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 26122,
                                                                                                "description": "selector position",
                                                                                                       "mask": 3,
                                                                                                  "max_value": 3,
                                                                                                   "shift_by": 0,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "limited_rotary"
                                                                 },
                                                "ENG4_START_SW": {
                                                                                "category": "Engine Start Panel",
                                                                            "control_type": "selector",
                                                                             "description": "Engine 4 Stop/Run/Start Selector",
                                                                              "identifier": "ENG4_START_SW",
                                                                                  "inputs": [ {
                                                                                                "description": "switch to previous or next state",
                                                                                                  "interface": "fixed_step"
                                                                                            }, {
                                                                                                "description": "set position",
                                                                                                  "interface": "set_state",
                                                                                                  "max_value": 3
                                                                                            } ],
                                                                     "momentary_positions": "none",
                                                                                 "outputs": [ {
                                                                                                    "address": 26122,
                                                                                                "description": "selector position",
                                                                                                       "mask": 12,
                                                                                                  "max_value": 3,
                                                                                                   "shift_by": 2,
                                                                                                     "suffix": "",
                                                                                                       "type": "integer"
                                                                                            } ],
                                                                        "physical_variant": "limited_rotary"
                                                                 }
                                            },
                 "External Aircraft Model": {
                                                 "EXT_LANDING_LIGHT_GEAR": {
                                                                                   "category": "External Aircraft Model",
                                                                               "control_type": "metadata",
                                                                                "description": "Gear Landing Light (white)",
                                                                                 "identifier": "EXT_LANDING_LIGHT_GEAR",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 26122,
                                                                                                   "description": "Gear Landing Light (white)",
                                                                                                          "mask": 32768,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 15,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                 "EXT_LANDING_LIGHT_LEFT": {
                                                                                   "category": "External Aircraft Model",
                                                                               "control_type": "metadata",
                                                                                "description": "Left Landing Light (white)",
                                                                                 "identifier": "EXT_LANDING_LIGHT_LEFT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 26122,
                                                                                                   "description": "Left Landing Light (white)",
                                                                                                          "mask": 8192,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 13,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                "EXT_LANDING_LIGHT_RIGHT": {
                                                                                   "category": "External Aircraft Model",
                                                                               "control_type": "metadata",
                                                                                "description": "Right Landing Light (white)",
                                                                                 "identifier": "EXT_LANDING_LIGHT_RIGHT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 26122,
                                                                                                   "description": "Right Landing Light (white)",
                                                                                                          "mask": 16384,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 14,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                       "EXT_SPEED_BRAKEs": {
                                                                                   "category": "External Aircraft Model",
                                                                               "control_type": "metadata",
                                                                                "description": "Speed Brakes",
                                                                                 "identifier": "EXT_SPEED_BRAKEs",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 26124,
                                                                                                   "description": "Speed Brakes",
                                                                                                          "mask": 65535,
                                                                                                     "max_value": 65535,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                           "EXT_WOW_LEFT": {
                                                                                   "category": "External Aircraft Model",
                                                                               "control_type": "metadata",
                                                                                "description": "Weight ON Wheels Left Gear",
                                                                                 "identifier": "EXT_WOW_LEFT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 26126,
                                                                                                   "description": "Weight ON Wheels Left Gear",
                                                                                                          "mask": 4,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 2,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                           "EXT_WOW_NOSE": {
                                                                                   "category": "External Aircraft Model",
                                                                               "control_type": "metadata",
                                                                                "description": "Weight ON Wheels Nose Gear",
                                                                                 "identifier": "EXT_WOW_NOSE",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 26126,
                                                                                                   "description": "Weight ON Wheels Nose Gear",
                                                                                                          "mask": 1,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 0,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           },
                                                          "EXT_WOW_RIGHT": {
                                                                                   "category": "External Aircraft Model",
                                                                               "control_type": "metadata",
                                                                                "description": "Weight ON Wheels Right Gear",
                                                                                 "identifier": "EXT_WOW_RIGHT",
                                                                                     "inputs": [  ],
                                                                                    "outputs": [ {
                                                                                                       "address": 26126,
                                                                                                   "description": "Weight ON Wheels Right Gear",
                                                                                                          "mask": 2,
                                                                                                     "max_value": 1,
                                                                                                      "shift_by": 1,
                                                                                                        "suffix": "",
                                                                                                          "type": "integer"
                                                                                               } ]
                                                                           }
                                            },
                               "ICS Panel": {
                                                 "CP_ICS_UN_KNB": {
                                                                          "category": "ICS Panel",
                                                                      "control_type": "limited_dial",
                                                                       "description": "COPILOT ICS Undefined Knob",
                                                                        "identifier": "CP_ICS_UN_KNB",
                                                                            "inputs": [ {
                                                                                          "description": "set the position of the dial",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 65535
                                                                                      }, {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 26120,
                                                                                          "description": "position of the potentiometer",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  },
                                                "CP_ICS_VOL_BTN": {
                                                                                 "category": "ICS Panel",
                                                                             "control_type": "selector",
                                                                              "description": "COPILOT ICS Volume (Pull)",
                                                                               "identifier": "CP_ICS_VOL_BTN",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 26112,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 2,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 1,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                "CP_ICS_VOL_KNB": {
                                                                          "category": "ICS Panel",
                                                                      "control_type": "limited_dial",
                                                                       "description": "COPILOT ICS Volume (Rotate)",
                                                                        "identifier": "CP_ICS_VOL_KNB",
                                                                            "inputs": [ {
                                                                                          "description": "set the position of the dial",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 65535
                                                                                      }, {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 26116,
                                                                                          "description": "position of the potentiometer",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  },
                                                  "P_ICS_UN_KNB": {
                                                                          "category": "ICS Panel",
                                                                      "control_type": "limited_dial",
                                                                       "description": "PILOT ICS Undefined Knob",
                                                                        "identifier": "P_ICS_UN_KNB",
                                                                            "inputs": [ {
                                                                                          "description": "set the position of the dial",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 65535
                                                                                      }, {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 26118,
                                                                                          "description": "position of the potentiometer",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  },
                                                 "P_ICS_VOL_BTN": {
                                                                                 "category": "ICS Panel",
                                                                             "control_type": "selector",
                                                                              "description": "PILOT ICS Volume (Pull)",
                                                                               "identifier": "P_ICS_VOL_BTN",
                                                                                   "inputs": [ {
                                                                                                 "description": "switch to previous or next state",
                                                                                                   "interface": "fixed_step"
                                                                                             }, {
                                                                                                 "description": "set position",
                                                                                                   "interface": "set_state",
                                                                                                   "max_value": 1
                                                                                             }, {
                                                                                                    "argument": "TOGGLE",
                                                                                                 "description": "Toggle switch state",
                                                                                                   "interface": "action"
                                                                                             } ],
                                                                      "momentary_positions": "none",
                                                                                  "outputs": [ {
                                                                                                     "address": 26112,
                                                                                                 "description": "selector position",
                                                                                                        "mask": 1,
                                                                                                   "max_value": 1,
                                                                                                    "shift_by": 0,
                                                                                                      "suffix": "",
                                                                                                        "type": "integer"
                                                                                             } ],
                                                                         "physical_variant": "toggle_switch"
                                                                  },
                                                 "P_ICS_VOL_KNB": {
                                                                          "category": "ICS Panel",
                                                                      "control_type": "limited_dial",
                                                                       "description": "PILOT ICS Volume (Rotate)",
                                                                        "identifier": "P_ICS_VOL_KNB",
                                                                            "inputs": [ {
                                                                                          "description": "set the position of the dial",
                                                                                            "interface": "set_state",
                                                                                            "max_value": 65535
                                                                                      }, {
                                                                                             "description": "turn the dial left or right",
                                                                                               "interface": "variable_step",
                                                                                               "max_value": 65535,
                                                                                          "suggested_step": 3200
                                                                                      } ],
                                                                           "outputs": [ {
                                                                                              "address": 26114,
                                                                                          "description": "position of the potentiometer",
                                                                                                 "mask": 65535,
                                                                                            "max_value": 65535,
                                                                                             "shift_by": 0,
                                                                                               "suffix": "",
                                                                                                 "type": "integer"
                                                                                      } ]
                                                                  }
                                            },
    "Warning, Caution and IndicatorLights": {
                                                 "APU_BLEED_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "APU Bleed Air Light (yellow)",
                                                                      "identifier": "APU_BLEED_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 26122,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 256,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 8,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                   "APU_SEL_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "APU Selector Light (green)",
                                                                      "identifier": "APU_SEL_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 26122,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 128,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 7,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                "ENG1_START_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Engine 1 Start Light (green)",
                                                                      "identifier": "ENG1_START_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 26122,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 512,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 9,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                "ENG2_START_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Engine 2 Start Light (green)",
                                                                      "identifier": "ENG2_START_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 26122,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 1024,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 10,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                "ENG3_START_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Engine 3 Start Light (green)",
                                                                      "identifier": "ENG3_START_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 26122,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 2048,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 11,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                "ENG4_START_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "Engine 4 Start Light (green)",
                                                                      "identifier": "ENG4_START_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 26122,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 4096,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 12,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                },
                                                    "EXT_PW_L": {
                                                                        "category": "Warning, Caution and IndicatorLights",
                                                                    "control_type": "led",
                                                                     "description": "External Power Indicator Light (green)",
                                                                      "identifier": "EXT_PW_L",
                                                                          "inputs": [  ],
                                                                         "outputs": [ {
                                                                                            "address": 26122,
                                                                                        "description": "0 if light is off, 1 if light is on",
                                                                                               "mask": 64,
                                                                                          "max_value": 1,
                                                                                           "shift_by": 6,
                                                                                             "suffix": "",
                                                                                               "type": "integer"
                                                                                    } ]
                                                                }
                                            }
};
